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KEY PROJECT INFORMATION
Key Project Information
	GS ID (s) of Project (s)
	GS11167

	Title of the project (s) covered by monitoring report
	[bookmark: _Hlk163655950]Taishan Geothermal Central Heating System

	Version number of the PDD/VPA-DD (s) applicable to this monitoring report
	04

	Version number of the monitoring report
	03

	Completion date of the monitoring report 
	28/08/2024

	Date of project design certification
	22/09/2021[footnoteRef:1]  [1:  For this project, the Design Review was approved on 19/10/2021.] 


	Date of Last Annual Report
	N/A

	Monitoring period number 
	04

	Duration of this monitoring period 
	The 4th monitoring period from 01/04/2023 to 31/03/2024 (first and last days included)

	Project Representative 
	The official focal point and project developer: Profit Carbon Environmental Energy Technology (Shanghai) Co., Ltd.
The project owner: Zhengzhou Onar Heating Co., Ltd

	Host Country
	People’s Republic of China

	Activity Requirements applied

	[bookmark: Check7]|X| Community Services Activities 
|_| Renewable Energy Activities 
|_| Land Use and Forestry Activities/Risks & Capacities 
|_| N/A 

	Methodology (ies) applied and version number
	AM0072 Fossil Fuel Displacement by Geothermal Resources for Space Heating (Version 03.0)

	Product Requirements applied
	|X| GHG Emissions Reduction & Sequestration 
|_| Renewable Energy Label 
|_| N/A 


Table 1 - Sustainable Development Contributions Achieved
	Sustainable Development Goals Targeted
	SDG Impact 
	Amount Achieved
	Units/ Products

	13 Climate Action
	GHG emission reductions
	136,205
	GS VERs

	8 Decent Work and Economic Growth
	Number of males and females employed by the project
	10 jobs created including 5 males and 5 females
	Number

	
	Average monthly salary
	4,550[footnoteRef:2] [2:  This monitoring period is from 01/04/2023 to 31/03/2024, the average monthly salary in year 2023 is 4,400 RMB/person, the average monthly salary in year 2024 is 5,000 RMB/person, thus, the average monthly salary in this monitoring period is (4,400 RMB/person *9 month+5,000 RMB/person*3 month)/12 month =4,550 RMB/person.] 

	RMB/person

	7 Affordable and Clean Energy
	Net heating area for construction type m (Am)
	2,459,732.33 m2 for residential buildings and 94,236.26 m2 for commercial buildings
	m2



Table 2 – Product Vintages


	SDG 13 Climate Action
	Amount Achieved

	Start Dates
	End Dates
	GHG emission reductions (tCO2e)

	01/04/2023
	31/12/2023
	54,495

	01/01/2024
	31/03/2024
	81,710









[bookmark: _Ref49860651]SECTION A. DESCRIPTION OF PROJECT
[bookmark: _Toc40962734]A.1. General description of project 
>>
The project activity is designed to introduce geothermal energy-based space heating system to realize heat supply to a series of new residential buildings and commercial buildings in Taishan village over winter season, which will displace heat supply from isolated coal-fired boilers as a business-as-usual scenario in the project area.

Taishan Village is in Longhu Town, Xinzheng City of Henan Province. In December 2019, it was selected as the National Rural Governance Demonstration Village. The project involves the construction and operation of geothermal production wells, reinjection wells, heat substations and heat supply pipelines. 

The project owner is Zhengzhou Onar Heating Co., Ltd and it has put into operation in November 2020 (winter season). It can supply geothermal heat to 2,480.907 thousand m2 of residential buildings and 94.516 thousand m2 of commercial buildings with a total heating load of 116.84MW. All the buildings covered by the project were newly built and there was no existing heating system prior to the project activity. In baseline scenario, heating supply in winter for the building areas will be provided by newly built coal-fired boilers in boiler house.  

Emission reduction credits will be earned by the use of geothermal energy instead of the combustion of fossil fuel for space heating. The annual average CO2 emission reductions are estimated as 143,987 tCO2e. This monitoring period is the 4th monitoring period, which is from 01/04/2023 to 31/03/2024, and a total 136,205 tCO2e emission reductions achieved.
[bookmark: _Toc40962735]A.2. Location of project 
>>
The project is in Taishan Village, Longhu Town, Xinzheng City of Henan Province, China. The geographical coordinates are Longitude east 113°37'23.8" to 113°38'33.1" and Latitude North 34°34'42.8" to 34°35'17.0". The detailed coordinates of the 6 heat substations are provided in Table 3 below.
Table 3 Coordinates of the 6 Heat Substations
	No.
	Sub-areas
	Heat Substations
	Geothermal Wells
	Coordinate

	1
	No.4 Village Group
	1# TS4G
	1# TS4G Production Well
	34°34'57.2"N 113°37'41.4"E

	
	
	
	1# TS4G Re-injection Well
	

	
	
	
	2# TS4G Production Well
	

	
	
	
	2# TS4G Re-injection Well
	

	
	
	2# TS4G
	3# TS4G Production Well
	34°35'00.1"N 113°38'10.4"E

	
	
	
	3# TS4G Re-injection Well
	

	
	
	
	4# TS4G Production Well
	

	
	
	
	4# TS4G Re-injection Well
	

	2
	Zhengrongfu
	3# TSZR
	5# TSZR Production Well
	34°34'59.1"N 113°38'33.1"E

	
	
	
	5# TSZR Re-injection Well
	

	
	
	
	6# TSZR Production Well
	

	
	
	
	6# TSZR Re-injection Well
	

	3
	Taishan Villa
	4# TSTS
	7# TSTS Production Well
	34°35'16.7"N 113°38'22.4"E

	
	
	
	7# TSTS Re-injection Well
	

	
	
	5# TSTS
	8# TSTS Production Well
	34°35'17.0"N 113°38'08.8"E

	
	
	
	8# TSTS Re-injection Well
	

	
	
	
	9# TSTS Production Well
	

	
	
	
	9# TSTS Re-injection Well
	

	4
	Wangdong Community
	6# TSWD
	10# TSWD Production Well
	34°34'42.8"N 113°37'23.8"E

	
	
	
	10# TSWD Re-injection Well
	

	
	
	
	11# TSWD Production Well
	

	
	
	
	11# TSWD Re-injection Well
	


[image: ][image: 5000万英文政区版(南海诸岛)]Henan Province

 [image: 建筑与房屋的城市空拍图与配字

描述已自动生成]Heat Substations

Figure 1 Location of the Project

[bookmark: _Toc40962736]A.3. Reference of applied methodology 
>>
Approved baseline and monitoring methodology: AM0072 Fossil Fuel Displacement by Geothermal Resources for Space Heating (Version 03.0)[footnoteRef:3].  [3:  https://cdm.unfccc.int/methodologies/DB/TMGAEU1XHW6BFN1CDFCTWV9VUGVI19] 

Tool applied: 
Tool 02 Combined tool to identify the baseline scenario and demonstrate additionality (Version 07.0)[footnoteRef:4] [4:  https://cdm.unfccc.int/methodologies/PAmethodologies/tools/am-tool-02-v7.0.pdf ] 

Tool 05 Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation (Version 03.0)[footnoteRef:5] [5:  https://cdm.unfccc.int/methodologies/PAmethodologies/tools/am-tool-05-v3.0.pdf ] 

Tool 07 Tool to calculate the emission factor for an electricity system (Version 07.0)[footnoteRef:6] [6:  https://cdm.unfccc.int/methodologies/PAmethodologies/tools/am-tool-07-v7.0.pdf ] 

Tool 24 Common practice (Version 03.1)[footnoteRef:7] [7:  https://cdm.unfccc.int/methodologies/PAmethodologies/tools/am-tool-24-v1.pdf ] 





[bookmark: _Toc40962737]A.4. Crediting period of project 
>>
Start date of first crediting period: 01/11/2020.
End date of first crediting period: 31/10/2025.
Total length of crediting period: 01/11/2020 to 31/10/2035 with two renewal cycles and in total 15 years. 
This monitoring period is from 01/04/2023 to 31/03/2024 (first and last days included), which belong to the first crediting period. Expected lifetime of the project: 15 years[footnoteRef:8]. [8:  As per manufacturer specifications of the geothermal space heating system, the lifetime of the equipment is more than 15 years.] 


[bookmark: _Ref49860659][bookmark: _Ref47706306][bookmark: _Toc40962738]SECTION B. IMPLEMENTATION OF PROJECT 
[bookmark: _Toc40962739][bookmark: _Ref418094175]B.1. Description of implemented project 
>>
The geothermal based space heating system was constructed from 20/05/2020 to 24/10/2020. The 22 geothermal (including 11 production wells and 11 reinjection wells) wells were connected to 6 Heat Substations in 4 Sub-areas to realize heat supply to the end-users in Taishan village over 2023-2024 heating season. The main actions made for implementation of the project are generalized in the following table.
Table 4 Milestone for implementation of the project
	Time
	Main actions

	07/01/2020
	Got water abstraction permits issued by Water Resources Bureau of Henan Province

	18/02/2020
	Approval by local Environmental Protection Bureau

	14/04/2020
	Approval by local Development and Reform Commission

	15/05/2020
	Start date of the project, the date on signing the geothermal well drilling contract

	01/11/2020
	Start date of fully operation of the geothermal heating system, and the start date of 2020-2021 winter heating season of Taishan village

	27/10/2021
	Date of finishing Design Review and Performance Review No.1

	10/10/2023
	Training for the employees for 2023-2024 heating season

	01/11/2023
	Start date of the 2023-2024 heating season

	31/03/2024
	End date of 2023-2024 winter heating season



The utilization hours of the geothermal heating system for residential buildings and commercial buildings were 3,648 and 2,525 hours respectively during this monitoring period (01/04/2023-31/03/2024). Also, the design heating area and heating load of each region described in approved PDD (Version 04), as well as the actual heating area and heating load in this monitoring period are shown in the table below. 
	No.
	Sub-area
	Heat substation
	Approved PDD
	This monitoring period

	
	
	
	Heat load[footnoteRef:9] (MW) [9:  Heating load can be calculated as heating aeras multiply heating index for construction type m. As per CJJ 34-2010 Design Code for City Heating Network published by Ministry of Housing and Urban-Rural Development of the People’s Republic of China, Heating index is 45 W/m2 for residential buildings and 55 W/m2 for commercial buildings.] 

	Heating area (thousand m3)
	Heat load[footnoteRef:10] (MW) [10:  Heating load can be calculated as heating aeras multiply heating index for construction type m. As per CJJ/T34-2022 Design standards for urban heating pipe networks published by Ministry of Housing and Urban-Rural Development of the People’s Republic of China, and this project has been put into operation in 2020, therefore, the heating index is 45 W/m2 for residential buildings and 55 W/m2 for commercial buildings.] 

	Heating area (thousand m3)

	1
	No.4 Village Group
	1# TS4G
	11.55
	256.6
	11.49
	255.2728

	
	
	2# TS4G
	23.11
	513.4
	22.92
	509.34984

	2
	Zhengrongfu
	3# TSZR
	32.86
	730.4
	32.43
	720.58243

	3
	Taishan Village
	4# TSTS
	5.2
	Commercial buildings 94.516
	5.18
	Commercial buildings 94.24

	
	
	5# TSTS
	19.37
	Residential buildings 430.507
	19.15
	Residential buildings 425.59873

	4
	Wangdong Community
	6# TSWD
	24.75
	550
	24.70
	548.92853

	Total
	6
	116.84
	Residential buildings 2,480.907
Commercial buildings 94.516
	115.87
	Residential buildings 2,459.73233
Commercial buildings 94.23626



The occupancy rate of the project area is less than 100%, unoccupied part of the residential area does not need heating supply during the 2023-2024 heating season. During the 2023-2024 heating season, the geothermal space heating system ran smoothly. There are no deviations or delays compared to information in approved Project Design Document (PDD).

[bookmark: _Toc40962740]B.1.1 Forward Action Requests 
>>
None.

B.2. Post-Design Certification changes
>>
[bookmark: _Toc40962741][bookmark: _Ref418094308]B.2.1. Temporary deviations from the approved Monitoring & Reporting Plan, methodology or standardized baseline
>>
None.

[bookmark: _Ref418094311][bookmark: _Toc40962742]B.2.2. Corrections
>>
None.

[bookmark: _Ref418094316][bookmark: _Toc40962743]B.2.3. Changes to start date of crediting period 
>>
None.

[bookmark: _Ref418094322][bookmark: _Toc40962744]B.2.4. Permanent changes from the Design Certified monitoring plan, applied methodology or applied standardized baseline
>>
None.

[bookmark: _Toc40962745][bookmark: _Ref418094327]B.2.5. Changes to project design of approved project
>>
None.









[bookmark: _Ref49860669][bookmark: _Toc40962746][bookmark: _Ref47706319]SECTION C. DESCRIPTION OF MONITORING SYSTEM APPLIED BY THE PROJECT
>>
Parameters to be monitored
According to section B.7.1 of the approved PDD, there are 10 parameters to be monitored,

SDG 7/SDG 13
a) Net heating area for construction type m, Am

SDG 8
b) Number of males and females employed by the project
c) Average monthly salary

SDG 13
d) Heating index for construction type m, HIm
e) Average technical transmission and distribution losses for providing electricity to source j in year y, TDLj,y
f) Combined margin emission factor for the grid in year y, EFEL,j,y (EFgrid,CM,y)
g) Hours per year heat utilization in well j, Tj
h) Average temperature difference between inlet and outlet temperatures at the downstream of substation heat exchanger in year y, Δtj,d,y
i) Average flow rate at the downstream of heat exchanger (upstream of which is connected with water supply from the geothermal well j) in year y, FRj,d,y
j) Electricity consumption for the year y in operating the geothermal heating system, ECPJ,j,y (ECy)

For the parameters of SDG 7 and SDG 13, net heating areas for construction type m (Am) were determined based on heating supply contracts signed for the related heating season and cross-checked by the business investment project approval. Net heating area for residential buildings and commercial buildings during the 4th monitoring period are 2,459,732.33 m2 and 94,236.26 m2. 

For the parameters of SDG 8, number of males and females employed by the project and average monthly salary were determined based on record keeping book. 10 jobs for local people were created and the average monthly salary were 4,550 RMB/person in this monitoring period[footnoteRef:11]. [11:  According to the Record Keeping Books, monthly salary of the employees (no matter males or females) was 4,400 RMB/person from 01/04/2023 to 31/12/2023 and 5,000 RMB/person from 01/01/2024 to 31/03/2024. In summary, the average monthly salary of the employees for this monitoring period can be calculated as (4,400 RMB/person*9+5,000 RMB/person*3)/12=4,550 RMB/person. Equal salaries were paid for men and women in the same position.] 


For the parameters of SDG 13
Heating index for construction type m (HIm) was sourced from the conservative standard index of CJJ/T34-2022[footnoteRef:12] Design standards for urban heating pipe networks published by Ministry of Housing and Urban-Rural Development of the People’s Republic of China, which is the latest related national and local standards. [12:  https://www.mohurd.gov.cn/gongkai/zhengce/zhengcefilelib/202207/20220704_767030.html] 


Average technical transmission and distribution losses for providing electricity to source j in year y (TDLj,y) was determined using the latest version of Tool 05 (Version 03.0).

Combined margin emission factor for the grid in year y (EFEL,j,y (EFgrid,CM,y)) was calculated using the procedures in the latest version of Tool 07 (Version 07.0). It was determined as per 2023 Baseline Emission Factors of China's Regional Power Grid for Emission Reduction Projects published by China National Climate Strategy Center[footnoteRef:13]. Taishan village is in Henan province, which belongs to Central China Regional Power Grid. EFgrid,OM Simple,y and EFgrid,BM,y were 0.8771 tCO2/MWh and 0.2696 tCO2/MWh separately in 2023. EFEL,j,y (EFgrid,CM,y) can be calculated as 0.8771 tCO2/MWh*0.5+0.2696 tCO2/MWh*0.5=0.57335 tCO2/MWh. [13:  https://ccer.cets.org.cn/notice/columnDetail?bulletinBoardId=1151185363440635904&bulletinBoardName=%E7%94%B5%E7%BD%91%E5%9F%BA%E5%87%86%E7%BA%BF%E6%8E%92%E6%94%BE%E5%9B%A0%E5%AD%90] 


Hours per heat utilization in well j (Tj) was sourced from statistical data of the geothermal space heating system. The 2023-2024 winter heating season of Taishan village was from 01/11/2023 to 31/03/2024 (152 days totally, 3,648 hours for residential buildings, 2,525 hours for commercial buildings). 

[bookmark: OLE_LINK2][bookmark: OLE_LINK4]Above all, the monitoring system only need to address the monitoring of parameter Δtj,d,y, FRj,d,y and ECPJ,j,y (ECy).

Monitoring framework
[bookmark: OLE_LINK3][bookmark: OLE_LINK7]Figure 2 below outlines the organization structure of the monitoring system. The project owner was responsible for the whole monitoring work. The GS monitoring team was formed，which was responsible for the monitoring of all the parameters to be monitored, mainly three parameters Δtj,d,y, FRj,d,y and ECPJ,j,y (ECy). All the data were reviewed by the project developer and VVB.


Figure 2 Organization Structure of the Monitoring Team

Monitoring equipment and installation
Inlet and outlet temperatures at the downstream of each heat exchanger are monitored by the ultrasonic calorimeters. There are 11 production wells and 11 re-injection wells. One production well and one re-injection well form one set of heat exchange system. There are totally 11 sets of heat exchange system. 22 ultrasonic calorimeters are needed to monitor the inlet and outlet temperatures of all the heat exchange system. The temperature measurement range of the ultrasonic calorimeters are 4 °C to 95 °C with an accuracy of 0.01 °C.

[bookmark: _Hlk78479035]Average flow rate at the downstream of each heat exchanger are monitored by the 11 ultrasonic calorimeters installed at downstream of each heat exchange system, which also can monitor the supply water temperature. The highest measurement flow rate range of the ultrasonic calorimeters are 1,000 m3/h with an accuracy of 0.01 m3/h.

Electricity consumptions of the geothermal heating system are monitored by the electricity meters installed at each heat substation. 6 electricity meters are needed. The accuracy of the electricity meters is 0.5S.

Installation and configuration of monitoring equipment are shown as Figure 3. All the monitoring equipment can measure continuously and installed in a manner that only the heat supplied by the geothermal heating system and the electricity consumed by it are measured.

In order to ensure measurements with a low degree of uncertainty, all the data monitoring equipment were calibrated by appropriately qualified third party according to appropriate national standard. The ultrasonic calorimeters are calibrated based on JJG 225-2001 Verification Regulation of Heat Meters[footnoteRef:14] and the electricity meters are calibrated based on JJG 596-2012 Electrical Meters for Measuring Alternating-current Electrical Energy[footnoteRef:15]. The specific calibration information of all monitoring equipment can be seen in section D.2 of this MR. [14:  https://www.wdfxw.net/doc60326801.htm]  [15:  https://www.wdfxw.net/doc91019332.htm] 


The point of heat measurement was not changed or added during the 4th monitoring period.

 
EM (1-6): 6 electricity meters installed at each heat substation to monitor the electricity consumptions of the geothermal heating system.
UC Inlet (1-11): 11 ultrasonic calorimeters installed at downstream of each heat exchange system to monitor the return water temperature from the end users.
UC Outlet (1-11): 11 ultrasonic calorimeters installed at downstream of each heat exchange system to monitor the supply water temperature from the geothermal heating system and the average flow rate of the supply water.
Figure 3 Installation and Configuration of Monitoring Equipment

Data management and archiving
Hourly volume flow rate, inlet temperature and outlet temperature of the heat exchange system were exported by the GS monitoring team at the beginning of the next month to form the monthly record. The average daily value of the related three parameters were calculated based on the 24-hourly data separately. The average monthly value of the related three parameters were calculated based on all the daily value of this month. Finally, the operation record of the geothermal heating system during the related heating season were summarized by all the monthly record.

Monthly operation time of the 11-heat exchange system were recorded by the GS monitoring team at the beginning of the next month as per the geothermal heating system. The operation record of the geothermal heating system during the related heating season were summarized by all the monthly record.

Before the 2023-2024 heating season, base number[footnoteRef:16] of all the 6 electricity meters were recorded by the GS monitoring team under the supervision of the representative of each sub-area[footnoteRef:17]. At the end of each heating month, the GS monitoring team recorded readings of the 6 electricity meters, which can calculate the electricity consumption of this month by minus last month’s base number of the related electricity meters. The operation record of the geothermal heating system during the related heating season were summarized by all the monthly record. [16:   The base number is basically equal to the final reading for last monitoring period.]  [17:  There are No.4 Village Group, Zhengrongfu, Taishan Villa and Wangdong Community 4 sub-areas.] 


As per B.7.3 of the registered PDD, all data collected as part of monitoring plan should be saved with at least 1 backup copy until the end of the crediting period. After the crediting period ends, the data should be archived electronically on hard disks and be kept at least 2 years after the end of the last crediting period.

Training for the GS monitoring team
Only skilled employees are allowed to undertake the monitoring work. During this monitoring period, one training session was conducted by the project owner on 10/10/2023. The contents included mechanism of GS Standard and emission reductions, basic understanding of climate change, all the parameters to be monitored, monitoring methodology and frequency for related parameters, requirements for data collecting and archiving, internal data verification procedures and some other attentions.
Training notice and attendance lists of the GS Monitoring Team can be taken as evidence.

Emergency procedure
In case of water leakage or other system error, the emergency plan shall be taken immediately and reported to the project owner. If necessary, the use of relevant equipment shall be suspended. The project owner shall arrange professionals to repair and maintain the equipment as soon as possible. For missing data, conservative value will be used as per the registered PDD. There was no emergency or missing data occurred during this monitoring period.

Corrective actions
The whole GS monitoring team fellow recognized standard data evaluation methods to guarantee that the data was reliable and accurate. There was no correction of nonconformities occurred in implementation of the project or the monitoring plan during this monitoring period. For QA/QC procedure, please refer to QA/QC procedures in section D.2 of the monitoring report.

Avoiding of double counting
There is a unique identification code for each heat substation (1# TS4G, 2# TS4G, 3# TSZR, 4# TSTS, 5# TSTS and 6# TSWD), which will prevent the geothermal heating system counted in the project activity to be part of any other voluntary market or emission reduction mechanism (CDM, CCER, VCS etc.) as well. Besides, the project owner has signed the Declaration of No Double Counting and not involved in other GHG scheme statement on 20/11/2023. 

[bookmark: _Hlk122684244]There is a cap & trade scheme in China. However, the project activity is not included in the mandatory emission control scheme since the scheme only cover the high-emission industries, such as power generation sector that emitted at least 26,000 tons of CO2e/year[footnoteRef:18]. China is planned to include another 7 industries (petrochemicals, chemicals, building materials, non-ferrous metals, papermaking, steel and aviation) in the national carbon market[footnoteRef:19]. Besides, Henan province is not among the nine pilot areas (Guangdong, Hubei, Tianjin, Beijing, Shanghai, Chongqing, Shenzhen, Sichuan and Fujian) of China Emission Trading System (CETS). As above, the project activity does not belong to the above compliance industry and there are no mandatory requirements on GHG emissions of the project owner[footnoteRef:20]. The emission reductions were not double counted during this monitoring period.   [18:  https://www.mee.gov.cn/xxgk2018/xxgk/xxgk06/202310/t20231018_1043427.html]  [19:  "Management Measures for Carbon Emissions Trading (Trial)" issued by the Ministry of Ecology and Environment in December of 2020. https://www.mee.gov.cn/gzk/gz/202112/t20211213_963865.shtml]  [20:  https://www.mee.gov.cn/xxgk2018/xxgk/xxgk03/202012/W020201230736907682380.pdf] 

[bookmark: _Ref47706326][bookmark: _Ref49860677][bookmark: _Toc40962747]SECTION D. DATA AND PARAMETERS
[bookmark: _Toc40962748][bookmark: _Ref418094907]D.1. Data and parameters fixed ex ante or at renewal of crediting period
>>
SDG13
	Data/parameter
	EFCO2,i

	Unit
	tCO2/TJ

	Description
	The CO2 emission factor per unit of energy of the fuel of technology i that would have been used in the baseline heating technology. 

	Source of data
	Option (d) IPCC default values at the lower limit of the uncertainty at a 95% confidence interval as provided in table 1.4 of Chapter 1 of Vol.2 (Energy) of 2006 IPCC Guidelines on National GHG Inventories is used as per Table 5 of the applied methodology AM0072 (Version 03.0).

	Value(s) applied
	87.3

	Choice of data or Measurement methods and procedures 
	Values provided by the fuel supplier are unavailable. IPCC default values at the lower limit of the uncertainty at a 95% confidence interval as provided in table 1.4 of Chapter 1 of Vol.2 (Energy) of 2006 IPCC Guidelines on National GHG Inventories[footnoteRef:21] are used. For coking coal, it is 87.3 tCO2/TJ. [21:  The latest IPCC methodology report “2019 Refinement to the 2006 IPCC Guidelines for National Greenhouse Gas Inventories” did not revise the relevant data for calculating this parameter, so the source is still IPCC 2006.] 


	Purpose of data
	To calculate baseline emissions

	Additional comment
	Where several fuel types are used in the boiler, use the fuel type with the lowest CO2 emission factor. CO2 emission factor of other bituminous coal and sub-bituminous coal are 89.5 tCO2/TJ and 92.8 tCO2/TJ separately, which are higher than that of coking coal. Coking coal and brown coal briquettes have the same CO2 emission factor. Coking coal is usually used for heating in coal boiler.



	Data/parameter
	ηBL,i

	Unit
	Dimensionless

	Description
	Net thermal efficiency of the boiler technology i using fossil fuel that would have been used in the absence of the project activity.

	Source of data
	Follow the guidance given in the applied methodology AM0072 (Version 03.0).

	Value(s) applied
	85

	Choice of data or Measurement methods and procedures 
	The highest efficiency of coal-fired boilers provided by Zozen Boilers (79%), Fengcheng Energy Equipment Factory (80%) and Henan Hengxin Boiler Manufacturing Co., Ltd (85%).
As per Table 4 Default baseline efficiency for different boilers of AM0072 (Version 03.0), the highest value of 85% for new coal-fired boiler is applicable for the project.
In summary, the efficiency of 85% is applied for the project.

	Purpose of data
	To calculate baseline emissions

	Additional comment
	N/A



	Data/parameter
	LossBLi,y

	Unit
	TJ/yr

	Description
	The net distribution losses of the heat supply system, in the absence of project activity, during the year y.

	Source of data
	Section 5.4.6.3 of AM0072 (Version 03.0).

	Value(s) applied
	0

	Choice of data or Measurement methods and procedures 
	The historic information is not available, a conservative value of 0% of losses can be used as per paragraph 66 option 1 of AM0072 (Version 03.0).

	Purpose of data
	To calculate baseline emissions

	Additional comment
	N/A



	Data/parameter
	Subscript i

	Unit
	/

	Description
	Type of technology used in the baseline scenario.

	Source of data
	Feasibility Study Report of the project

	Value(s) applied
	Coal fired boilers in boiler houses, supplying several buildings through a heat distribution network.

	Choice of data or Measurement methods and procedures 
	As per section 5.2 of AM0072 Fossil Fuel Displacement by Geothermal Resources for Space Heating (Version 03.0), the most plausible baseline scenario shall be determined through the use of Tool 02 Combined tool to identify the baseline scenario and demonstrate additionality (Version 07.0). Heat supply system using coal-fired boilers is identified as the baseline scenario of the project activity. Refer to section B.4 of the PDD for more details.

	Purpose of data
	To calculate baseline emissions

	Additional comment
	Data shall be stored in an excel sheet/database



	Data/parameter
	Subscript j

	Unit
	/

	Description
	Geothermal well number.

	Source of data
	Feasibility Study Report of the project

	Value(s) applied
	Geothermal wells number j = 1 to 22.

	Choice of data or Measurement methods and procedures 
	There are a total of 22 geothermal wells including 11 production wells and 11 re-injection wells in the boundary of the project activity as per Feasibility Study Report, which can be identified through unique identification code.

	Purpose of data
	To calculate baseline emissions

	Additional comment
	Distinct geothermal well with distinct properties of temperature, pressure and flow volume.



	Data/parameter
	Subscript m

	Unit
	/

	Description
	Space heating construction type

	Source of data
	Feasibility Study Report of the project

	Value(s) applied
	Residential and commercial

	Choice of data or Measurement methods and procedures 
	Identified by local urban planners under a short to medium term development plan for the area.

	Purpose of data
	To calculate baseline emissions

	Additional comment
	Areas designated for space heating under the categories of residential, commercial and industrial space heat



	Data/parameter
	Subscript k

	Unit
	/

	Description
	Sub-station number

	Source of data
	Feasibility Study Report of the project

	Value(s) applied
	Sub-station number k=1 to 6

	Choice of data or Measurement methods and procedures 
	There is a total of 6 sub-stations in the boundary of the project activity, which can be identified through unique identification code and GPS coordinates.

	Purpose of data
	To calculate baseline emissions

	Additional comment
	Includes a heat exchanger as part of the sub-station.



	Data/parameter
	LossPJy

	Unit
	TJ/yr

	Description
	Net distribution loss of the geothermal heat supply system during the year y.

	Source of data
	Calculated based on design heat losses from heat network manufacturer per the methodology. 

	Value(s) applied
	Refer to ER calculation sheet for more details.

	Choice of data or Measurement methods and procedures 
	As per approved PDD, the heat losses are determined based on heat losses from pipeline, valves, fittings based on maximum of option (a) 10% design heat losses provided by the engineering specifications of the manufacturer of the heat network. Therefore,  
Where:
Am=Net heating area for construction type m
HIm=Heating index for construction type m
Tj=Hours per hear heat utilization in well j
CF=Conversion factor from GWh to TJ (3.6).

	Purpose of data
	To calculate baseline emissions

	Additional comment
	N/A



	Data/parameter
	wi

	Unit
	/

	Description
	Heat generation ratio for baseline heating technology i

	Source of data
	Paragraph 51(a)(ii) option 2 Assign weights based on available historical records of AM0072 (Version 03.0).

	Value(s) applied
	1

	Choice of data or Measurement methods and procedures 
	As per section B.4 of this PDD, the baseline scenario of the project is 3(i) “Coal fired boilers in boiler houses, supplying several buildings through a heat distribution network”. Only one technology would be used. According to Research on Heating in Winter of Taishan village published by Xinzheng Housing and Urban-Rural Development Bureau, all the heating in winter of residential and commercial buildings were supplied by coal fired boilers. As per paragraph 51(a)(ii) option 2 Assign weights based on available historical records of AM0072 (Version 03.0), wi is equal to 1.

	Purpose of data
	To calculate baseline emissions

	Additional comment
	N/A



	Data / Parameter
	Hff

	Unit
	TJ

	Description
	Heat supplied by fossil fuel boiler; in case a boiler is used to meet the heat demand of network.

	Source of data
	On site metering of heat (e.g. flow of steam/hot water multiplied by enthalpy) at the outlet of the boiler. 

	Value(s) applied
	There are no fossil fuel boilers used to meet the heat demand of the project heating network. Therefore, Hff=0 TJ.

	Choice of data or Measurement methods and procedures
	/

	Purpose of data
	To calculate baseline emissions

	Additional comment
	N/A



[bookmark: _Toc40962777][bookmark: _Ref418094911]D.2 Data and parameters monitored
>>
The start date of the 2023-2024 heating season is 01/11/2023, and heating supply is not needed from 01/04/2023 to 31/10/2023. Therefore 0 value is used for the parameter of Δtj,d,y, FRj,d,y, Tj and ECPJ,j,y (ECy) from 01/04/2023 to 31/10/2023.

SDG 13
	Data / Parameter
	Δtj,d,y

	Unit
	°C

	Description
	Average temperature difference between inlet and outlet temperatures at the downstream of each heat exchanger in year y.

	Source of data
	Operation record of the geothermal based space heating system. 

	Value(s) of monitored parameter
		Sub-areas
	Heat Substations
	Production and Re-injection Well
	Nov-2023
	Dec-2023
	Jan-2024
	Feb-2024
	Mar-2024

	No.4 Village Group
	1# TS4G
	1#
	11.53
	11.49
	11.49
	11.51
	11.52

	
	
	2#
	11.49
	11.54
	11.49
	11.48
	11.45

	
	2# TS4G
	3#
	11.47
	11.47
	11.47
	11.49
	11.42

	
	
	4#
	11.25
	11.22
	11.18
	11.20
	11.26

	Zhengrongfu
	3# TSZR
	5#
	11.44
	11.39
	11.41
	11.44
	11.48

	
	
	6#
	11.29
	11.27
	11.26
	11.24
	11.26

	Taishan Villa
	4# TSTS
	7#
	11.69
	11.72
	11.77
	11.72
	11.73

	
	5# TSTS
	8#
	11.29
	11.23
	11.25
	11.27
	11.27

	
	
	9#
	11.45
	11.49
	11.55
	11.51
	11.48

	Wangdong Community
	6# TSWD
	10#
	10.98
	11.08
	11.02
	10.94
	11.03

	
	
	11#
	11.19
	11.05
	11.09
	11.09
	11.17




	Measurement methods and procedures
	Outlet temperature minus inlet temperature at the downstream of each heat exchanger j. The outlet temperature is monitored by the 11 ultrasonic calorimeters installed at the “UC outlet” in figure 3 in section C. The inlet temperature is monitored by the 11 ultrasonic calorimeters installed at the “UC inlet” in figure 3 in section C.
Inlet and outlet temperatures at the downstream of each heat exchanger are monitored by the ultrasonic calorimeters. There are 11 production wells and 11 re-injection wells. One production well and one re-injection well form one set of heat exchange system. There are totally 11 sets of heat exchange system. 22 ultrasonic calorimeters are needed to monitor the inlet and outlet temperatures of all the heat exchange system. Refer to Figure 3 of the MR for more details on installation and configuration of the ultrasonic calorimeters. 
Serial No. of the ultrasonic calorimeters are Lu00000858, Lu00000859, Lu00000860, Lu00000861, Lu00000862, Lu00000863, Lu00000864, Lu00000865, Lu00000866, Lu00000867, Lu00000868, Lu00000869, Lu00000870, Lu00000871, Lu00000872, Lu00000873, Lu00000874, Lu00000875, Lu00000876, Lu00000877, Lu00000878 and Lu00000879 separately.
The ultrasonic calorimeters can monitor the inlet and outlet temperature of each heat exchange system continuously and record the temperature data per hour. All the hourly temperature data were exported by the GS monitoring team to form the monthly record at the beginning of the next month. The average daily inlet and outlet temperature were calculated based on the 24-hourly temperature data separately. The average monthly inlet and outlet temperature were calculated based on all the daily inlet and outlet temperature of this month. Finally, the operation record of the geothermal heating system during the related heating season were summarized by all the monthly record.

	Monitoring frequency
	Measured Hourly/Recording Monthly

	QA/QC procedures
	Ultrasonic calorimeters have been checked regularly for potentially performance-reducing anomalies by the GS monitoring team. The temperature measurement range of the ultrasonic calorimeters are 4 °C to 95 °C with an accuracy of 0.01 °C.
The ultrasonic calorimeters are calibrated based on JJG 225-2001 Verification Regulation of Heat Meters. Calibration of the 22 ultrasonic calorimeters is shown as the following table.
	NO.
	Serial No.
	Purpose
	Calibration Date
	Term of Validity

	1
	Lu00000858
	To monitor supply water temperature of 1# heat exchange system
	16/10/2023
	15/10/2026

	2
	Lu00000859
	To monitor supply water temperature of 2# heat exchange system
	16/10/2023
	15/10/2026

	3
	Lu00000860
	To monitor supply water temperature of 3# heat exchange system
	16/10/2023
	15/10/2026

	4
	Lu00000861
	To monitor supply water temperature of 4# heat exchange system
	17/10/2023
	16/10/2026

	5
	Lu00000862
	To monitor supply water temperature of 5# heat exchange system
	17/10/2023
	16/10/2026

	6
	Lu00000863
	To monitor supply water temperature of 6# heat exchange system
	17/10/2023
	16/10/2026

	7
	Lu00000864
	To monitor supply water temperature of 7# heat exchange system
	18/10/2023
	17/10/2026

	8
	Lu00000865
	To monitor supply water temperature of 8# heat exchange system
	18/10/2023
	17/10/2026

	9
	Lu00000866
	To monitor supply water temperature of 9# heat exchange system
	18/10/2023
	17/10/2026

	10
	Lu00000867
	To monitor supply water temperature of 10# heat exchange system
	19/10/2023
	18/10/2026

	11
	Lu00000868
	To monitor supply water temperature of 11# heat exchange system
	19/10/2023
	18/10/2026

	12
	Lu00000869
	To monitor return water temperature of 1# heat exchange system
	19/10/2023
	18/10/2026

	13
	Lu00000870
	To monitor return water temperature of 2# heat exchange system
	20/10/2023
	19/10/2026

	14
	Lu00000871
	To monitor return water temperature of 3# heat exchange system
	20/10/2023
	19/10/2026

	15
	Lu00000872
	To monitor return water temperature of 4# heat exchange system
	20/10/2023
	19/10/2026

	16
	Lu00000873
	To monitor return water temperature of 5# heat exchange system
	21/10/2023
	20/10/2026

	17
	Lu00000874
	To monitor return water temperature of 6# heat exchange system
	21/10/2023
	20/10/2026

	18
	Lu00000875
	To monitor return water temperature of 7# heat exchange system
	22/10/2023
	21/10/2026

	19
	Lu00000876
	To monitor return water temperature of 8# heat exchange system
	22/10/2023
	21/10/2026

	20
	Lu00000877
	To monitor return water temperature of 9# heat exchange system
	22/10/2023
	21/10/2026

	21
	Lu00000878
	To monitor return water temperature of 10# heat exchange system
	23/10/2023
	22/10/2026

	22
	Lu00000879
	To monitor return water temperature of 11# heat exchange system
	23/10/2023
	22/10/2026


There were no missing data or damaged data during this monitoring period. The average temperature change of the 11 heat exchange systems of the 2023-2024 heating season is 11.36°C[footnoteRef:22]. As per feedback from the space heating experts at the project site, the design temperature difference of the end-user is 10-15 °C and the average temperature change of the 11 heat exchange systems of the Taishan geothermal heating system is about 12°C. Therefore, the average temperature change of 11.36°C in this monitoring period is reasonable and conservative. [22:  The average temperature change of the 11 heat exchange systems of the 2023-2024 heating season can be calculated as average temperature changes in November 2023, December 2023, January 2024, February 2024 and March 2024, which is (11.37℃+11.36℃+11.36℃+11.35℃+11.37℃)/5=11.36℃.] 


	Purpose of data
	To calculate baseline emissions

	Additional comment
	The heat exchanger should handle the heat supplied by geothermal well only and not by any other source. The temperature readings should be taken at immediate inlet and outlet point of heat exchanger.



	Data / Parameter
	FRj,d,y

	Unit
	kg/h

	Description
	Average flow rate at the downstream of each heat exchanger (upstream of which is connected with water supply from the geothermal well j) in year y.

	Source of data
	Operation record of the geothermal based space heating system.

	Value(s) of monitored parameter
		Sub-areas
	Heat Substations
	Production and Re-injection Well
	Nov-2023
	Dec-2023
	Jan-2024
	Feb-2024
	Mar-2024

	No.4 Village Group
	1# TS4G
	1#
	850,190.00
	850,278.91
	851,228.98
	849,992.04
	849,809.41

	
	
	2#
	838,977.00
	838,756.90
	837,378.43
	837,076.78
	838,075.73

	
	2# TS4G
	3#
	846,560.86
	845,323.23
	846,891.95
	845,277.13
	845,129.40

	
	
	4#
	830,940.86
	830,644.34
	830,598.51
	829,738.23
	830,593.31

	Zhengrongfu
	3# TSZR
	5#
	852,414.86
	850,659.95
	850,869.66
	852,596.93
	851,461.47

	
	
	6#
	837,284.46
	837,191.77
	837,484.03
	837,189.83
	837,247.85

	Taishan Villa
	4# TSTS
	7#
	845,621.22
	845,513.94
	845,088.02
	844,915.60
	845,226.10

	
	5# TSTS
	8#
	845,210.07
	844,846.01
	845,914.41
	845,624.05
	844,313.90

	
	
	9#
	830,087.44
	831,464.45
	831,843.88
	830,837.30
	831,272.22

	Wangdong Community
	6# TSWD
	10#
	860,592.25
	860,072.92
	861,129.02
	861,498.26
	861,290.55

	
	
	11#
	850,072.50
	849,788.55
	850,228.32
	849,111.06
	850,259.99




	Measurement methods and procedures
	Average flow rate at the downstream of each heat exchanger are monitored by the 11 ultrasonic calorimeters. Refer to “UC outlet” in Figure 3 of the MR for more details on installation and configuration of the ultrasonic calorimeters. Serial No. of the ultrasonic calorimeters are Lu00000858, Lu00000859, Lu00000860, Lu00000861, Lu00000862, Lu00000863, Lu00000864, Lu00000865, Lu00000866, Lu00000867, Lu00000868 separately.
The ultrasonic calorimeters can monitor the volume flow rate of each heat exchange system continuously and record it per hour. All the hourly volume flow rate data were exported by the GS monitoring team to form the monthly record at the beginning of the next month. The average daily volume flow rate was calculated based on the 24-hourly data. The average monthly volume flow rate was calculated based on all the daily data of this month. Finally, the operation record of the geothermal heating system during the related heating season were summarized by all the monthly record. Density of the water is 1,000 kg/m3. Mass flow can be calculated as volume flow rate times density of water.

	Monitoring frequency
	Measured hourly/Recording monthly

	QA/QC procedures
	Ultrasonic calorimeters have been checked regularly for potentially performance-reducing anomalies by the GS monitoring team. The highest measurement flow rate range of the ultrasonic calorimeters are 1,000 m3/h with an accuracy of 0.01 m3/h.
The ultrasonic calorimeters are calibrated based on JJG 225-2001 Verification Regulation of Heat Meters. Calibration of the 11 ultrasonic calorimeters is shown as the following table.
	NO.
	Serial No.
	Purpose
	Calibration Date
	Term of Validity

	1
	Lu00000858
	To monitor flow rate of 1# heat exchange system
	16/10/2023
	15/10/2026

	2
	Lu00000859
	To monitor flow rate of 2# heat exchange system
	16/10/2023
	15/10/2026

	3
	Lu00000860
	To monitor flow rate of 3# heat exchange system
	16/10/2023
	15/10/2026

	4
	Lu00000861
	To monitor flow rate of 4# heat exchange system
	17/10/2023
	16/10/2026

	5
	Lu00000862
	To monitor flow rate of 5# heat exchange system
	17/10/2023
	16/10/2026

	6
	Lu00000863
	To monitor flow rate of 6# heat exchange system
	17/10/2023
	16/10/2026

	7
	Lu00000864
	To monitor flow rate of 7# heat exchange system
	18/10/2023
	17/10/2026

	8
	Lu00000865
	To monitor flow rate of 8# heat exchange system
	18/10/2023
	17/10/2026

	9
	Lu00000866
	To monitor flow rate of 9# heat exchange system
	18/10/2023
	17/10/2026

	10
	Lu00000867
	To monitor flow rate of 10# heat exchange system
	19/10/2023
	18/10/2026

	11
	Lu00000868
	To monitor flow rate of 11# heat exchange system
	19/10/2023
	18/10/2026



There were no missing data or damaged data during this monitoring period. The average volume flow rate of the 11 heat exchange system of the 2023-2024 heating season (844.18 m3/h)[footnoteRef:23] were cross checked by the rated flow of the circulating pumps, which are 1,750 m3/h (250 m3/h*7) for 1#TS4G heat substation, 2,340 m3/h (260 m3/h*9) of 2# TS4G heat substation, 2,700 m3/h (300 m3/h*9) for 3#TSZR heat substation, 1,600 m3/h (200 m3/h*8) for 4#TSTS heat substation, 2,000 m3/h (250 m3/h*8) for 5# TSTS heat substation and 2,450  m3/h (350 m3/h*7) for 6# TSWD heat substation (refer to Table 3 of the registered PDD for more details).  The average volume flow rate of the 11 heat exchange systems of the 2023-2024 heating season were lower than the least rated flow of the circulating pumps (1,600 m3/h). As per feedback from the space heating experts at the project site, average volume flow rate of the 11 heat exchange systems of the Taishan geothermal heating system is about 845 m3/h.  Therefore, the average flow rate of 844.18 m3/h in this monitoring period is reasonable and conservative. [23:  The average volume flow rate of the 11 heat exchange systems of the 2023-2024 heating season can be calculated as (850.30 m3/h +838.05 m3/h +845.84 m3/h +830.50m3/h +851.60 m3/h +837.28 m3/h +845.27 m3/h +845.18 m3/h +831.10 m3/h +860.92 m3/h +849.89 m3/h)/11=844.18 m3/h. ] 


	Purpose of data
	To calculate baseline emissions

	Additional comment
	The heat exchanger should handle the heat supplied by geothermal well only and not by any other source.



	Data / Parameter
	Tj

	Unit
	Hours

	Description
	[bookmark: OLE_LINK1]Hours per hear heat utilization in well j.

	Source of data
	Operation record of the geothermal based space heating system.

	Value(s) of monitored parameter
		Sub-areas
	Heat Substations
	Production and Re-injection Well
	Nov-2023
	Dec-2023
	Jan-2024
	Feb-2024
	Mar-2024

	No.4 Village Group
	1# TS4G
	1# 
	720
	744
	744
	696
	744

	
	
	2# 
	720
	744
	744
	696
	744

	
	2# TS4G
	3# 
	720
	744
	744
	696
	744

	
	
	4# 
	720
	744
	744
	696
	744

	Zhengrongfu
	3# TSZR
	5# 
	720
	744
	744
	696
	744

	
	
	6# 
	720
	744
	744
	696
	744

	Taishan Villa
	[bookmark: _Hlk76834834]4# TSTS
	7# 
	480
	496
	527
	464
	558

	
	5# TSTS
	8# 
	720
	744
	744
	696
	744

	
	
	9# 
	720
	744
	744
	696
	744

	Wangdong Community
	6# TSWD
	10# 
	720
	744
	744
	696
	744

	
	
	11# 
	720
	744
	744
	696
	744




	Measurement methods and procedures
	The actual number of heating hours are sourced from operation record of the geothermal based space heating system. 
Monthly operation time of the 11 heat exchange systems were recorded by the GS monitoring team based on the geothermal based space heating system at the beginning of the next month. The operation record of the geothermal heating system during the related heating season were summarized by all the monthly record.

	Monitoring frequency
	Monthly

	QA/QC procedures
	The winter heating season is usually fixed by local regulations. As per Research on Heating in Winter of Taishan Village published by Xinzheng Housing and Urban-Rural Development Bureau, winter heating season of Taishan Village is usually from November 1 to March 31 of the next year (last day excluded[footnoteRef:24], 150 days). The actual 2023-2024 heating season of Taishan Village is from 01/11/2023 to 31/03/2024 (first and last days included, totally 152 days). For residential buildings, 24-hour continuous heating supply are needed, and for commercial buildings, 24-hour continuous heating supply is not required (usually 15-20 hours a day)[footnoteRef:25]. The heating hours of commercial buildings from November 2023 to March 2024 are 480h, 496h, 527h, 464h and 558h respectively. Therefore, the total number heating hours of commercial buildings in this monitoring period is 480+496+527+464+558=2,525h, and the total number heating hours of residential buildings in this monitoring period is 720+744+744+696+744=3,648h. [24:  As per Research on Heating in Winter of Taishan Village published by Xinzheng Housing and Urban-Rural Development Bureau, the cut-off time of winter heating usually to be 24:00 of the 30th-March of each year. The last day of March usually to be the settlement day. But the actual number of heating hours may vary from year to year, which is determined by the winter climate of the year.]  [25:  As per Research on Heating in Winter of Taishan Village published by Xinzheng Housing and Urban-Rural Development Bureau, the heating hours of commercial buildings is usually 15-20 hour a day. Actual heating hours may vary for different commercial types.] 


	Purpose of data
	To calculate baseline emissions

	Additional comment
	The heat exchanger should handle the heat supplied by geothermal well only and not by any other source.



	Data / Parameter
	[bookmark: _Hlk76804280]HIm

	Unit
	W/m2

	Description
	Heating index for construction type m.

	Source of data
	The conservative standard index for construction type m as provided by the standards institute of China (CJJ/T34-2022 Design standards for urban heating pipe networks published on 29/04/2022 by Ministry of Housing and Urban-Rural Development of the People’s Republic of China[footnoteRef:26]).  [26:  https://www.mohurd.gov.cn/gongkai/zhengce/zhengcefilelib/202207/20220704_767030.html] 


	Value(s) of monitored parameter
	45 W/m2 for residential buildings and 55 W/m2 for commercial buildings.

	Measurement methods and procedures
	/

	Monitoring frequency
	Once every monitoring period.

	QA/QC procedures
	As per feedback from the space heating experts at the project site, heating index of the Taishan geothermal heating system is 45 W/m2 for residential buildings and 55 W/m2 for commercial buildings, which are comply with requirement of CJJ/T34-2022 Design standards for urban heating pipe networks published on 29/04/2022 by Ministry of Housing and Urban-Rural Development of the People’s Republic of China.

	Purpose of data
	To calculate baseline emissions

	Additional comment
	N/A



	Data / Parameter
	ECPJ,j,y (ECy)

	Unit
	MWh

	Description
	Electricity consumption for the year y in operating the geothermal heating system.

	Source of data
	Record of the Electricity Meters

	Value(s) of monitored parameter
		Time
	ECPJ,j,y (MWh)

	01/04/2023-31/10/2023
	0

	01/11/2023-31/11/2023
	2,617,675.38 

	01/12/2023-31/12/2023
	2,630.33779 

	01/01/2024-31/01/2024
	2,524.74886

	01/02/2024-29/02/2024
	2,522.86790 

	01/03/2024-31/03/2024
	2,682.45439

	Total
	12,978,084.32




	Measurement methods and procedures
	Electricity consumptions of the geothermal heating system are monitored by the electricity meters installed at each heat substation. Totally 6 electricity meters are needed. Refer to Figure 3 of the MR for more details on installation and configuration of the electricity meters. Serial No. of the electricity meters are 111520042063, 111520042064, 111520042065, 111520042066, 111520042067 and 111520042068 separately.
Before the 2023-2024 heating season, base number of all the 6 electricity meters were recorded by the GS monitoring team under the supervision of the representative of each sub-area[footnoteRef:27]. At the end of each heating month, the GS monitoring team recorded readings of the 6 electricity meters, which can calculate the electricity consumption of this month by minus last month’s base number of meters. The operation record of the geothermal heating system during the related heating season were summarized by all the monthly record. [27:  There are No.4 Village Group, Zhengrongfu, Taishan Villa and Wangdong Community 4 sub-areas.] 

Electricity consumption of the geothermal space heating system is only part of the power consumption in public area of each sub-area. All the electricity costs during the heating season were settled by the community property service company of each sub-area and local power grid company, which includes the electricity consumption of the geothermal heating system. 
Electricity settlement agreement was signed between the project owner and the community property service company of each sub-area. At the end of each winter heating season, the project owner prepares electricity bill to the related community property service company for confirmation, which contains name of the community property service company, period of the electricity consumption, related electricity consumption, information of the electricity meters (location, serial number, accuracy, highest range and stop number of this heating season) and the related charges. The project owner would pay the bill and payment receipt would be provided by the related community property service company.

	Monitoring frequency
	Measured Continuously/Recorded monthly

	QA/QC procedures
	The accuracy of the electricity meters is 0.5S.
The electricity meters are calibrated based on JJG 596-2012 Electrical Meters for Measuring Alternating-current Electrical Energy. All the 6 electricity meters were calibrated during test run period (24/10/2020-31/10/2020) of the geothermal heating system and as per the JJG 596-2012, the calibration cycle should not exceed 6 years.  Calibration of the 6 electricity meters is shown as the following table. 
	NO.
	Serial No.
	Location
	Model/Accuracy
	Calibration Date
	Term of Validity

	1
	[bookmark: _Hlk78991604]111520042063
	1# TS4G heat substation
	DDS606 15(60)A/0.5S
	24/10/2020
	23/10/2025

	2
	111520042064
	2# TS4G heat substation
	DDS606 15(60)A/0.5S
	24/10/2020
	23/10/2025

	3
	111520042065
	3# TSZR heat substation
	DDS606 15(60)A/0.5S
	24/10/2020
	23/10/2025

	4
	111520042066
	4# TSTS heat substation
	DDS606 15(60)A/0.5S
	25/10/2020
	24/10/2025

	5
	111520042067
	5# TSTS heat substation
	DDS606 15(60)A/0.5S
	25/10/2020
	24/10/2025

	6
	111520042068
	6# TSWD heat substation
	DDS606 15(60)A/0.5S
	25/10/2020
	24/10/2025



There were no missing data or damaged data during this monitoring period. All the electricity consumption data was cross checked with the electricity bill confirmed by each community property service company and payment receipt of the geothermal heating system. The electricity consumption data of the 2023-2024 heating season used in the MR were consist with the electricity bills of each sub-area.

	Purpose of data
	To calculate project emissions

	Additional comment
	N/A



	Data / Parameter
	EFEL,j,y (EFgrid,CM,y)

	Unit
	tCO2/MWh

	Description
	Combined margin emission factor for the grid in year y.

	Source of data
	Taishan village is in Henan province, which belongs to Central China Regional Power Grid (CCPG). The data of CCPG’s Baseline emission factors of China's regional power grid for emission reduction projects in 2023 published by China National Climate Strategy Center on 08/07/2024[footnoteRef:28], which calculated EFgrid,OM,y and EFgrid,BM,y based on Tool 07 (Version 07.0).  [28:  https://ccer.cets.org.cn/notice/columnDetail?bulletinBoardId=1151185363440635904&bulletinBoardName=%E7%94%B5%E7%BD%91%E5%9F%BA%E5%87%86%E7%BA%BF%E6%8E%92%E6%94%BE%E5%9B%A0%E5%AD%90] 

As per formular 15 of the registered PDD, EFgrid,CM,y can be calculated as EFgrid,CM,y=EFgrid,OM,yωOM+EFgrid,BM,yωBM.  As per paragraph 86(b) of Tool 07 (Version 07.0), ωOM=0.5 and ωBM=0.5 are used for the 1st crediting period. It’s the 4th monitoring period of the project which belongs to the first crediting period. Therefore, ωOM=0.5 and ωBM=0.5 were used.

	Value(s) of monitored parameter
	0.57335 (0.8771 tCO2/MWh*0.5+0.2696 tCO2/MWh*0.5)

	Measurement methods and procedures
	Taishan village is in Henan province, which belongs to Central China Regional Power Grid (CCPG). The data of CCPG’s EFgrid,OM,y and EFgrid,BM,y were taken from Baseline emission factors of China's regional power grid for emission reduction projects in 2023, which are the latest version published by China National Climate Strategy Center on 08/07/2024. If new version issued, the value of EFgrid,OM,y and EFgrid,BM,y should be updated. 

	Monitoring frequency
	Once per year

	QA/QC procedures
	The latest version of Baseline emission factors of China's regional power grid for emission reduction projects published by China National Climate Strategy Center were used for the 4th monitoring period. It calculated EFgrid,OM,y and EFgrid,BM,y based on the latest version of Tool 07 (Version 07.0).

	Purpose of data
	To calculate project emissions

	Additional comment
	N/A



	Data / Parameter
	TDLj,y

	Unit
	/

	Description
	Average technical transmission and distribution losses for providing electricity to source j in year y.

	Source of data
	As per Tool 05 (Version 03.0), In case of scenario B and scenario C, case C.II, assume TDLj,y=0 as a simplification. In case of other scenarios (scenario A and scenario C, cases C.I and C.III), choose one of the following options: 
1. Use annual average value based on the most recent data available within the host country; 
2. Use as default values of 20% for: 
(a) project or leakage electricity consumption sources; (b) baseline electricity consumption sources if the electricity consumption by all project and leakage electricity consumption sources to which scenario A or scenario C (cases C.I or C.III) applies is larger than the electricity consumption of all baseline electricity consumption sources to which scenario A or scenario C (cases C.I or C.III) applies; 
3. Use as default values of 3% for: 
(a) baseline electricity consumption sources; 
(b) project and leakage electricity consumption sources if the electricity consumption by all project and leakage electricity consumption sources to which scenario A or scenario C (cases C.I or C.III) applies is smaller than the electricity consumption of all baseline electricity consumption sources to which scenario A or scenario C (cases C.I or C.III) applies.

	Value(s) of monitored parameter
	20%

	Measurement methods and procedures
	Scenario A: Electricity consumption from the grid is applied to the project. For project electricity consumption sources, a default value of 20% is used for TDLj,y.

	Monitoring frequency
	Annually. In the absence of data from the relevant year, most recent figures should be used, but not older than 5 years.

	QA/QC procedures
	/

	Purpose of data
	To calculate project emissions

	Additional comment
	For (a): TDLj,y should be estimated for the distribution and transmission networks of the electricity grid of the same voltage as the connection where the project activity is connected to. The technical distribution losses should not contain other types of grid losses (e.g. commercial losses/theft). The distribution losses can either be calculated by the project participants or be based on references from utilities, network operators or other official documentation.



SDG7 and SDG 13
	Data / Parameter
	Am

	Unit
	m2

	[bookmark: _Hlk68798412]Description
	Net heating area for construction type m.

	Source of data
	Heating supply contracts. (2023-2024 Heating season)

	Value(s) of monitored parameter
		Sub-areas
	Heat Substations
	Residential
	Commercial

	No.4 Village Group
	1# TS4G
	255,272.8
	0.00

	
	
	
	

	
	2# TS4G
	509,349.84
	0.00

	
	
	
	

	Zhengrongfu
	3# TSZR
	720,582.43
	0.00

	
	
	
	

	Taishan Villa
	4# TSTS
	0.00
	94,236.26

	
	5# TSTS
	425,598.73
	0.00

	
	
	
	

	Wangdong Community
	6# TSWD
	548,928.53
	0.00

	
	
	
	

	Total
	2,459,732.33
	94,236.26




	Measurement methods and procedures
	Yearly measurement.

	Monitoring frequency
	Yearly

	QA/QC procedures
	The data was cross-checked with Certificate of Enterprise Investment Project in Henan Province issued by Xinzheng Development and Reform Commission. The net heating areas sourced from the heating supply contracts signed for the 2023-2024 heating season were lower than that of the government approval. The occupancy rate of the project area is less than 100%, unoccupied part of the residential area does not need heating supply during the 2023-2024 heating season.

	Purpose of data
	To calculate baseline emissions

	Additional comment
	N/A



SDG 8
	Data / Parameter
	Number of males and females employed by the project

	Unit
	Number

	Description
	Jobs created for both men and women.

	Source of data
	Record keeping book

	Value(s) of monitored parameter
	10 jobs created including 5 males and 5 females.

	Measurement methods and procedures
	Source of data was record keeping book and cross checked with the labor contracts.

	Monitoring frequency
	Once for each monitoring period.

	QA/QC procedures
	The results were also cross checked with training records of employees.

	Purpose of data
	To demonstrate contribution to SDG 8.

	Additional comment
	N/A



	[bookmark: _Hlk68774593]Data / Parameter
	Average monthly salary

	Unit
	RMB/person

	Description
	This parameter states the payment conditions of the people employed within the project. Equal pay for work of equal value regardless of gender.

	Source of data
	Record keeping book

	Value(s) of monitored parameter
	The project provides equal salaries for male and female in the same post. The monthly salary of the employees was:
4,400 RMB/person from 01/04/2023 to 31/12/2023, 5,000 RMB/person from 01/01/2024 to 31/03/2024 and 4,550 RMB/person for the 4th monitoring period.
[bookmark: OLE_LINK9][bookmark: OLE_LINK11][bookmark: OLE_LINK10][bookmark: OLE_LINK12][bookmark: OLE_LINK8]As per Notice on Adjusting the Minimum Wage Standard of Henan Province[footnoteRef:29] published by Henan Provincial People's Government on 27/12/2023, the minimum wage of Xinzheng is 2,100 RMB/month. In addition, as per the latest public information shows[footnoteRef:30] that the average salary in Zhengzhou[footnoteRef:31] in 2024 is 3,864 RMB/month. [29:  https://fgw.henan.gov.cn/2024/01-05/2880296.html]  [30:  https://upup.li/tools/salary/report/%e9%83%91%e5%b7%9e#:~:text=%E5%B9%B3%E5%9D%87%E5%B7%A5%E8%B5%84,%EF%BF%A53864]  [31:  This project is in Xinzheng city, which is a county-level city under the jurisdiction of Zhengzhou City, Henan Province, China.] 

[bookmark: OLE_LINK14]The average monthly salary provided by the project is 4,550 RMB/month from 01/04/2023 to 31/03/2024, which is higher than the minimum and average wage of Xinzheng.

	Measurement methods and procedures
	The average monthly salary was determined by the record keeping book and cross checked by the salary slips.

	Monitoring frequency
	Once for each monitoring period.

	QA/QC procedures
	The results were also cross checked with labor contracts.

	Purpose of data
	To demonstrate contribution to SDG 8.

	Additional comment
	N/A



[bookmark: _Toc40962778][bookmark: _Toc341456040]D.3. Comparison of monitored parameters with last monitoring period
	Data/Parameter
	Value obtained in this monitoring period
	Value obtained last monitoring period

	Δtj,d,y 
	11.36℃
	11.85℃

	FRj,d,y 
	844.18 m3/h
	844.41 m3/h

	Tj 
	152 days, 3,648 hours for residential buildings and 152 days, 2,525 hours for commercial buildings.
	151 days, 3,624 hours for residential buildings and 151 days, 2,420 hours for commercial buildings.

	HIm
	45 W/m2 for residential buildings and 55 W/m2 for commercial buildings.
	45 W/m2 for residential buildings and 55 W/m2 for commercial buildings.

	Am 
	2,459,732.33 m2 for residential buildings and 94,236.26 m2 for commercial buildings.
	2,441,477.26 m2 for residential buildings and 93,676.08 m2 for commercial buildings.

	ECPJ,j,y (ECy)
	12,978.08MWh
	13,160.08 MWh

	EFEL,j,y (EFgrid,CM,y)
	0.57335 tCO2/MWh
	0.5721 tCO2/MWh

	TDLj,y
	20%
	20%

	Number of males and females employed by the project
	10 jobs created including 5 males and 5 females.
	10 jobs created including 5 males and 5 females.

	Average monthly salary
	4,550 RMB/person
	4,100 RMB/person



[bookmark: _Hlk69481221]For the 4th monitoring period (01/04/2023-31/03/2024), all the 10 employees (including 5 females and 5 males) were the same as the last monitoring period. From 01/01/2024, monthly earnings of the employees were raised to 5,000 RMB/person (equal salaries paid for men and women in the same position). Therefore, the average monthly salary of employees in this monitoring period were more than that of last monitoring period. 

The value of HIm is sourced from FSR of the project, and it is the same with the last monitoring period. It meets the requirements of national standard CJJ/T 34-2022 Design standards for urban heating pipe networks published by Ministry of Housing and Urban-Rural Development of the People’s Republic of China, which is the latest version of the related standard. 

The value of TDLj,y is determined by the latest version of Tool 05. For this monitoring period, the Version 03.0 is used, which is the same as the last monitoring period.

The value of EFEL,j,y (EFgrid,CM,y) is calculated based on the latest baseline emission factors of China's regional power grid for emission reduction projects published by Chinese official government. Therefore, for this monitoring period, the latest available baseline emission factors should be sourced from Baseline emission factors of China's regional power grid for emission reduction projects in 2023, which is published on 08/07/2024 by National Climate Strategy Center[footnoteRef:32]. [32:  https://ccer.cets.org.cn/notice/noticeDetail?bulletinInfoId=1259913708889575424] 


The value of Am for the residential buildings during the 4th monitoring period is 0.75% higher than that of the 3rd monitoring period, which is determined by the occupancy rate of the project area for each heating season. Heating supply is not needed for the unoccupied part of the residential area. The value of Am for the commercial buildings is 0.60% higher than that of the 3rd monitoring period monitoring period, which is determined by the utilization rate of the commercial area for each heating season. Heating supply is also not needed for the vacant commercial area.

The value of Tj for residential buildings of the 4th monitoring period is 1 day longer than that of the last monitoring period. The actual 2023-2024 heating season of Taishan Village is from 01/11/2023 to 31/03/2024 (first and last days included, totally 152 days), 1 day longer than that of the last monitoring period. For the commercial buildings, the value of Tj is higher than that of the last monitoring period. For residential buildings, 24-hour continuous heating supply are needed, and for commercial buildings, 24-hour continuous heating supply is not required (usually 15-20 hour a day). The actual value recorded by the monitoring system shall prevail.

The values of Δtj,d,y ,FRj,d,y and ECPJ,j,y (ECy) during the 4th monitoring period are close to last monitoring period. There are slight changes in values of these parameters mainly determined by the heating demand of the end-users, which are affected by atmospheric environment temperature, running status of the geothermal heating system and other aspects. 
D.4. Implementation of sampling plan
>>
Not applicable.

[bookmark: _Toc317860226][bookmark: _Toc315189228][bookmark: _Toc341474081][bookmark: _Ref47706333][bookmark: _Toc40962779][bookmark: _Ref49860683]SECTION E. CALCULATION OF SDG IMPACTS
[bookmark: _Ref315873983][bookmark: _Ref418095428][bookmark: _Toc40962780]E.1. Calculation of baseline value or estimation of baseline situation of each SDG Impact
>>

[bookmark: _Hlk129097737]SDG 7 Impact of baseline situation
Without the project activity, 0 m2 of the building can access to geothermal energy-based space heating system in winter season.

SDG 8 Impact of baseline situation
Without the project activity, SDG 8 baseline impact was 0 job created and 0 monthly earning got.

SDG 13 Impact of baseline situation
Without the project activity, SDG 13 baseline impact was 0 tCO2e emission reduction achieved.

[bookmark: _Ref418095432][bookmark: _Ref315873986][bookmark: _Toc40962781]E.2. Calculation of project value or estimation of project situation of each SDG Impact
>>
SDG 7 Impact of project situation
As per the signed heating supply contract, heating areas (2023-2024 heating season) are summarized as the following table.
	Sub-areas
	Heat Substations
	Am (m2)

	
	
	Residential
	Commercial

	No.4 Village Group
	1# TS4G
	255,272.8
	0.00

	
	2# TS4G
	509,349.84
	0.00

	Zhengrongfu
	3# TSZR
	720,582.43
	0.00

	Taishan Villa
	4# TSTS
	0.00
	94,236.26

	
	5# TSTS
	425,598.73
	0.00

	Wangdong Community
	6# TSWD
	548,928.53
	0.00

	Total
	2,459,732.33
	94,236.26



Heating supply is not needed from 01/04/2023 to 31/10/2023. From 01/11/2023 to 31/12/2023, 2,459,732.33 m2 of residential buildings and 94,236.26 m2 of commercial buildings can access to geothermal energy-based space heating system in winter season.

From 01/01/2024 to 31/03/2024, 2,459,732.33 m2 of residential buildings and 94,236.26 m2 of commercial buildings can access to geothermal energy-based space heating system in winter season.

For the 4th monitoring period from 01/04/2023 to 31/03/2024, 2,459,732.33 m2 of residential buildings and 94,236.26 m2 of commercial buildings can access to geothermal energy-based space heating system in winter season.

SDG 8 Impact of project situation
From 01/04/2023 to 31/12/2023, 10 jobs for local people were created (including 5 females and 5 males), the average monthly earnings of employees were 4,400 RMB/person. Equal salaries were paid for men and women in the same position.

From 01/01/2024 to 31/03/2024, 10 jobs for local people were created (including 5 females and 5 males), the average monthly earnings of employees were raised to 5,000 RMB/person. Equal salaries were paid for men and women in the same position.

For the 4th monitoring period from 01/04/2023 to 31/03/2024, 10 jobs for local people were created (including 5 females and 5 males), the average monthly earnings of employees were 4,550 RMB/person. Equal salaries were paid for men and women in the same position.

SDG 13 Impact of project situation
As per section B.6.1 of approved PDD, for this project, the GHG emission reduction achieved in project situation should be calculated based on the Geothermal Resources for Space Heating (Version 03.0), which provides specific calculation methods for baseline, project and leakage emissions as well as monitoring plan. This monitoring period is the 4th monitoring period and the baseline, project and leakage emissions for this monitoring period is calculated as follows.

Baseline emission
As per section B.6.1 of the approved PDD, baseline emissions in year y (BEy) can be calculated as follows,

                                                                             (1)

Where:
	BEy
	=
	The baseline emissions from heat displaced by the project activity during the year y (t CO2e/yr).

	EFCO2,i
	=
	The CO2 emission factor per unit of energy of the fuel of technology i that would have been used in the baseline heating technology in (t CO2/TJ). Where several fuel types are used in the boiler, use the fuel type with the lowest CO2 emission factor.

	ηBL,i
	=
	The net thermal efficiency of the heating technology i using fossil fuel that would have been used in the absence of the project activity.

	HSBLi,y
	=
	The net output of heat generated by the baseline heat supply system using the technology i measured at the end point of the heat facility, during the year y (TJ/yr).



Baseline scenario of the project is establishment of new isolated district heating networks using isolated coal-fired boilers in boiler houses. EFCO2,i=87.3 tCO2/TJ (the lower limit of the uncertainty at a 95% confidence interval as provided in table 1.4 of Chapter 1 of Vol.2 (Energy) of 2006 IPCC Guidelines on National GHG Inventories for coking coal) and ηBL,j=85%.

HSBLi,y can be calculated as follows,
HSBLi,y=wi(HSy-LossPJy+LossBLy)                                                                          (2)
Where:
	HSBLi,y
	=
	The net output of heat generated by the baseline heat supply system using the technology i measured at the end point of the heat facility, during the year y (TJ/yr).

	wi
	=
	Assign weights for heat generated by technology i. As per section B.4 of this PDD, the baseline scenario of the project is 3(i) “Coal fired boilers in boiler houses, supplying several buildings through a heat distribution network”. Only one technology will be used. According to Research on Heating in Winter of Taishan village published by Xinzheng Housing and Urban-Rural Development Bureau, all the heating in winter of residential and commercial buildings were supplied by coal fired boilers. As per paragraph 51(a)(ii) option 2 Assign weights based on available historical records of AM0072 (Version 03.0), wi is equal to 1.

	HSy
	=
	Net quantity of heat supplied by the geothermal heat resource(s) in the project activity, during the year y (TJ/yr).

	LossPJy
	=
	The net distribution losses of the geothermal heat supply system during the year y (TJ/yr).

	LossBLy
	=
	The net distribution losses of the heat supply system, in the absence of project activity, during the year y (TJ/yr). Option 1: A conservative value of 0% of loss is used as historic information is not available.



The net quantity of heat supplied by the project activity is estimated based on the heat provided by the geothermal well. It considers flow rates, temperature and usage time for each geothermal well to be considered by the project activity.

HSy=min {HCAP,HSy,estimated}                                                                                     (3)

HSy,estimated can be determined by the use of the flow and temperature of water supplied by the substation heat exchanger k to the demand side space heating.

                                                                               (4)
Where:
	HSy,estimated
	=
	Estimated quantity of heat supplied by the geothermal heat resource(s) in the project activity, during the year y (TJ)

	Qj,d,y
	=
	Heat supplied at the downstream of heat exchanger (upstream of which is connected with water supply from the geothermal well j) (GW). It can be calculated as formula (5).

	Tj
	=
	Number of hours per year heat utilization at well j. 

	CF
	=
	Conversion factor from GWh to TJ (3.6).



                                                                                        (5)

Where:
	FRj,d,y
	=
	Average flow rate at the downstream of heat exchanger (upstream of which is connected with water supply from the geothermal well j) in year y (kg/hr). 

	
	=
	Heat supplied at the downstream of heat exchanger (upstream of which is connected with water supply from the geothermal well j) (°C). 



To ensure that the geothermal well is providing the required amount of energy a cap is defined. The basis to define the cap is from the space heating design, which considers the net heating area, the heating index, the type of construction that will utilize the heat and the time used throughout the year for each construction type. 

                                                                (8)

Where:
	HCAP
	=
	The net quantity of heat supplied by the geothermal heat resource(s) in the project activity, during the year y (TJ).

	Am
	=
	Net heating area for construction type m (m2).

	HIm
	=
	Heating index for construction type m (GW/m2). 45 W/m2 for residential buildings and 55 W/m2 for commercial buildings.

	Tj
	=
	Number of hours per year heat utilization at well j.

	CF
	=
	Conversion factor from GWh to TJ (3.6).

	LossPJy
	=
	Heat distribution losses from substation k to space heating areas (To be determined in Sub-step 2.b of AM0072).

	Hff
	=
	Heat supplied by fossil fuel boiler; in case a boiler is used to meet the heat demand of network. No fossil fuel boiler is utilized in the project activity and Hff is 0TJ.



Based on the results of monitored parameters (refer to section D.2 of the MR for more details), heat supplied by the geothermal based heating system (each heat exchangers) is summarized as Table 5 and Table 6.
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Table 5 The heat distribution losses and heating supplied calculated by Heating index
	Sub-areas
	Heat Substations
	Am (m2)
	Nov-2023
	Dec-2023
	Jan-2024
	Feb-2024
	Mar-2024

	
	
	Residential
	Commercial
	LossPJy (TJ)
	Am*HIm*Tj *CF*10-9
	LossPJy (TJ)
	Am*HIm*Tj *CF*10-9
	LossPJy (TJ)
	Am*HIm*Tj *CF*10-9
	LossPJy (TJ)
	Am*HIm*Tj *CF*10-9
	LossPJy (TJ)
	Am*HIm*Tj *CF*10-9

	No.4 Village Group
	1# TS4G
	255,272.8
	0.00
	2.98
	29.78
	3.08
	30.77
	3.08
	30.77
	2.88
	28.78
	3.08
	30.77

	
	2# TS4G
	509,349.84
	0.00
	5.94
	59.41
	6.14
	61.39
	6.14
	61.39
	5.74
	57.43
	6.14
	61.39

	Zhengrongfu
	3# TSZR
	720,582.43
	0.00
	8.40
	84.05
	8.69
	86.85
	8.69
	86.85
	8.12
	81.25
	8.69
	86.85

	Taishan Villa
	4# TSTS
	0.00
	94,236.26
	0.73
	7.33
	0.76
	7.57
	0.80
	8.05
	0.71
	7.08
	0.85
	8.52

	
	5# TSTS
	425,598.73
	0.00
	4.96
	49.64
	5.13
	51.30
	5.13
	51.3
	4.8
	47.99
	5.13
	51.30

	Wangdong Community
	6# TSWD
	548,928.53
	0.00
	6.40
	64.03
	6.62
	66.16
	6.62
	66.16
	6.19
	61.89
	6.62
	66.16



Table 6 The net quantity of heat supplied by the geothermal heat resource(s)

	Time Interval
	HCAP (TJ)

	01/04/2023-31/10/2023
	0

	01/11/2023-31/11/2023
	323.65

	01/12/2023-31/12/2023
	334.44

	01/01/2024-31/01/2024
	334.96

	01/02/2024-29/02/2024
	312.87

	01/03/2024-31/03/2024
	335.48

	01/04/2023-31/12/2023
	658.10

	01/01/2024-31/03/2024
	335.48

	01/04/2023-31/03/2024
	993.58




Table 7 Estimated quantity of heat supplied by the geothermal heat resource(s)
	November 2023

	Sub-areas
	Heat Substations
	Geothermal Wells
	FRj,d,y (kg/hr)
	 (°C)
	Qj,d,y (GW)
	Tj (h)
	HSy,estimated (TJ)

	No.4 Village Group
	1# TS4G
	1# Production and Re-injection Well
	850,190.00
	11.53
	0.01138 
	720
	29.50

	
	
	2# Production and Re-injection Well
	838,977.00
	11.49
	0.01120 
	720
	29.02

	
	2# TS4G
	3# Production and Re-injection Well
	846,560.86
	11.47
	0.01128 
	720
	29.23

	
	
	4# Production and Re-injection Well
	830,940.86
	11.25
	0.01086 
	720
	28.14

	Zhengrongfu
	3# TSZR
	5# Production and Re-injection Well
	852,414.86
	11.44
	0.01132 
	720
	29.35

	
	
	6# Production and Re-injection Well
	837,284.46
	11.29
	0.01097 
	720
	28.44

	Taishan Villa
	4# TSTS
	7# Production and Re-injection Well
	845,621.22
	11.69
	0.01148 
	480
	19.84

	
	5# TSTS
	8# Production and Re-injection Well
	845,210.07
	11.29
	0.01108 
	720
	28.73

	
	
	9# Production and Re-injection Well
	830,087.44
	11.45
	0.01104 
	720
	28.60

	Wangdong Community
	6# TSWD
	10# Production and Re-injection Well
	860,592.25
	10.98
	0.01098 
	720
	28.45

	
	
	11# Production and Re-injection Well
	850,072.50
	11.19
	0.01104 
	720
	28.62

	Total
	307.91

	December 2023

	Sub-areas
	Heat Substations
	Geothermal Wells
	FRj,d,y (kg/hr)
	 (°C)
	Qj,d,y (GW)
	Tj (h)
	HSy,estimated (TJ)

	No.4 Village Group
	1# TS4G
	1# Production and Re-injection Well
	850,278.91
	11.49
	0.01135 
	744
	30.39

	
	
	2# Production and Re-injection Well
	838,756.90
	11.54
	0.01124 
	744
	30.10

	
	2# TS4G
	3# Production and Re-injection Well
	845,323.23
	11.47
	0.01125 
	744
	30.14

	
	
	4# Production and Re-injection Well
	830,644.34
	11.22
	0.01082 
	744
	28.98

	Zhengrongfu
	3# TSZR
	5# Production and Re-injection Well
	850,659.95
	11.39
	0.01125 
	744
	30.12

	
	
	6# Production and Re-injection Well
	837,191.77
	11.27
	0.01096 
	744
	29.35

	Taishan Villa
	4# TSTS
	7# Production and Re-injection Well
	845,513.94
	11.72
	0.01151 
	496
	20.55

	
	5# TSTS
	8# Production and Re-injection Well
	844,846.01
	11.23
	0.01102 
	744
	29.50

	
	
	9# Production and Re-injection Well
	831,464.45
	11.49
	0.01110 
	744
	29.72

	Wangdong Community
	6# TSWD
	10# Production and Re-injection Well
	860,072.92
	11.08
	0.01107 
	744
	29.64

	
	
	11# Production and Re-injection Well
	849,788.55
	11.05
	0.01090 
	744
	29.20

	Total
	317.69

	January 2024

	Sub-areas
	Heat Substations
	Geothermal Wells
	FRj,d,y (kg/hr)
	 (°C)
	Qj,d,y (GW)
	Tj (h)
	HSy,estimated (TJ)

	No.4 Village Group
	1# TS4G
	1# Production and Re-injection Well
	851,228.98
	11.49
	0.01136 
	744
	30.42

	
	
	2# Production and Re-injection Well
	837,378.43
	11.49
	0.01117 
	744
	29.91

	
	2# TS4G
	3# Production and Re-injection Well
	846,891.95
	11.47
	0.01128 
	744
	30.20

	
	
	4# Production and Re-injection Well
	830,598.51
	11.18
	0.01079 
	744
	28.89

	Zhengrongfu
	3# TSZR
	5# Production and Re-injection Well
	850,869.66
	11.41
	0.01127 
	744
	30.18

	
	
	6# Production and Re-injection Well
	837,484.03
	11.26
	0.01095 
	744
	29.34

	Taishan Villa
	4# TSTS
	7# Production and Re-injection Well
	845,088.02
	11.77
	0.01155 
	527
	21.92

	
	5# TSTS
	8# Production and Re-injection Well
	845,914.41
	11.25
	0.01105 
	744
	29.60

	
	
	9# Production and Re-injection Well
	831,843.88
	11.55
	0.01115 
	744
	29.87

	Wangdong Community
	6# TSWD
	10# Production and Re-injection Well
	861,129.02
	11.02
	0.01102 
	744
	29.52

	
	
	11# Production and Re-injection Well
	850,228.32
	11.09
	0.01095 
	744
	29.33

	Total
	319.17

	February 2024

	Sub-areas
	Heat Substations
	Geothermal Wells
	FRj,d,y (kg/hr)
	 (°C)
	Qj,d,y (GW)
	Tj (h)
	HSy,estimated (TJ)

	No.4 Village Group
	1# TS4G
	1# Production and Re-injection Well
	849,992.04
	11.51
	0.01136 
	696
	28.46

	
	
	2# Production and Re-injection Well
	837,076.78
	11.48
	0.01116 
	696
	27.95

	
	2# TS4G
	3# Production and Re-injection Well
	845,277.13
	11.49
	0.01127 
	696
	28.24

	
	
	4# Production and Re-injection Well
	829,738.23
	11.20
	0.01079 
	696
	27.03

	Zhengrongfu
	3# TSZR
	5# Production and Re-injection Well
	852,596.93
	11.44
	0.01132 
	696
	28.37

	
	
	6# Production and Re-injection Well
	837,189.83
	11.24
	0.01092 
	696
	27.37

	Taishan Villa
	4# TSTS
	7# Production and Re-injection Well
	844,915.60
	11.72
	0.01149 
	464
	19.20

	
	5# TSTS
	8# Production and Re-injection Well
	845,624.05
	11.27
	0.01107 
	696
	27.73

	
	
	9# Production and Re-injection Well
	830,837.30
	11.51
	0.01110 
	696
	27.81

	Wangdong Community
	6# TSWD
	10# Production and Re-injection Well
	861,498.26
	10.94
	0.01095 
	696
	27.42

	
	
	11# Production and Re-injection Well
	849,111.06
	11.09
	0.01093 
	696
	27.39

	Total
	296.99

	March 2024

	Sub-areas
	Heat Substations
	Geothermal Wells
	FRj,d,y (kg/hr)
	 (°C)
	Qj,d,y (GW)
	Tj (h)
	HSy,estimated (TJ)

	No.4 Village Group
	1# TS4G
	1# Production and Re-injection Well
	849,809.41
	11.52
	0.01137 
	744
	30.44

	
	
	2# Production and Re-injection Well
	838,075.73
	11.45
	0.01115 
	744
	29.85

	
	2# TS4G
	3# Production and Re-injection Well
	845,129.40
	11.42
	0.01121 
	744
	30.02

	
	
	4# Production and Re-injection Well
	830,593.31
	11.26
	0.01086 
	744
	29.09

	Zhengrongfu
	3# TSZR
	5# Production and Re-injection Well
	851,461.47
	11.48
	0.01135 
	744
	30.41

	
	
	6# Production and Re-injection Well
	837,247.85
	11.26
	0.01095 
	744
	29.32

	Taishan Villa
	4# TSTS
	7# Production and Re-injection Well
	845,226.10
	11.73
	0.01151 
	558
	23.12

	
	5# TSTS
	8# Production and Re-injection Well
	844,313.90
	11.27
	0.01105 
	744
	29.60

	
	
	9# Production and Re-injection Well
	831,272.22
	11.48
	0.01108 
	744
	29.69

	Wangdong Community
	6# TSWD
	10# Production and Re-injection Well
	861,290.55
	11.03
	0.01103 
	744
	29.54

	
	
	11# Production and Re-injection Well
	850,259.99
	11.17
	0.01103 
	744
	29.54

	Total
	320.61



Calculation results of baseline emissions in year y (BEy) are summarized as Table 8.
Table 8 Calculation results of baseline emissions 
	Date
	HCAP (TJ)
	HSy,estimated (TJ)
	HSy(TJ)
	LossPLy (TJ)
	LossBLy (TJ)
	HSBLi,y (TJ)
	EFCO2,i (tCO2/TJ)
	ηBL,i
	BEy (tCO2e/yr)

	
	A
	B
	C=min(A,B)
	D
	E
	F=C-D+E
	G
	H
	I=F*G/H

	01/04/2023-31/10/2023
	0
	0
	0
	0
	0
	0
	87.3
	85%
	0

	01/11/2023-31/11/2023
	323.65
	307.91
	307.91
	29.42
	0
	278.48
	
	
	28,601

	01/12/2023-31/12/2023
	334.44
	317.69
	317.69
	30.40
	0
	287.29
	
	
	29,506

	01/01/2024-31/01/2024
	334.96
	319.17
	319.17
	30.45
	0
	288.72
	
	
	29,653

	01/02/2024-29/02/2024
	312.87
	296.99
	296.99
	28.44
	0
	268.55
	
	
	27,581

	01/03/2024-31/03/2024
	335.48
	320.61
	320.61
	30.50
	0
	290.11
	
	
	29,796

	01/04/2023-31/12/2023
	658.10
	625.60
	625.60
	59.83
	0
	565.77
	
	
	58,107

	01/01/2024-31/03/2024
	983.31
	936.77
	936.77
	89.39
	0
	847.38
	
	
	87,030

	01/04/2023-31/03/2024
	1,641.41
	1,562.37
	1,562.37
	149.22
	0
	1,413.15
	
	
	145,137




TEMPLATE- Monitoring Report


Project emission

As per section B.6.1 of the approved PDD, project emissions can be calculated as follows,

PEy=PEFE,y+PEEC,y+PEFF,y                                                                                       (9)

Where:
	PEy
	=
	Project emissions during the year y (t CO2e/yr).

	PEFE,y
	=
	Fugitive emissions of carbon dioxide and methane due to release of non-condensable gases from geothermal resources (t CO2e/yr).

	PEEC,y
	=
	Project emissions from additional electricity consumption as a result of the project activity (t CO2e/yr).

	PEFF,y
	=
	Project emissions from fossil fuel consumed as a direct result of the operations of the project activity (t CO2e/yr).



Step 1: Calculate project emissions from fugitive emissions resulting from non-condensable gases from the geothermal vents during the year y

The geothermal system of the project is designed to operate by extracting geothermal water at approximately 75°C, which is considered to be a low-temperature system. As per paragraph 84 of AM0072 (Version 03.0), fugitive emissions from low temperature geothermal system are considered negligible. Therefore, PEFE,y=0 tCO2.

Step 2: Calculate project emissions from additional electricity consumption as a result of the project activity 

Project emissions from electricity consumption (PEEC) used to pump geothermal water and operate the geothermal facility were calculated using Tool 05 Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation (Version 03.0). 

                                                                   (10)

Where:
	PEEC,y
	=
	Project emissions from electricity consumption in year y (t CO2/yr).

	ECPJ,j,y
	=
	Quantity of electricity consumed by the project electricity consumption source j in year y (MWh/yr).

	EFEL,j,y
	=
	Emission factor for electricity generation for source j in year y
(t CO2/MWh).

	TDLj,y
	=
	Average technical transmission and distribution losses for providing electricity to source j in year y.



Calculation results of project emissions during the year y (PEy) are summarized as Table 9.

Table 9 Calculation results of project emissions 
	Date
	ECPJ,j,y (kWh)
	ECPJ,j,y(MWh)
	EFEL,j,y (tCO2/MWh)
	(1+TDLj,y)
	PEEC,y (tCO2e/yr)

	01/04/2023-31/10/2023
	0
	0
	0.57335
	1.2
	0

	01/11/2023-31/11/2023
	2,617,675.38 
	2,617.67538 
	0.57335
	1.2
	1,802

	01/12/2023-31/12/2023
	2,630,337.79 
	2,630.33779 
	0.57335
	1.2
	1,810

	01/01/2024-31/01/2024
	2,524,748.86 
	2,524.74886 
	0.57335
	1.2
	1,738

	01/02/2024-29/02/2024
	2,522,867.90 
	2,522.86790 
	0.57335
	1.2
	1,736

	01/03/2024-31/03/2024
	2,682,454.39 
	2,682.45439 
	0.57335
	1.2
	1,846

	01/04/2023-31/12/2023
	5,248,013.17 
	5,248.01317 
	0.57335
	1.2
	3,612

	01/01/2024-31/03/2024
	7,730,071.15 
	7,730.07115 
	0.57335
	1.2
	5,320

	01/04/2023-31/03/2024
	12,978,084.32 
	12,978.08432 
	0.57335
	1.2
	8,932



Step 3: Calculate project emissions from fossil fuel consumed as a direct result of the operations of the project activity
No fossil fuel was used to operate the geothermal facilities. Therefore, PEFF,y=0 tCO2.

Therefore, for the 4th monitoring period, PEy=PEEC,y.

Leakage emission
As per section B.6.1 of approved PDD, no leakage emissions have been identified for the project activity. Therefore, for the 4th monitoring period, LEy=0 tCO2.

Therefore, the BEy, PEy, LEy in this monitoring period is listed below:
Table 10 The Calculation results of BEy, PEy and LEy
	Time Interval
	BEy
(tCO2e)
	PEy
(tCO2e)
	LEy
(tCO2e)
	Emission reductions
(tCO2e)

	01/04/2023-31/10/2023
	0
	0
	0
	0

	01/11/2023-31/11/2023
	28,601
	1,802
	0
	26,799

	01/12/2023-31/12/2023
	29,506
	1,810
	0
	27,696

	01/01/2024-31/01/2024
	29,653
	1,738
	0
	27,915

	01/02/2024-29/02/2024
	27,581
	1,736
	0
	25,845

	01/03/2024-31/03/2024
	29,796
	1,846
	0
	27,950

	01/04/2023-31/12/2023
	58,107
	3,612
	0
	54,495

	01/01/2024-31/03/2024
	87,030
	5,320
	0
	81,710

	01/04/2023-31/03/2024
	145,137
	8,932
	0
	136,205



Therefore, the project value or estimation of project situation of SDG13 in this monitoring period is: 
GHGs emission reduction achieved from 01/04/2023 to 31/12/2023 is 54,495 tCO2e.
GHGs emission reduction achieved from 01/01/2024 to 31/03/2024 is 81,710 tCO2e.
For the 4th monitoring period from 01/04/2023 to 31/03/2024, total 136,205 tCO2e emission reductions achieved.
[bookmark: _Toc40962782]E.3. Calculation of leakage 
>>
As per section B.6.1 of approved PDD, no leakage emissions have been identified for the project activity. Therefore, for the 4th monitoring period, LEy=0 tCO2.
[bookmark: _Toc40962783][bookmark: _Toc40953319][bookmark: _Toc40953601][bookmark: _Ref315873988][bookmark: _Toc40962784][bookmark: _Toc40962785]E.4. Calculation of net benefits or direct calculation for each SDG Impact
	SDG
	SDG Impact
	Baseline 
estimate
	Project 
estimate
	Net 
benefit

	13
	Emission reductions
	0 tCO2e
	136,205 tCO2e
	136,205 tCO2e

	8
	Number of males and females employed by the project
	0 jobs for local people were created
	10 jobs for local people were created (including 5 females and 5 males)
	10 jobs for local people were created (including 5 females and 5 males)

	
	Average monthly salary
	0 income.
	4,550 RMB/person, and equal salaries were paid for men and women in the same position.
	4,550 RMB/person, and equal salaries were paid for men and women in the same position.

	7
	Am
	0 m2 of the building can access to geothermal energy-based space heating system in winter season
	2,459,732.33 m2 of residential buildings and 94,236.26 m2 of commercial buildings can access to geothermal energy-based space heating system in winter season
	2,459,732.33 m2 of residential buildings and 94,236.26 m2 of commercial buildings can access to geothermal energy-based space heating system in winter season



[bookmark: _Toc40962786]E.5. Comparison of actual SDG Impacts with estimates in approved PDD 
	SDG
	Values estimated in ex ante calculation of approved PDD 
for this monitoring period
	Actual values[footnoteRef:33] achieved during this monitoring period [33:  Whenever emission reductions are capped, both the original and capped values used for calculations must be transparently reported.  Use brackets to denote original values.] 


	13
	143,987 tCO2e
	136,205 tCO2e

	8
	01/04/2023-31/03/2024, 10 jobs for local people created (including 5 females and 5 males).
Average monthly salary 3,500 RMB/person, and equal salaries paid for men and women in the same position.
	01/04/2023-31/03/2024, 10 jobs for local people created (including 5 females and 5 males).
Average monthly salary 4,550 RMB/person, and equal salaries paid for men and women in the same position.

	7
	2,480,907 m2 of residential buildings and 94,516 m2 of commercial buildings can access to geothermal energy-based space heating system in winter season.
	2,459,732.33 m2 of residential buildings and 94,236.26 m2 of commercial buildings can access to geothermal energy-based space heating system in 2023-2024 winter season.



[bookmark: _Ref4665389]E.5.1. Explanation of calculation of value estimated ex ante calculation of approved PDD for this monitoring period
>>
[bookmark: OLE_LINK16][bookmark: OLE_LINK17]For SDG 7, as per section B.6.3 of the approved PDD, the geothermal based space heating system can supply heat to 2,480.907 thousand m2 of residential buildings and 94.516 thousand m2 of commercial buildings. Actual heating areas of the 4th monitoring period were determined by the heating supply contracts signed for the 2023-2024 heating season. As per heating supply contracts signed by the project owner and the property management company of each community, 2,459,732.33 m2 of residential buildings and 94,236.26 m2 of commercial buildings can access to geothermal energy-based space heating system in 2023-2024 winter season.

[bookmark: _Hlk75263125][bookmark: OLE_LINK19]For SDG 8, as per section B.7.1 of the approved PDD, Number of males and females employed by the project and average monthly salary should be monitored. For ex ante calculation, it assumes that 10 jobs for local people will be created (including 5 females and 5 males), the average monthly earnings of employees are 3,500 RMB/person (equal salaries paid for men and women in the same position). According to the Record Keeping Book, Labor contracts and Payrolls, during the 4th monitoring period (01/04/2023-31/03/2024), 10 jobs for local people were created (including 5 females and 5 males). The average monthly salary was 4,550 RMB/person (equal salaries paid for men and women in the same position).

Emission reductions of SDG 13 can be calculated based on AM0072 Fossil Fuel Displacement by Geothermal Resources for Space Heating (Version 03.0). The estimated outcomes for SDG 13 for the 4th monitoring period (01/04/2023-31/03/2024) is 143,987 tCO2e. The parameter of net heating area for construction type m (Am), average temperature difference between inlet and outlet temperatures at the downstream of each substation heat exchanger in year y (Δtj,d,y), average flow rate at the downstream of each heat exchanger in year y (FRj,d,y), hours per hear heat utilization in well j (Tj) and electricity consumption for the year y in operating the geothermal heating system(ECPJ,j,y (ECy)) should be monitored. Emission reductions for the 4th monitoring period was 136,205 tCO2e, and the changes of the five parameters lead to the difference between the estimated value and actual value for emission reductions. 
[bookmark: _Toc40962789]E.6. Remarks on increase in achieved SDG Impacts from estimated value in approved PDD
>>
The outcomes for SDG 7 Affordable and Clean Energy and SDG 13 Climate Action were lower than the estimated value in the approved PDD. 

The estimated outcomes of SDG 7 are 2,480.907 thousand m2 of residential buildings and 94.516 thousand m2 of commercial buildings can access to geothermal energy-based space heating system. And the actual outcome was 2,459,732.33 m2 of residential buildings and 94,236.26 m2 of commercial buildings can access to geothermal energy-based space heating system in 2023-2024 heating season, which is slightly lower than the estimated value. The difference mainly due to the actual heating areas supplied by the geothermal energy-based space heating system, which is determined by the heating supply contract signed by the project owner and the property management company of each community. 

The estimated value of the outcomes of SDG 13 for the 4th monitoring period is 143,987 tCO2e, and the actual value is 136,205 tCO2e, which is 5.40% lower than the estimated value. The decline of actual SDG 13 impact is due to the change of the actual occupancy rate in year y (Am), average temperature difference between inlet and outlet temperatures at the downstream of each substation heat exchanger in year y (Δtj,d,y), average flow rate at the downstream of each heat exchanger in year y (FRj,d,y), hours per hear heat utilization in well j (Tj), and electricity consumption for the year y in operating the geothermal heating system (ECPJ,j,y (ECy)). Am determined by the occupancy rate of the project area, and heating supply is not needed for the unoccupied part of the residential and commercial area. Tj is determined by the actual heating supply period of each heating season. The parameters of Δtj,d,y, FRj,d,y and ECPJ,j,y (ECy) are mainly determined by the heating demand of the end-users, which are affected by atmospheric environment temperature, running status of the geothermal heating system, heating supply period and other aspects.

Number of males and females employed by the project and average monthly salary were determined by the Record Keeping Book, Labor contracts and Salary slips, during the 4th monitoring period (01/04/2023-31/03/2024), 10 jobs for local people were created (including 5 females and 5 males). The average monthly salary was 4,550 RMB/person (equal salaries paid for male and female in the same position), which is higher than the estimated value in the approved PDD (3,500 RMB/person). According to the Record Keeping Books, the monthly salary of the employees was 4,400 RMB/person from 01/04/2023 to 31/12/2023 and 5,000 RMB/person from 01/01/2024 to 31/03/2024. In summary, the average monthly salary of the employees for the 4th monitoring period can be calculated as (4,400 RMB/person*9+5,000 RMB/person*3)/12=4,550 RMB/person. Equal salaries were paid for men and women in the same position.
[bookmark: _Ref49860694][bookmark: _Toc40962790][bookmark: _Ref47706347]SECTION F. SAFEGUARDS REPORTING
[bookmark: _Toc40962791]>>
As per section D.1 Safeguarding principles assessment and appendix 1 of the approved PDD, all the safeguarding principles are not relevant to the project and the safeguards reporting is not needed.

[bookmark: _Toc40962792][bookmark: _Ref49860701][bookmark: _Ref47706354]SECTION G. STAKEHOLDER INPUTS AND LEGAL DISPUTES 
[bookmark: _Toc40962793]G.1. List all Inputs and Grievances which have been received via the Continuous Input and Grievance Mechanism together with their respective responses/mitigations. 
>>
The inputs/grievances methods are Continuous Input / Grievance Expression Process Book and email access. In addition, people can give inputs/grievances through visiting Zhengzhou Onar Heating Co., Ltd.
	Method
	Include all details of Chosen Method (s) so that they may be understood and, where relevant, used by readers.  

	Continuous Input / Grievance Expression Process Book (mandatory)
	A grievance book was put in Taishan village. All stakeholders are allowed to record their grievances or comments in the book. The project owner will assign specific person in each sub county to deal with related issues. When assessing the relevance and appropriateness of the stakeholders’ comments, the project owner will apply a gender lens.

	GS Contact (mandatory)
	help@goldstandard.org 

	Other
	Feedback can be made directly through visiting Zhengzhou Onar Heating Co., Ltd. (260m to the north at the intersection of Yanhuang Avenue and Daodong Road, Hezhuang Town, Xinzheng City, Henan Province, China) or through e-mail yliu_onar@163.com or telephone +86 186 0383 3642.



No inputs/grievances received during the 4th monitoring period through all the methods.

G.2. Report on any stakeholder mitigations that were agreed to be monitored. 
>>
This is the 4th monitoring period and there is no input/grievance from the previous monitoring period where follow up action need to be verified. As per section D.1 of the approved PDD, all the safeguarding principles are not relevant to the project and there are no stakeholder mitigations to be monitored.
[bookmark: _Toc40962796]G.3. Provide details of any legal contest that has arisen with the project during the monitoring period
>>
No legal contest or dispute has been arisen with the project during the 4th monitoring period.
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	Version
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	1.1
	14 October 2020
	Hyperlinked section summary to enable quick access to key sections
Improved clarity on Key Project Information
Section for POA monitoring
Forward action request section
Improved Clarity on SDG contribution/SDG Impact term used throughout
Clarity on safeguard reporting
Clarity on design changes
Leakage section added for VER/CER projects
Addition of Comparison of monitored parameters with last monitoring period
Provision of an accompanying Guide to help the user understand detailed rules and requirements
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