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KEY PROJECT INFORMATION
	GS ID (s) of Project (s)
	GS11222

	Title of the project (s) covered by monitoring report
	Ganzhou Swine Farm Animal Manure Management System GHG Mitigation Project

	Version number of the PDD/VPA-DD (s) applicable to this monitoring report
	05

	Version number of the monitoring report
	03

	Completion date of the monitoring report 
	15/12/2022

	Date of project design certification
	12/01/2022

	Date of Last Annual Report
	N/A

	Monitoring period number 
	2

	Duration of this monitoring period 
	The 2nd monitoring period from 01/08/2021 to 31/07/2022 (first and last days included)

	Project Representative 
	The official focal point and project developer: Profit Carbon Environmental Energy Technology (Shanghai) Co., Ltd.
The project owner: Jiangxi Zhengbang Breeding Co. Ltd

	Host Country
	People’s Republic of China

	Activity Requirements applied

	[bookmark: Check7]|X| Community Services Activities 
|_| Renewable Energy Activities 
|_| Land Use and Forestry Activities/Risks & Capacities 
|_| N/A 

	Methodology (ies) applied and version number
	[bookmark: OLE_LINK18]ACM0010 GHG emission reductions from manure management systems (Version 08.0)

	Product Requirements applied
	[bookmark: Check4]|X| GHG Emissions Reduction & Sequestration 
|_| Renewable Energy Label 
|_| N/A 



Table 1 - Sustainable Development Contributions Achieved
	Sustainable Development Goals Targeted
	SDG Impact 
	Amount Achieved
	Units/ Products

	SDG 13: Climate Action
	Emission reductions
	400,450
	tCO2e

	SDG 8: Decent Work and Economic Growth
	The number of males and females employed by the project
	20 jobs created including 10 females and 10 males
	Number

	
	the Average monthly salary
	5,000
	RMB/person

	SDG 7:  Affordable and Clean Energy
	Quantity of electricity generation by capturing biogas
	74,627.41
	MWh



Table 2 – Product Vintages
	SDG 7 Affordable and Clean Energy
	Amount Achieved

	Start Dates
	End Dates
	Quantity of electricity generation by capturing biogas (MWh)

	01/08/2021
	31/12/2021
	31,911.21 

	01/01/2022
	31/07/2022
	42,716.20 

	01/08/2021
	31/07/2022
	74,627.41



	SDG 8 Decent Work and Economic Growth
	Amount Achieved

	Start Dates
	End Dates
	The number of males and females employed by the project
	Average monthly earnings of employees

	01/08/2021
	31/12/2021
	20 jobs created including 10 males and 10 females
	5,000 RMB/person, the salary for men and women was the same.

	01/01/2022
	31/07/2022
	20 jobs created including 10 males and 10 females
	5,000 RMB/person, the salary for men and women was the same.

	01/08/2021
	31/07/2022
	20 jobs created including 10 males and 10 females
	5,000 RMB/person, the salary for men and women was the same.



	SDG 13 Climate Action
	Amount Achieved

	Start Dates
	End Dates
	GHG emission reductions (tCO2e)

	01/08/2021
	31/12/2021
	167,696

	01/01/2022
	31/07/2022
	232,754

	01/08/2021
	31/07/2022
	400,450



[bookmark: _Ref49860651]DESCRIPTION OF PROJECT
[bookmark: _Toc40962734]General description of project 
>>
The project introduces 10 sets of Animal Waste Management Systems (AWMSs) in 10 existing swine farms in Ganzhou City of Jiangxi Province. The purpose of the project activity is to treat the manure and wastewater from the 10 swine farms to avoid methane emissions. 

[bookmark: _Hlk86257092][bookmark: _Hlk86259381][bookmark: OLE_LINK7][bookmark: _Hlk86258620]The project activity replaces the current open anaerobic lagoons with new AWMSs, and Each subsidiary swine farm installs one AWMS. The manure and waster are collected into the anaerobic digesters and then biogas generated during the anaerobic treatment process is captured and total 8,632.3824*104m3 biogas are expected to be generated annually. And then the biogas is sent into the biogas generating system for power generation. Each generator is installed in each subsidiary swine farm, total installed capacity of the proposed project is 12.55MW. The electricity generated are all used by the AWMSs and the swine farms, and the Residual biogas (if any) is flared. After anaerobic digestion, the fermented sludge is treated in aerobic composting system, which is used as fertilizer. Wastewater from the anaerobic digesters is treated aerobically and then used for agriculture irrigation.

The scenario prior to the implementation of the proposed project activity is that the manure and wastewater from the 10 swine farms were treated in uncovered anaerobic lagoons.

The project activity reduces GHG in the atmosphere through avoiding methane emissions from anaerobic treatment of swine manure and wastewater. The annual average CO2 emission reductions are estimated 498,011 tCO2e.

The project has been put into operation in 01/10/2020. This monitoring report is for the 2nd monitoring period, which is from 01/08/2021 to 31/07/2022. Total emission reductions achieved in this monitoring period are 400,450 tCO2e.

[bookmark: _Toc40962735]Location of project 
>>
The project activity is located in Ganzhou City, Jiangxi Province, China. There are ten subsidiary farms involved in the project, including 8 Fattening farms: Guanxi, Jiading, Datang, Baishu, Zhongshi, Babaodong, Tangcun, Taojiang and 2 Breeding farms: Tianxiang, Fuwang. The location of the ten subsidiary farms is shown below:

Table1 the location of the project
	Swine farm
	East longitude
	North latitude

	Guanxi(关西猪场)
	114°58’3.07”
	24°51’43.46”

	Jiading(嘉定猪场)
	115°04’35.20”
	25°27’41.57”

	Datang(大塘猪场)
	114°55’50.6”
	25°16’10.87”

	Baishu(柏树猪场)
	115°03’27.19”
	25°26’47.21”

	Zhongshi(重石猪场)
	115°23’48.06”
	25°22’7.24”

	Babaodong(八宝洞猪场)
	114°56’26.09”
	24°54’56.01”

	Tangcun(塘村猪场)
	115°21’1.36”
	25°32’7.28”

	Taojiang(桃江猪场)
	114°40’25.17”
	24°56’2.64”

	Tianxiang(天香猪场)
	116°42’31.02”
	27°58’43.55”

	Fuwang(福旺猪场)
	116°09’24.54”
	27°51’46.99”
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Figure 1 The Geographic Location of the project

[bookmark: _Toc40962736]Reference of applied methodology 
>>
The approved methodology applied by this project is referenced as ACM0010” GHG emission reductions from manure management systems (Version 08.0)”. https://cdm.unfccc.int/filestorage/O/J/W/OJW9BM0HFSPXNGVD1KER3C2QU86I5T/EB%2075_repan14_ACM0010_ver%2008.0.pdf?t=U2x8cXlxcWZqfDAeA1TM6bDy5KQgFxHcnd1j

Tool applied: 
Tool 02: “Combined tool to identify the baseline scenario and demonstrate additionality(version07.0)”
[bookmark: _Hlk81408109]Tool 05 “Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation (Version 03.0)”
Tool 06” Project emissions from flaring (Version 03.0)”
Tool 08 “Tool to determine the mass flow of a greenhouse gas in a gaseous stream (version03.0)”
Tool 14 “Project and leakage emissions from anaerobic digesters (Version 02.0)”
Tool 24 “Common practice (Version 03.1)”

All above tools can be found through https://cdm.unfccc.int/Reference/tools/index.html 

[bookmark: _Toc40962737]Crediting period of project 
>>
Start date of crediting period: 01/10/2020.
Total length of crediting period: 01/10/2020 to 30/09/2025 (first and last days included) for the first crediting period (two renewal cycles and in total 15 years). The 2nd monitoring period is from 01/08/2021 to 31/07/2022 (first and last days included), which belong to the first crediting period.
Expected lifetime of the project: 15 years[footnoteRef:1]. [1:  As per manufacturer specifications of the power generator, the lifetime of the equipment is up to 30 years, which is greater than 15 years  (https://www.zjtcn.com/baike/kdHxlrqfdjzxxjscs).] 



[bookmark: _Toc40962738][bookmark: _Ref47706306][bookmark: _Ref49860659]IMPLEMENTATION OF PROJECT 
[bookmark: _Toc40962739][bookmark: _Ref418094175]Description of implemented project 
>>
10 sets of Animal Waste Management Systems (AWMSs) in 10 swine farms have been implemented. The raw materials such as pig manure, urine and washing water are collected, and then put into the homogenate regulating tank. After further hydrolysis and grit settling, all are put into the anaerobic tank for fermentation.

Anaerobic tanks adopt Upflow Anaerobic Sludge Bed Reactor (UASB) as its anaerobic digester technology, and the biogas generated from the anaerobic digesters enter the biogas generator set after biological desulfurization and dehydration purification. The generated electricity is used for daily operation of AWMSs and the swine farms, and the waste heat of the generator is recycled for increasing the temperature of the anaerobic reactor. At the same time, and the residual biogas is flared if there is any surplus biogas.

After anaerobic fermentation, the fermentation liquid is separated by solid and liquid, and the biogas residue is used to produce solid organic fertilizer. The biogas slurry is used as liquid organic fertilizer to irrigate the crops. The sludge produced during the aerobic treatment process is used as high-quality fertilizer. Only a small portion of organic fertilizers are supplied to the farmers living around for free. And the surplus fertilizes are sold to the end-users at below-market prices. The technical flow of the project activity is shown below:
[bookmark: _Hlk72145106][image: ]
Figure 2 Process flow of biogas project in the swine farms

The project was implemented in 10 existing swine farms and the technology implemented at each swine farm was same. while the treatment capacities of each AWMS and the size of each swine farm and corresponding design of the AWMS was different. The processing capacity and equipment of the system are designed according to the size of the farm. The construction date, commissioning date and start date of operation of each farm are summarized in Table2. The other mainly milestone for implementation of the project are summarized in Table 3. The volume for original uncovered anaerobic lagoons and the equipment parameters used of each swine farm are shown in the following Table 4:

Table 2 The construction, commissioning and start operation date of swine farms involved in this project
	Swine farm name
	Construction date
	Commissioning date
	start Operation date

	Guanxi
	05/07/2020
	20/09/2020
	01/10/2020

	Jiading
	05/07/2020
	20/09/2020
	01/10/2020

	Dating
	07/07/2020
	22/09/2020
	01/10/2020

	Baishu
	05/07/2020
	20/09/2020
	01/10/2020

	Zhongshi
	05/07/2020
	20/09/2020
	01/10/2020

	Babaodong
	08/07/2020
	23/09/2020
	01/10/2020

	Tangcun
	05/07/2020
	20/09/2020
	01/10/2020

	Taojiang
	05/07/2020
	20/09/2020
	01/10/2020

	Tianxiang
	08/07/2020
	23/09/2020
	01/10/2020

	Fuwang
	05/07/2020
	20/09/2020
	01/10/2020



	Table 3 Milestone for implementation of the project
	Milestone(s) in the Project’s Development and Implementation
	Date

	Completion of Project evaluation report
	18/10/2019

	EIA Approval by local Ecology and Environment Department
	16/04/2020

	Start date of the project, the date on signing the equipment purchase contract
	01/07/2020

	Training for the GS monitoring plan and biogas safety operation
	01/09/2020

	Formally put into operation of all the 10 sets of AWMSs
	01/10/2020

	First renewable crediting period
	01/10/2020-30/09/2025

	Submission for preliminary review
	21/06/2021

	Local stakeholder consulting physical meeting
	02/08/2021

	Employee training in 2021(including monitoring plan and biogas safety operation) 
	23/08/2021

	The 1st monitoring period
	01/10/2021-31/07/2021

	The 2nd monitoring period
	01/08/2021-31/07/2022

	Date of Project design certification
	12/01/2022



There are no deviations or delays compared to information in approved PDD. 

During this monitoring period, there was no special event occurred, such as overhaul and downtimes of biogas digesters and power generators. All the equipment operated well, and no equipment was under maintenance during this monitoring period.
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Table 4 technical parameters of main equipment and uncovered anaerobic lagoons
	Farm name
	Guanxi
	Jiading
	Dating
	Baishu
	Zhongshi
	Babaodong
	Tangcun
	Taojiang
	Tianxiang
	Fuwang

	Treatment capacities of AWMS(t/d)
	65
	300
	450
	240
	500
	630
	320
	200
	320
	320

	Baseline anaerobic lagoon 

	Size of baseline anaerobic lagoon(length*width*depth) (m3)
	60*40*3
	80*80*4.5
	100*100*4.5
	80*80*3.5
	100*100*4.5
	120*100*5
	80*80*4.5
	80*80*3.5
	80*80*4.5
	80*80*4.5

	Technical life
	No Less than 15 years

	 Biogas Generator 

	Type
	KDGH-250G
	KDGH-1200G
	KDGH-1600G
	KDGH-800G
	KDGH-1800G
	KDGH-2500G
	KDGH-1200G
	KDGH-800G
	KDGH-1200G
	KDGH-1200G

	Unit power(kw/kvA)
	250
	1,200
	1,600
	800
	1,800
	2500
	1,200
	800
	1,200
	1,200

	Frequency (Hz)
	50
	50
	50
	50
	50
	50
	50
	50
	50
	50

	Rated speed (rpm)
	1,500
	1,500
	1,500
	1,500
	1,500
	1,500
	1,500
	1,500
	1,500
	1,500

	Equipment Quantity
	1
	1
	1
	1
	1
	1
	1
	1
	1
	1

	Equipment technical life
	No Less than 30 years

	Anaerobic tank 

	Design capacity (m3)
	1,000
	2,500*2
	3,000*1+2,000*2
	1,500+2,000
	3,000*2+2,000*1
	3,000*1+2,500*3
	2,000+3,000
	2,500+1,000
	2,500+3,000
	2,500+3,000

	Anaerobic technology
	UASB
	UASB
	UASB
	UASB
	UASB
	UASB
	UASB
	UASB
	UASB
	UASB

	Stay time(day)
	15.8
	15.8
	15.8
	15.8
	15.8
	15.8
	15.8
	15.8
	15.8
	15.8

	Fermentation temperature(℃)
	38
	38
	38
	38
	38
	38
	38
	38
	38
	38

	Equipment Quantity
	1
	2
	3
	2
	3
	4
	2
	2
	2
	2

	Equipment technical life
	No Less than 30 years
	

	Turnover machine 

	Type
	FJL 6000*1050
	FJL 6000*1050
	FJL6000*1350
	FJL 6000*1050
	FJL6000*1350
	FJL6000*1350
	FJL 6000*1050
	FJL 6000*1050
	FJL 6000*1050
	FJL 6000*1050

	Supporting power(kw)
	25.74
	25.74
	41.5
	25.74
	41.5
	41.5
	25.74
	25.74
	25.74
	25.74

	Speed of work(m/h)
	50
	50
	50
	50
	50
	50
	50
	50
	50
	50

	No-load speed(m/h)
	100
	100
	100
	100
	100
	100
	100
	100
	100
	100

	Height of mixing rod(mm)
	3,400
	3,400
	4,500
	3,400
	4,500
	4,500
	3,400
	3,400
	3,400
	3,400

	Turning depth(mm)
	1,500-1,800
	1,500-1,800
	1,500-1,800
	1,500-1,800
	1,500-1,800
	1,500-1,800
	1,500-1,800
	1,500-1,800
	1,500-1,800
	1,500-1,800

	Equipment Quantity
	1
	1
	1
	1
	1
	1
	1
	1
	1
	1

	Equipment technical life
	No Less than 15 years

	Flared system 

	Type
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare
	Open flare

	Treatment capacities (m3/h)
	0-90
	0-90
	0-90
	0-90
	0-90
	0-90
	0-90
	0-90
	0-90
	0-90

	Material
	304 stainless steel
	304 stainless steel
	304 stainless steel
	304 stainless steel
	304 stainless steel
	304 stainless steel
	304 stainless steel
	304 stainless steel
	304 stainless steel
	304 stainless steel

	Height (m)
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5
	3.5

	Main wall thickness (mm)
	3
	3
	3
	3
	3
	3
	3
	3
	3
	3

	Equipment technical life
	No Less than 15 years




[bookmark: _Toc40962740]
Forward Action Requests 
>>
[bookmark: _Hlk110951645]FAR # 1: PD and the VVB shall ensure that the parameters FAer, MS%j, and B0, LT are monitored in the subsequent monitoring periods.
Reply: 
[bookmark: _Hlk122340219][bookmark: _Hlk122340397][bookmark: _Hlk110514453][bookmark: _Hlk122340800][bookmark: _Hlk122340232][bookmark: _Hlk122340438]Parameters of FAer, MS%j  are not monitored by corresponding equipment during this monitoring period. Instead, the maximum value of 100% is applied for these two parameters, which cause a lower emission reduction. It is more conservative. Therefore, design change is need for above issue.  And the design change for the project only involves the permanent changes to the registered monitoring plan as per Design Change Requirements (Version1.0). i.e. permanent changes on applying the maximum and conservative value of 100% for parameters of FAer, MS%j during the monitoring period. This can ensure that emission reduction will not be overestimated and can be reported and verified as a result of the permanent change. Therefore, the change to the monitoring plan is compliance with the applied methodology. Please refer to design change memo and revised PDD for details.
[bookmark: _Hlk121749936][bookmark: _Hlk121749984]The data source of parameter of B0, LT is 2006 IPCC and the value should be updated on the latest available public data source as per the registered PDD. As per official website of IPCC[footnoteRef:2], 2019 Refinement to the 2006 IPCC Guidelines is the latest version. 0.29 m3CH4/kg VS in Tables 10.16 chapter 10, volume 4 of is applied for the project, which is the same with the value in IPCC 2006. Therefore, B0, LT is monitored during this monitoring period.  [2:  https://www.ipcc.ch/report/2019-refinement-to-the-2006-ipcc-guidelines-for-national-greenhouse-gas-inventories/ ] 

FAR#2: The PD shall provide a confirmation from the Ministry of Ecology and Environment of China that the change of capacity from 7.3MW to 12.55MW is not considered a major design change and that a re-designed EIA is not required. The same shall be submitted to GS during or before second performance review submission.
Reply: According to the relevant requirements of the Environmental Impact Assessment Law and the Regulations on the Administration of Environmental Protection of Construction Project, the proposed project that may cause any potential environmental impact must carry out the corresponding environmental impact assessment (EIA) prior to construction. Without approval of the environmental impact assessment document, the construction shall not start. Therefore, the EIA and related approval is needed for the project.
The total number of biogas generators and the technology used by the project activity is not changed, and the installed capacity of each biogas generator was enlarged from 7.3MW to 12.55MW during the construction period. However, this change is not considered as a major change due to the purpose of the project activity is to treat the manure instead of power generation. Besides, the electricity generated by the project is only used by the swine farms and is not connected to other users or the regional power grid. The enlarged generator set, which is only larger in size, can merely result in a slight increase in site area, without generating any other adverse environmental impact. 
[bookmark: _Hlk121750081] If the change of project design will not result in significant impact on environment, there is no need to re-design the EIA. Only major change in 9 industries including Hydropower Construction Projects, Water Construction Projects (Hub Category and Diversion Projects), Thermal power construction projects, Coal construction projects, Oil and gas pipeline construction projects, Railway construction projects, Highway construction projects, Port construction projects, and Petroleum refining and petrochemical construction projects must be re-designed and re-approved as per the latest “Notice on Printing the List of Major Changes in Environmental Assessment Management of Construction Projects”[footnoteRef:3]   published on 4 June 2015 by Ministry of Ecology and Environment of the People’s Republic of China, which is the highest governing authority for environmental related matters. Biogas generation and animal manure management is not involved in the Notice. Therefore, the previous EIA approval is enough for the expansion of the installed capacity. Furthermore, by checking the public information, Notice-2015 is the latest version available for this issue.  [3:  https://www.mee.gov.cn/gkml/hbb/bgt/201506/t20150610_303328.htm] 


Post-Design Certification changes
>>
[bookmark: _Ref418094308][bookmark: _Toc40962741]Temporary deviations from the approved Monitoring & Reporting Plan, methodology or standardized baseline
>>
NA
[bookmark: _Ref418094311][bookmark: _Toc40962742]Corrections
>>
NA
[bookmark: _Ref418094316][bookmark: _Toc40962743]Changes to start date of crediting period 
>>
NA
[bookmark: _Ref418094322][bookmark: _Toc40962744]Permanent changes from the Design Certified monitoring plan, applied methodology or applied standardized baseline
>>
 Parameters of FAer, MS%j  are not monitored by corresponding equipment during this monitoring period. Instead, the maximum value of 100% is applied for these two parameters, which cause a lower emission reduction. It is more conservative. Therefore, design change is requested.  And the design change for the project only involves the permanent changes to the registered monitoring plan as per Design Change Requirements (Version1.0). i.e. permanent changes on applying the maximum and conservative value of 100% for parameters of FAer, MS%j during the monitoring period.
[bookmark: _Ref418094327][bookmark: _Toc40962745]Changes to project design of approved project
>>
NA


[bookmark: _Toc40962746][bookmark: _Ref47706319][bookmark: _Ref49860669]DESCRIPTION OF MONITORING SYSTEM APPLIED BY THE PROJECT
>>
Parameters to be monitored
According to section B.7.1 of the PDD, parameters need to be monitored is as following,
[bookmark: _Hlk88142259]Table 5 The details Monitoring Process of the monitoring parameters engaged in the project
	parameter
	Measurement methods and procedures

	For Mitigation Measure for Safeguarding Principles

	Employee Training of biogas safety operation
	Determined by the training record which was held once a year.
[bookmark: _Hlk87279290][bookmark: _Hlk87279279]For this monitoring period, biogas safety operation training was held on 23/08/2021, which can be proved by training notice and meeting attendance record.

	SDG 7

	Quantity of electricity generation by capturing biogas, EGd,y
	Measured continuously by the electricity meters installed at the outlet of generator in each farm. Total 10 electricity meters were installed. The meter reading was recorded daily by the staff.
The readout records of electricity meter have been recorded at 24:00 of every day by the staff during the monitoring period. The daily electricity generation is equal to the difference between the previous day's and the next day's readings. Monthly value is the sum of the daily electricity generation.
The electricity meter in each farm was calibratedon 19/09/2020 by an officially accredited entity. Collected data is archived in both electronic and printed copies.  Detailed information on meters including accuracy, calibration date, calibration agency and calibration standard etc can be obtained in below Table 6 and Table 7.

	SDG 8

	Number of males and females employed by the project;
Average monthly salary;

	[bookmark: _Hlk87272748]Parameters for SDG 8 were determined based on record keeping book, labor contract and Payroll. 20 jobs for local people were created and the average monthly salary were 5,000 RMB/person in this monitoring period.

	SDG 13

	[bookmark: _Hlk87272821]Number of animals of type LT produced annually for the year y, Np,LT
	[bookmark: _Hlk87272933]Each pig involved in this project has a unique electronic ear tag when was born, which is an electronic device dedicated to the identification and electronic management of animals, can track automatically. This electronic ear tag can be connected to the Data Collection System (DCS), which can store and read information. Therefore, the number of swine produced in the farm can be monitored through the auto tracking devices of electronic ear tag once pig slaughter monthly and obtained by the DCS. At the same time, the technicians in farms record manually the number of swine produced in the farms monthly and this parameter is sourced from the data logged in each swine farm. Monthly sale records for each farm can be crosschecked during this monitoring period.

	[bookmark: _Hlk87273021]Number of days animal of type LT is alive in the farm in the year y, Nda,LT
	The days of swine alive in the farm can be traced through the electronic ear tag by the technical staff in each farm and obtained by the DCS. At the same time recorded manually by the technicians in farms and sourced from the data logged in each swine farm. 

	[bookmark: _Hlk87273145]Daily stock of animals in the farm, discounting dead and discarded animals, NAA,LT
	Traced through the electronic ear tag by the technical staff in each farm and obtained by the DCS. At the same time recorded daily by the technicians in farms and sourced from the data logged in each swine farm. The technicians in farms begin to record the daily stock number of animals from the first day of monitoring period, and this record data including the new imported animal and discounting dead and discharge animals. The annual average number of animals (NAA,LT) was calculated as an average of the daily stock of breeding swine in the farms without considering dead animals and discarded animals.

	[bookmark: _Hlk87273619]Average animal weight of a defined livestock population at the project site, Wsite
	[bookmark: _Hlk87273487][bookmark: _Hlk87273633]Measured by the weight measurer on a certain day of every month. One weight measure was equipped for each farm at least, total 10 weight measures were included for this project. Wsite was conducted by sampling in the three age groups of Nursery phase, Growing phase and Mature phase in each swine farm monthly[footnoteRef:4]. The weight data is recorded by the technicians in farms and then average animal weight of a defined livestock population at the project site was calculated based on these data. The weight measures were calibrated periodically by an officially accredited entity. Detailed information on weight measures including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7. [4:  The project involves 10 swine farms, including 8 Fattening farms and 2 Breeding farms. The swine in the fattening farm are all market swine, without breeding swine. The swine in the breeding farm are all breeding swine, without market swine. Therefore, for this project, the sampling of each swine farm only needs to be considered the three-age group and there is no need to consider the type of pig.] 


	[bookmark: _Hlk87273960]Number of days treatment plant was operational in year y, ndy
	Monitored by PP and sourced from data logged in each of the manure treatment plant.

	Quantity of electricity consumed by the proposed project in year y, ECPJ,j,y
	Measured continuously by the electricity meters installed in project site in each farm. Total 10 electricity meters were installed. The meter reading was recorded daily by the staff.
The readout records of electricity meter have been recorded at 24:00 of every day by the staff during the monitoring period. The daily electricity consumption is equal to the difference between the previous day's and the next day's readings. Monthly value is the sum of the daily electricity consumption.
The staff in each swine farm recorded monthly electricity consumption at 24:00 of last day in each month and then reported the results to the grid company. The grid company checked and supplied the reading records (Electricity Transaction Notes) of the meters to the PP monthly.
The electricity meter was calibrated periodically by an officially accredited entity. Collected data is archived in both electronic and printed copies. Detailed information on meters including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below and Table 7.


	Average technical transmission and distribution losses for providing electricity to source j in year y, TDLj,y
	Sourced from tool 05 “Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation (version 03.0)”, the value is 20% in this monitoring period. This value will be renewed once the tool is updated.

	Biogas flow, Vf
	[bookmark: _Hlk87274318][bookmark: _Hlk87274489][bookmark: _Hlk87274501]Continuously measurement by the biogas flow meters (biogas flow meter 1 installed at the outlet of the anaerobic digestion, biogas flow meter 2 installed at the inlet of the power generator and biogas flow meter 3 installed in the inlet of flare and record daily. There were three flow meters in each farm and total 30 flow meters were included for this project. The monthly biogas production, biogas flow to the power generator and biogas flow to flare system is the sum of the daily output. The biogas flow meters used were calibrated on 18/09/2020 by an officially accredited entity. In addition, the biogas flow meter automatically measured the instantaneous flow rate, temperature and pressure per hour, so it is not necessary to install other equipment separately to measure the instantaneous flow rate (Vt,db), the biogas temperature (Tt) and pressure (Pt). Collected data is archived in both electronic and printed copies. Detailed information on flowmeters including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7.

	Volumetric flow of the gaseous stream in time interval t on a dry basis, Vt,db
	Measured by flowmeters, which can record hourly and saved automatically in the DCS system. As per described in monitoring parameter Vf, the flowmeters to monitor Vt,db are the same as the flowmeters that monitor Vf since the flowmeter can monitor other parameter such as Vt,db, Tt and Pt simultaneously. So, the data can be obtained from system and the monthly data was exported by the staff at the beginning of next month. Daily biogas flow is equal to the cumulative value of 24 hours, and monthly biogas flow can be accumulated on daily basis. Original collected data can be exported through the system and is archived in electronic.

	Volumetric fraction of greenhouse gas i in a time interval t on a dry basis, m³ gas i/m³ dry gas, Vi,t,db
	Continuously measurement and record hourly by online gas analyser installed at the outlet of the anaerobic digester and saved automatically in the DCS system. One gas analyser was equipped in each farm and there are 10 gas analysers totally. Therefore, the data can be obtained from system and the monthly data was exported by the staff at the beginning of next month. Daily and monthly CH4 concentration was calculated based on the 24-hour average and daily average CH4 concentration. Gas analyzers were calibrated on 10/09/2020 and 30/08/2021 by an officially accredited entity. Original collected data can be exported through the system and is archived in electronic. Detailed information on gas analyzers including accuracy, calibration date, calibration agency and calibration standard etc can be obtained in below Table 6 and Table 7.

	Temperature of the gaseous stream in time interval t, Tt;
Pressure of the gaseous stream in time interval t, Pt.
	Continuously Measurement by the biogas flow meter, which can record hourly and saved automatically in the DCS system. As per described in monitoring parameter Vf, the flowmeters to monitor Tt and Pt are the same as the flowmeters that monitor Vf since the flowmeter can monitor other parameter such as Vt,db, Tt and Pt simultaneously. So, the data can be obtained from system and the monthly data was exported by the staff at the beginning of next month.  Daily and monthly Temperature and Pressure of the biogas flow was calculated based on the 24-hour average and daily average values. Original collected data can be exported through the system and is archived in electronic. Detailed information on Flow meters including accuracy, calibration date, calibration agency and calibration standard etc. can be obtained in below Table 6 and Table 7.

	Density of greenhouse gas i in the gaseous stream in time interval t, ρi,t
	[bookmark: OLE_LINK2][bookmark: OLE_LINK3]This parameter was calculated based on the temperature and pressure of the gaseous stream in time interval t. the monitor of the temperature and pressure of the gaseous stream see the description of the above two parameters.

	[bookmark: _Hlk87274930]Fraction of volatile solids directed to aerobic treatment, FAer
	All the manure and wastewater are collected and then be taken into anaerobic digestion for treatment. After anaerobic fermentation, the fermentation liquid is separated by solid and liquid, and the biogas residue is used to produce solid organic fertilizer. The biogas slurry is used as liquid organic fertilizer to irrigate the crops.  Therefore, there is only a part of the manure that be treated through aerobic AWMS treatment.  Fraction of volatile solids directed to aerobic treatment (FAer) was determined by the VS concentration and the quantity of manure entering into aerobic treatment, and the maximum value of it is 100%. To calculate the project emissions, the maximum value of 100% will be used during this monitoring period, which is the most conservative.

	Fraction of manure handled in system j in project activity, MS%j
	Since all manure and wastewater produced by the involved swine farms was sent into AWMSs to be handled and no any manure discharged outside that is prohibited. And the treatment process of the project is an anaerobic-aerobic combined treatment technology, main including anaerobic fermentation, and aerobic composting. Therefore 100% is applied for MS%j indifferent treatment system during the monitoring period, which is the maximum value and also more conservative.

	Maximum methane producing potential of the volatile solid generated by animal type LT, B0, LT
	
The data source of parameter of B0, LT is 2006 IPCC and the value should be updated on the latest available public data source as per the registered PDD. As per official website of IPCC, 2019 Refinement to the 2006 IPCC Guidelines is the latest version. 0.29 m3CH4/kg VS in Tables 10.16 chapter 10, volume 4 of is applied for the project, which is the same with the value in IPCC 2006. Therefore, B0, LT is monitored during this monitoring period.


	Type of the barn and AWMS, Type
	The type of barn and AWMS was not changed as the design. 

	Annual average ambient temperature at project site, T
	As this project is located in Ganzhou city, Jiangxi Province, so the project site temperature is sourced from the Ganzhou Meteorological Bureau and cross check with the public website. In this monitoring period, the average project site temperature sourced from Ganzhou Meteorological Bureau is 19.6℃ and the Annual average ambient temperature from public website is 19.8℃, so the Annual average ambient temperature at project site in this monitoring period is 19.6℃ and the MCF applied in the ER calculations is 77%, which is Conservative.



Monitoring framework
[bookmark: _Hlk88143292][bookmark: _Hlk56590379][bookmark: _Hlk87279254]The project owner is responsible for the whole monitoring work. The GS Monitoring Team is established to collect and record monitoring data within the project boundary. The GS monitoring team is responsible for the normal operation of the AWMSs and the collection and record of all the monitoring data. All the data is reviewed by the project developer and VVB. Each member of the GS monitoring team is trained by the project owner at least once a year. The overall monitoring system structure of the project shows as below:



Figure 3 The Organization Structure of the Monitoring Team

Monitoring equipment and installation
Installation and configuration of monitoring equipment are shown as Figure 4. In order to ensure measurements with a low degree of uncertainty, the data monitoring equipment have been calibrated and checked by appropriately qualified third party according to appropriate national standard. 
For this monitoring period, all the monitoring equipment were calibrated according to relevant regulations.
[image: ]
[bookmark: _Hlk81557214]Figure 4 The monitoring system of the project (Same monitoring system for each farm)


Table 6 General description of monitoring equipment
	[bookmark: _Hlk80952523]Monitoring equipment
	Parameter to be monitored
	Installed location
	Type
	Series number
	Accuracy
	Date of calibration
	Calibration standard
	Validity
	Calibration agency

	Flow meter 1
	Vf
Tt
 Pt
	at the outlet of the anaerobic digestion
	LUGB
	Please refer to below Table 7
	1.5
	18/09/2020
	JJG1029-2007(Verification Regulation of Vortex-shedding Flowmeter[footnoteRef:5]) [5:  https://max.book118.com/html/2015/1030/28187671.shtm] 

	17/09/2022
	Henan Institute of Metrology

	Flow meter 2
	Vf
Tt
 Pt
	at the inlet of generator
	LUGB
	Please refer to below Table 7
	1.5
	18/09/2020
	JJG1029-2007(Verification Regulation of Vortex-shedding Flowmeter)
	17/09/2022
	Henan Institute of Metrology

	Flow meter 3
	Vf
Tt
 Pt
	in inlet of flare
	LUGB
	Please refer to below Table 7
	1.5
	18/09/2020
	JJG1029-2007(Verification Regulation of Vortex-shedding Flowmeter)
	17/09/2022
	Henan Institute of Metrology

	Electricity meter 1
	EGd,y
	at the outlet of generator
	DSSD331
	Please refer to below Table 7
	0.5S
	19/09/2020
	JJG596-2012(Electrical Meters for Measuring Alternating-current Electrical Energy[footnoteRef:6]) [6:  https://jz.docin.com/p-604653542.html] 

	18/09/2025
	State Grid Jiangxi Electric Power Research Institute

	Electricity meter 2
	ECPJ,j,y
	in the project site
	DSSD331
	Please refer to below Table 7
	0.5S
	19/09/2020
	JJG596-2012 (Electrical Meters for Measuring Alternating-current Electrical Energy)
	18/09/2025
	State Grid Jiangxi Electric Power Research Institute

	Weight measurer
	wsite
	in each pig farm
	SCS
	Please refer to below Table 7
	Ⅲlevel
	15/08/2020
09/08/2021
	JJG539-2016(Digital Indicator Scale Verification Regulations)
	14/08/2021
08/08/2022
	Jiangxi Institute of Metrology & Testing

	Gas analyser
	Vi,t,db
	at the outlet of the anaerobic digesters
	ADOS Biogas 401
	Please refer to below Table 7
	Lower than 1%
	10/09/2020
30/08/2021
	JJG693-2011(Verification Regulation of Alarmer Detectors of Combustible Gas)
	09/09/2021
29/08/2022
	Jiangxi Institute of Metrology & Testing





[bookmark: _Hlk110608511]Table 7 Series number of monitoring equipment
	Swine farm
	Series number

	
	Flowmeter 1
	Flowmeter 2
	Flowmeter 3
	Electricity meter 1
	Electricity meter 2
	Weight measurer
	Gas analyser

	Guanxi
	1908270
	1908271
	1908340
	1910194029000161
	1910194029000162
	19105195
	56260

	Jiading
	1908272
	1908273
	1908341
	1910194029000163
	1910194029000164
	19105234
	56261

	Datang
	1908274
	1908275
	1908342
	1909121944000001
	1909121944000002
	19016301
	56262

	Baishu
	1908276
	1908277
	1908343
	2001133126000100
	2001133126000101
	19016742
	56304

	Zhongshi
	1908278
	1908279
	1908344
	1908183024000072
	1908183024000073
	19023524
	56305

	Babaodong
	1908280
	1908281
	1908345
	1909121944000003
	1909121944000004
	19023246
	56306

	Tangcun
	1908282
	1908283
	1908346
	1908183024000074
	1908183024000075
	19031612
	56307

	Taojiang
	1908284
	1908285
	1908347
	2001133126000102
	2001133126000103
	19031004
	56480

	Tianxiang
	1908286
	1908287
	1908348
	1911144012000020
	1911144012000021
	19042837
	56481

	Fuwang
	1908288
	1908289
	1908349
	1912133876000122
	1912133876000123
	19042012
	56482





Corrective actions
[bookmark: _Hlk81557243]The whole GS monitoring team fellow recognized standard data evaluation methods to guarantee that the data was reliable and accurate. There was no correction of nonconformities occurred in implementation of the project or the monitoring plan during the 2nd monitoring period. For QA/QC procedure, please refer to QA/QC procedures in section D.2 of the monitoring report.

Data management
Records are the most important exercise in relation to the monitoring process. Without accurate and efficient record keeping, project emission reductions cannot be verified. 
Once missing data on a given day or a certain period of time happened, the most appropriate values such as daily average or monthly average will be used for calculation, which is to ensure that emission reductions are conservative.
All data collected as part of the monitoring plan shall be archived in electronic form and paper until at least two years after the entry period. 

[bookmark: _Hlk88143535]Emergency procedure
Employees need to be familiar with the process flow and emergency situations that may occur during project operation and operate in strict accordance with the technical specifications of each process treatment equipment and monitoring equipment. During the operation of the project, all equipment and related instruments shall be checked regularly according to the manufacturer’s recommendations. If necessary, calibration and/or proper repair have to be carried out immediately.
In case of malfunction and/or damage of any system or piece of the process, it may cause damage to the operation of the system, especially serious damage to the biogas generation system and combustion system it must be dealt with as soon as possible and reported to the responsible technician immediately.
There was no emergency happened during this monitoring period.

Avoiding of double counting
All swine farms involved in this project can be identified through its GPS coordinates, which will prevent the farms counted in the project activity to be part of any other voluntary market or emission reduction mechanism (CDM, CCER, VCS etc.) as well. Besides, the project owner has signed the Declaration of No Double Counting Statement and Declaration of not involved in other GHG scheme on 12/01/2022. The emission reductions were not double counted during the 2nd monitoring period. 
[bookmark: _Toc40962747][bookmark: _Ref47706326][bookmark: _Ref49860677]DATA AND PARAMETERS
[bookmark: _Ref418094907][bookmark: _Toc40962748]Data and parameters fixed ex ante or at renewal of crediting period
>>
SDG13
	Data/parameter
	GWPCH4

	Unit
	tCO2e/tCH4

	Description
	Global Warming Potential of CH4

	Source of data
	IPCC Fifth Assessment Report

	Value(s) applied
	28

	Choice of data or Measurement methods and procedures 
	100-year values are adopted from IPCC Fifth Assessment Report

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	All monitoring, verifications and requests for performance certification of Certified products and / or Impact Statements for the period starting 01 January 2021 shall use the AR5 GWP values (28) for calculating emission reductions and removals according to applicability of global warming potential for gold standard for the global goals projects.



	Data/parameter
	GWPN2O

	Unit
	tCO2e/tN2O

	Description
	Global Warming Potential of N2O

	Source of data
	IPCC Fifth Assessment Report

	Value(s) applied
	265

	Choice of data or Measurement methods and procedures 
	100-year values are adopted from IPCC Fifth Assessment Report

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	All monitoring, verifications and requests for performance certification of Certified products and / or Impact Statements for the period starting 01 January 2021 shall use the AR5 GWP values (265) for calculating emission reductions and removals according to applicability of global warming potential for gold standard for the global goals projects.



	Data/parameter
	DCH4

	Unit
	t/m3

	Description
	Density of CH4 

	Source of data
	ACM0010 Version 08.0

	Value(s) applied
	0.00067

	Choice of data or Measurement methods and procedures 
	0.00067 t/m3 at room temperature 20℃ and 1 atm pressure.

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	N/A



	Data/parameter
	MCFj

	Unit
	-

	Description
	Methane conversion factor for the baseline AWMSj

	Source of data
	IPCC 2006 Table 10.17, chapter 10, volume 4 

	Value(s) applied
	72.38%

	Choice of data or Measurement methods and procedures 
	MCFj value for uncovered anaerobic lagoon (baseline AWMS) is chosen.
A conservativeness factor has been applied by multiplying MCFj value (i.e., 77%) with a value of 0.94, to account for the 20 per cent uncertainty in the MCFj values as reported by IPCC 2006. 
For this project, the annual average temperature is 19.8ºC [footnoteRef:7] and the value of 77 % is applied. Therefore, MCFj value of 72.38% will be applied. [7:  https://baike.baidu.com/item/%E8%B5%A3%E5%B7%9E/142839?fr=aladdin] 


	Purpose of data
	project/baseline emission calculations

	Additional comment
	N/A



	Data/parameter
	MS%Bl,j

	Unit
	Fraction

	Description
	Fraction of manure handled in system j in the baseline. 

	Source of data
	Project proponents 

	Value(s) applied
	100%

	Choice of data or Measurement methods and procedures 
	In this project, the baseline manure management system is uncovered anaerobic lagoon only. The amount of manure handled by the anaerobic lagoon is 100%. 

	Purpose of data
	Calculation of baseline emissions

	Additional comment
	N/A



	Data/parameter
	Wdefault

	Unit
	kg

	Description
	[bookmark: OLE_LINK52]Default average animal weight of a defined population

	Source of data
	IPCC 2006 Table 10A-7 and 10A-8, chapter 10, volume 4

	Value(s) applied
	Wdefault(Market swine)=28kg
Wdefault(Breeding swine)=28kg

	Choice of data or Measurement methods and procedures 
	The values in IPCC 2006 and US-EPA are compared and the lower value from IPCC 2006 is applied.

	Purpose of data
	Calculation of Baseline emissions

	Additional comment
	N/A



	Data/parameter
	VSdefault

	Unit
	kg-dm/animal/day

	Description
	Default value for the volatile solid excretion per day on a dry-matter basis for a defined livestock population

	Source of data
	IPCC 2006 Table 10A-7 and 10A-8, chapter 10, volume 4

	Value(s) applied
	VSdefault(Market swine)=0.3
VSdefault(Breeding swine)=0.3

	Choice of data or Measurement methods and procedures 
	The values in IPCC 2006 and US-EPA are compared and the lower value from IPCC 2006 is applied.

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	N/A



	Data/parameter
	NEXIPCC default

	Unit
	kg N/ animal/year 

	Description
	Default value for the nitrogen excretion per head of a defined livestock population

	Source of data
	Calculated by the equation: 
NEXIPCC default =Nrate(T)* TAM/1000*365[footnoteRef:8] [8:  365 in this formula represents 365 days per year, which corresponds to the unit of this parameter: kg N / animal / year and Nrate(T) means the default N excretion rate with the unit of kg N/ (1000 kg animal mass)/ day. the baseline emission, project emission and leakage is calculated separately each month. Therefore, this parameter is also calculated according to the actual number of days in each month during this monitoring period.] 


	Value(s) applied
		Period
	Market Swine
	Breeding Swine

	01/08/2021-31/08/2021
	0.36
	0.21

	01/09/2021-30/09/2021
	0.35
	0.20

	01/10/2021-31/10/2021
	0.36
	0.21

	01/11/2021-30/11/2021
	0.35
	0.20

	01/12/2021-31/12/2021
	0.36
	0.21

	01/01/2022-31/01/2022
	0.36
	0.21

	01/02/2022-28/02/2022
	0.33
	0.19

	01/03/2022-31/03/2022
	0.36
	0.21

	01/04/2022-30/04/2022
	0.35
	0.20

	01/05/2022-31/05/2022
	0.36
	0.21

	01/06/2022-30/06/2022
	0.35
	0.20

	01/07/2022-31/07/2022
	0.36
	0.21




	Choice of data or Measurement methods and procedures 
	NEXIPCC default is calculated as equation 10.30 in IPCC2006, Nrate(T) and TAM are default value from IPCC 2006

	Purpose of data
	Baseline, Project and leakage emissions calculations

	Additional comment
	N/A



	Data/parameter
	Nrate(T)

	Unit
	kg N (1000 kg animal mass)-1 day-1 

	Description
	default N excretion rate

	Source of data
	IPCC 2006 Table 10.19, chapter 10, volume 4

	Value(s) applied
	Nrate(T) (Market swine) =0.42
Nrate(T)(Breeding swine) =0.24

	Choice of data or Measurement methods and procedures 
	Default value from IPCC 2006 is applied.

	Purpose of data
	NEXIPCC default calculations

	Additional comment
	N/A



	Data/parameter
	TAM

	Unit
	kg animal-1 

	Description
	typical animal mass for livestock category

	Source of data
	IPCC 2006 Table 10A-7 and 10A-8, chapter 10, volume 4

	Value(s) applied
	TAM (Market swine) =28
TAM (Breeding swine) =28

	Choice of data or Measurement methods and procedures 
	Default value from IPCC 2006 is applied.

	Purpose of data
	NEXIPCC default calculations

	Additional comment
	N/A



	Data/parameter
	Fgas MS,j,LT

	Unit
	Fraction

	Description
	Default values for nitrogen loss due to volatilisation of NH3 and NOX from manure management

	Source of data
	IPCC 2006 Table 10.22, chapter 10, volume 4

	Value(s) applied
	FgasMS,j,LT,  (anaerobic lagoon) : 40%
FgasMS,j,LT ,  (solid storage) : 45%

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Used in project/baseline emission calculations

	Additional comment
	N/A



	Data/parameter
	EFN2O,D,j

	Unit
	Kg N2O-N/kg N

	Description
	Direct N2O emission factor for the treatment system j of the manure management system

	Source of data
	IPCC 2006 Table 10.21, chapter 10, volume 4

	Value(s) applied
	EFN2O,D,j  for anaerobic lagoon and digester,  EFN2O,D,j =0.01 for aerobic system 

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Used in project/baseline emission calculations

	Additional comment
	N/A



	[bookmark: OLE_LINK54]Data/parameter
	EFN2O,ID

	Unit
	kgN2O-N/kg NH3-N and NOX-N

	Description
	Indirect N2O emission factor for the treatment system j of the manure management system

	Source of data
	IPCC 2006 Table 11.3, chapter 11, volume 4

	Value(s) applied
	0.01 

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Used in project/baseline emission calculations

	Additional comment
	N/A



	Data/parameter
	EFCH4,default

	Unit
	t CH4 leaked / t CH4 produced

	Description
	Default emission factor for the fraction of CH4 produced that leaks from the anaerobic digester (fraction)

	Source of data
	Tool 14:” Project and leakage emissions from anaerobic digesters (version02.0)

	Value(s) applied
	0.05 

	Choice of data or Measurement methods and procedures 
	UASB type digesters, floating gas holders with no external water seal 

	Purpose of data
	Calculation of project emissions

	Additional comment
	PECH4,y for ex ante estimation adopted equation(4) of  Methodological tool “Project and leakage emissions from anaerobic digesters”. In this monitor period, the amount of biogas collected at the digester was monitored by flowmeters.



	Data/parameter
	RVS,n

	Unit
	Fraction

	Description
	Fraction of volatile solid degraded in AWMS treatment method n of the N treatment steps prior to waste being treated

	Source of data
	Refer to Appendix 1 of methodology ACM0010 and project evaluation report

	Value(s) applied
	RVS,n, aerobic treatment  anaerobic digester: 2%, 45% and 35% for  leakage N2O emission released during project activity
RVS,n, one cell lagoon: 85%  for leakage N2O emission released during baseline scenario

	Choice of data or Measurement methods and procedures 
	For this project, values from Table provided in Appendix 1 of ACM0010 and Project evaluation report are compared in order to adopt the most conservative value for the given technology.

	Purpose of data
	project emission/ leakage calculation

	Additional comment
	N/A



	Data/parameter
	RN,n

	Unit
	Fraction

	Description
	Nitrogen reduction factor 

	Source of data
	Refer to Appendix 1 of methodology ACM0010

	Value(s) applied
	RN,n,  project activity (anaerobic digester) : 0.25
RN,n,  baseline (uncovered anaerobic lagoon) : 0.80

	Choice of data or Measurement methods and procedures 
	Anaerobic digester has been assumed as a covered first cell of two cell lagoon.
Uncovered anaerobic lagoon has been assumed as one cell lagoon.
The most conservative value for the given technology has been used.

	Purpose of data
	Calculation of leakage emission

	Additional comment
	N/A



	Data/parameter
	EF1, EF4, EF5

	Unit
	kg N2O-N/kg N for EF1, EF5 and [kg N2O-N/ (kg NH3-N and NOX-N) for EF4

	Description
	Emission factor for N2O emissions from N inputs; from N leaching and runoff; from atmospheric deposition of N on soils and water surfaces 

	Source of data
	IPCC 2006 Guidelines default values are be used, since country specific or region-specific data are not available. EF1 from Table 11.1, chapter 11, volume 4. EF4 and EF5 from Table 11.3, chapter 11, volume 4

	Value(s) applied
	EF1 = 0.010
EF4 =0.010
EF5 = 0.0075

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Calculation of leakage emission

	Additional comment
	N/A



	Data/parameter
	Fgasm

	Unit
	Fraction

	Description
	Fraction of N lost due to volatilization

	Source of data
	Default values from Table 11.3, chapter 11, volume 4 of IPCC 2006 guidelines 

	Value(s) applied
	0.2

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Used in project/baseline emission calculations

	Additional comment
	N/A



	Data/parameter
	Fleach

	Unit
	Fraction

	Description
	Fraction of all N added to/mineralised in managed soils in regions where leaching/runoff occurs that is lost through leaching and runoff

	Source of data
	Default values from Table 11.3, chapter 11, volume 4 of IPCC 2006 guidelines 

	Value(s) applied
	0.3

	Choice of data or Measurement methods and procedures 
	Site specific data is unavailable therefore default values are opted for.

	Purpose of data
	Calculation of leakage emission

	Additional comment
	N/A



	Data/parameter
	MCFd

	Unit
	-

	Description
	Methane conversion factor for leakage calculation

	Source of data
	Methodology ACM0010(version 08.0)

	Value(s) applied
	1

	Choice of data or Measurement methods and procedures 
	According to paragraph 51 of the methodology ACM0010” GHG emission reductions from manure management systems (version08.0)”, Methane conversion factor for leakage calculation assumed to be equal 1

	Purpose of data
	Calculation of leakage emission

	Additional comment
	N/A



	Data/parameter
	EFEF,j,y

	Unit
	tCO2/MWh

	Description
	Emission factor for electricity generation 

	Source of data
	Published by Ministry of Ecology and Environment of the People's Republic of China, which is the DNA of China

	Value(s) applied
	0.57205

	Choice of data or Measurement methods and procedures 
	According to tool” Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation”

	Purpose of data
	Calculation of project emission

	Additional comment
	N/A



	Data/parameter
	Ru

	Unit
	Pa.m3/kmol.K 

	Description
	Universal ideal gases constant 

	Source of data
	Tool 08:” Tool to determine the mass flow of a greenhouse gas in a gaseous stream (version 03.0)”

	Value(s) applied
	8,314

	Choice of data or Measurement methods and procedures 
	Value is fixed as Tool 08

	Purpose of data
	Calculation of project emission

	Additional comment
	/



	Data/parameter
	MMi

	Unit
	kg/kmol 

	Description
	Molecular mass of greenhouse gas i  

	Source of data
	Tool 08:” Tool to determine the mass flow of a greenhouse gas in a gaseous stream (version 03.0)”

	Value(s) applied
	16.04 kg/mol for methane

	Choice of data or Measurement methods and procedures 
	Value is fixed as Tool 08

	Purpose of data
	Calculation of project emission

	Additional comment
	/



	Data/parameter
	ηflare,m

	Unit
	%

	Description
	Flare efficiency in minute m

	Source of data
	Tool 06” Project emissions from flaring (Version 03.0)”

	Value(s) applied
	0%

	Choice of data or Measurement methods and procedures 
	0% is the conservative value.

	Purpose of data
	Calculation of project emission

	Additional comment
	/


[bookmark: _Ref418094911][bookmark: _Toc40962777]Data and parameters monitored
>>
SDG 13
	Data / Parameter
	Np,LT

	Unit
	Number

	Description
	Number of animals of type LT produced annually for the year y 

	Source of data
	Production record of market swine

	Value(s) of monitored parameter
		Period
	 Np,LT (head)

	01/08/2021-31/08/2021
	      79,447 

	01/09/2021-30/09/2021
	      78,935 

	01/10/2021-31/10/2021
	      78,187 

	01/11/2021-30/11/2021
	      81,037 

	01/12/2021-31/12/2021
	      84,822 

	01/01/2022-31/01/2022
	      87,149 

	01/02/2022-28/02/2022
	      90,132 

	01/03/2022-31/03/2022
	      91,710 

	01/04/2022-30/04/2022
	      90,315 

	01/05/2022-31/05/2022
	      91,388 

	01/06/2022-30/06/2022
	      85,190 

	01/07/2022-31/07/2022
	      89,969 

	01/08/2021-31/07/2022
	  1,028,281 




	Measurement methods and procedures
	To be collected for each swine population in all of the pig barns.  The number of swine produced in the swine farms had been recorded manually by the responsible staff. 
Please refer to Section C of the MR for more details.

	Monitoring frequency
	Monitored monthly.

	QA/QC procedures
	Archive electronically during project plus 5 years.

	Purpose of data
	Use for the calculation of NLT

	Additional comment
	According to the Equation 4 in PDD, the calculated NLT is 507,097 heads (1,028,281heads*180days/365days). Therefore, the 507,097 heads was applied in the calculations of emission reductions in MR. Np,LT has been crosschecked through the monthly sale records of 10 swine farms during this monitoring period and according to the monthly sale records of 10 swine farms, total 1,028,281heads of market swine is produced and sold into the market, which is consistent with the value from monthly production record of market swine.
Therefore, Np,LT is reasonable and credible. 



	Data / Parameter
	Nda,LT

	Unit
	Number

	Description
	Number of days animal of type LT is alive in the farm in the year y

	Source of data
	Production record of market swine 

	Value(s) of monitored parameter
		Period
	 Nda,LT

	01/08/2021-31/08/2021
	180days

	01/09/2021-30/09/2021
	180days

	01/10/2021-31/10/2021
	180days

	01/11/2021-30/11/2021
	180days

	01/12/2021-31/12/2021
	180days

	01/01/2022-31/01/2022
	180days

	01/02/2022-28/02/2022
	180days

	01/03/2022-31/03/2022
	180days

	01/04/2022-30/04/2022
	180days

	01/05/2022-31/05/2022
	180days

	01/06/2022-30/06/2022
	180days

	01/07/2022-31/07/2022
	180days

	01/08/2021-31/07/2022
	180days 




	Measurement methods and procedures
	The days of swine alive in the farm was recorded manually by the responsible staff. 

	Monitoring frequency
	Monitored monthly.

	QA/QC procedures
	Archive electronically during project plus 5 years.

	Purpose of data
	Use for the calculation of NLT

	Additional comment
	During this monitoring period, a certain number of market swine are slaughtered in each farm every month and the  number of days market swine alive in the farm is 180days as per monthly production record of  market swine. Also this  parameter needs to be monitored every month, therefore, the number of days of the market swine alive in the farm is 180 day.
The number of days the animal alive in the farm is crosschecked through the monthly sale records of 10 swine farms during this monitoring period. and it can be concluded that the data is consistent.
In addition, this value is in line with the number of days for swine to be slaughtered by existing large-scale breeding groups in China[footnoteRef:9]. [9:  https://zhuanlan.zhihu.com/p/38676811
http://finance.people.com.cn/n1/2017/1121/c1004-29658996.html] 




	Data / Parameter
	NAA,LT

	Unit
	Number

	Description
	Daily stock of animals in the farm, discounting dead and discarded animals

	Source of data
	Breeding swine stock record

	Value(s) of monitored parameter
		[bookmark: _Hlk76729060]Period
	 NAA,LT (head)

	01/08/2021-31/08/2021
	      128,305 

	01/09/2021-30/09/2021
	      128,299 

	01/10/2021-31/10/2021
	      128,566 

	01/11/2021-30/11/2021
	      128,716 

	01/12/2021-31/12/2021
	      128,899 

	01/01/2022-31/01/2022
	      128,260 

	01/02/2022-28/02/2022
	      128,323 

	01/03/2022-31/03/2022
	      128,393 

	01/04/2022-30/04/2022
	      128,419 

	01/05/2022-31/05/2022
	      128,852 

	01/06/2022-30/06/2022
	      128,473 

	01/07/2022-31/07/2022
	      128,555 

	01/08/2021-31/07/2022(average)
	     128,505 




	Measurement methods and procedures
	Monitored daily through the auto tracking devices of electronic ear tag and the data can be obtained from DCS. The technicians in farms record the daily stock number of animals, and this record data including the new imported animal and discounting dead and discharge animals. Archive electronically during project plus 5 years 
Please see the Section C of MR for details. 

	Monitoring frequency
	daily

	QA/QC procedures
	The system on monitoring the number of livestock population was described in the PDD.

	Purpose of data
	Use for the calculation of baseline/project emission and leakage

	Additional comment
	The system on monitoring the daily stock of breeding swine in the farm was descried in Section C of MR. 



	Data / Parameter
	Wsite

	Unit
	kg

	Description
	Average animal weight of a defined livestock population at the project site

	Source of data
	Weight record table

	Value(s) of monitored parameter
		Period
	Market swine
	Breeding swine

	01/08/2021-31/08/2021
	65.2
	79.4

	01/09/2021-30/09/2021
	64.6
	80.2

	01/10/2021-31/10/2021
	65.0
	78.1

	01/11/2021-30/11/2021
	64.7
	80.8

	01/12/2021-31/12/2021
	64.2
	78.4

	01/01/2022-31/01/2022
	64.8
	79.6

	01/02/2022-28/02/2022
	65.4
	80.2

	01/03/2022-31/03/2022
	64.6
	78.3

	01/04/2022-30/04/2022
	65.9
	79.1

	01/05/2022-31/05/2022
	64.4
	79.1

	01/06/2022-30/06/2022
	65.1
	77.5

	01/07/2022-31/07/2022
	65.2
	79.0

	01/08/2021-31/07/2022
	64.92 
	79.13 




	Measurement methods and procedures
	Measured by the weight measurers and record by the technical staff in each farm monthly
Please refer to Section D.4 of the MR for more details.

	Monitoring frequency
	monthly

	QA/QC procedures
	As describe in registered PDD, there are 10 subsidiary farms involved in the project, of which, 8 fatting farms that only including market swine and 2 breeding farms that only including breeding swine. The three age categories are classified according to the age in days of each kind of swine. For marketing swine, Nursery phase with 30-60days, Growing phase with 60-130days and Mature phase with 130-180days, while for breeding swine, Nursery phase with 30-70days, Growing phase with 70-220days and Mature phase with 220-310days. So, the sampling method is Stratified random sampling. 
The sample size and the specific sampling methods are followed as registered PDD, and described as below during this monitoring period.
1. the overall sample size based on the actual population of pigs in stock firstly is calculated. 
2. As the project involved 10 swine farms, then the sample size in each swine farm is determined based on the proportion of the number of each farm in the total number of 10 farms. 
3. Similarly, the sample size of each age group of Market swine and Breeding swine in a farm is also calculated based on the proportion of the number of each age group of Market swine and Breeding swine to the total number of swine in the farm.   
4. After the sample size in each age group of Market swine and Breeding swine of each swine farm determined, the sample is conducted in every swine farm. Since swine in different age are kept in the different pig houses, samples can be randomly selected from pig houses of this age group. 
5. After the samples are selected, the weight is measured in each farm monthly by weight measurers and recorded in the weight record table. 
6. The sample will be marked after weighting and if the sample swine is still drawn next month, then this sample swine needs to be discarded and a new sample swine is drawn. This will be done every month until the end of the monitoring period.
[bookmark: OLE_LINK9]Weight measurers were calibrated on 15/08/2020 and 09/08/2021 by an officially accredited entity in compliance with JJG539-2016 “Verification Regulation of Digital Indicating Weighting Instruments” in China.
Please refer to Section C of the MR for more details.

	Purpose of data
	Used for estimating VSLT,y

	Additional comment
	Please see section D.4 for detail about sampling.



	Data/parameter
	ndy

	Unit
	number

	Description
	Number of days treatment plant was operational in year y.

	Source of data
	[bookmark: _Hlk87290954]Daily operation report

	Value(s) of monitored parameter
	The actual number of days treatment plant in each farm that was operational are 365 days during this monitoring period 
	Period
	ndy(days)

	01/08/2021-31/08/2021
	31

	01/09/2021-30/09/2021
	30

	01/10/2021-31/10/2021
	31

	01/11/2021-30/11/2021
	30

	01/12/2021-31/12/2021
	31

	01/01/2022-31/01/2022
	31

	01/02/2022-28/02/2022
	28

	01/03/2022-31/03/2022
	31

	01/04/2022-30/04/2022
	30

	01/05/2022-31/05/2022
	31

	01/06/2022-30/06/2022
	30

	01/07/2022-31/07/2022
	31

	01/08/2021-31/07/2022
	365




	Measurement methods and procedures
	The staff in each manure treatment plant record the number of operation days daily and then record the total monthly number of operation days in end of each month through monthly operation report.

	Monitoring frequency
	Daily

	QA/QC procedures
	The accumulated meter reading of flowmeters installed in the outlet of anaerobic digesters in each farm daily can be demonstrated that the AWMSs are actually running on a daily basis. The 10 treatment plants are operational every day during this monitoring period according to the actual daily reading of flowmeters installed in the outlet of anaerobic digesters in each farm.

	Purpose of data
	Calculation of Baseline emissions

	Additional comment
	ndy is the number of days treatment plants was operational. As the anaerobic fermentation is the main process of the treatment process for the project, so the operating days of the anaerobic tank in each farm can be considered as the operating days of the treatment plant. as long as the anaerobic tank is running, biogas will be generated, so the period of biogas generation monitored by the flow meter is the operating days of the treatment plant. Therefore, each farm was operational for 365 days and there was no breakdown/ non –operational day at any of the farms according to the daily meter reading of flowmeter installed in the outlet of anaerobic digesters in each farm.



	Data/parameter
	ECPJ,j,y

	Unit
	MWh

	Description
	Quantity of electricity consumed by the project in year y

	[bookmark: _Hlk74926311]Source of data
	Daily operation report

	Value(s) of monitored parameter
		Period
	ECPJ,j,y  (MWh)

	01/08/2021-31/08/2021
	238.3080 

	01/09/2021-30/09/2021
	230.8488 

	01/10/2021-31/10/2021
	238.7772 

	01/11/2021-30/11/2021
	231.3072 

	01/12/2021-31/12/2021
	239.2488 

	01/01/2022-31/01/2022
	239.4864 

	01/02/2022-28/02/2022
	216.5220 

	01/03/2022-31/03/2022
	239.9592 

	01/04/2022-30/04/2022
	232.4460

	01/05/2022-31/05/2022
	240.4284

	01/06/2022-30/06/2022
	232.9008 

	01/07/2022-31/07/2022
	240.9012 

	01/08/2021-31/07/2022
	2,821.1340 




	Measurement methods and procedures
	Use electricity meters 2 installed in the 10 manure treatment plants. 
The readout records of electricity meter have been recorded at 24:00 of every day by the staff during the monitoring period. The daily electricity consumption is equal to the difference between the previous day's and the next day's readings. Monthly value is the sum of the daily electricity consumption.
The electricity generated by the project was used firstly for the operation of AWMSs normally, only when the biogas generators were not operation, the electricity consumption of AWMSs were sourced from the grid company.

	Monitoring frequency
	Continuous measurement and daily recording

	QA/QC procedures
	Total 10 meters were calibrated on 19/09/2020 by an officially accredited entity in compliance with JJG596-2012” Electrical Meters for Measuring Alternating-current Electrical Energy” in China.  
The electricity sourced from the grid company was cross-checked with the grid statement, and the value is consistent.
Please refer to Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	[bookmark: _Hlk74749965]Data/parameter
	TDLj,y

	Unit
	%

	Description
	Average technical transmission and distribution losses for providing electricity to source j in year y  

	Source of data
	Tool 05 (Version 03.0)” Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation”

	Value(s) of monitored parameter
	20

	Measurement methods and procedures
	If the generator set is in a shutdown state or the electricity is insufficient for the operation of AWMSs, then the electricity consumption shall be from the power grid. Scenario A: Electricity consumption from the grid is applied to the project. During this monitoring period, all the electricity consumed by the project is comes from the electricity generated by the biogas generated from the anaerobic fermentation process of the project, therefore TDLj,y is not applicable. 

	Monitoring frequency
	The value can be changed once the tool is updated.

	QA/QC procedures
	Default value of 20% is applied, which is the maximum value as per Methodology tool 05 Version 03.0 and conservative 

	Purpose of data
	Calculation of project emission

	Additional comment
	N/A



	Data / Parameter
	FAer

	Unit
	Fraction

	Description
	Fraction of volatile solids directed to aerobic treatment

	Source of data
	PDD

	Value(s) of monitored parameter
	100%

	Measurement methods and procedures
	As this parameter is not monitored by corresponding equipment. So in the monitoring period, to be conservative, the value of this parameter in the emission reduction calculation is 100%.

	Monitoring frequency
	Annually

	QA/QC procedures
	Value of FAer is applied as 100%, which is conservative.

	Purpose of data
	Calculation of project emission

	Additional comment
	FAer is used for calculation of project emission. All the manure and wastewater are collected and then be taken into anaerobic digestion for treatment. After anaerobic fermentation, the fermentation liquid is separated by solid and liquid, and the biogas residue is used to produce solid organic fertilizer. The biogas slurry is used as liquid organic fertilizer to irrigate the crops.  Therefore, there is only a part of the manure that be treated through aerobic AWMS treatment.  Fraction of volatile solids directed to aerobic treatment (FAer) was determined by the VS concentration and the quantity of manure entering into aerobic treatment. Therefore FAer  cannot exceed to 100%. So, 100% is applied for FAer during the monitoring period for calculation of project emission, which is the maximum value and also more conservative.



	[bookmark: _Hlk88209644]Data/parameter
	MS%j

	Unit
	Fraction

	Description
	Fraction of manure handled in system j in project activity

	Source of data
	PDD

	Value(s) of monitored parameter
	[bookmark: OLE_LINK33]100%. As this parameter is not monitored by corresponding equipment. so, to be conservative, the value of this parameter in the emission reduction calculation is 100%.

	Measurement methods and procedures
	All the manure flew into AWMSs to be treated, therefore, value of 100% is applied.

	Monitoring frequency
	Annually

	QA/QC procedures
	All the manure flew into AWMSs to be treated; no any manure will be discharged outside. Therefore, the value of this parameter is 100%.

	Purpose of data
	Calculation of project emissions

	Additional comment
	MS%j is used for calculation of project emission. However, MS%j is not monitored by corresponding equipment during this monitoring period. since all manure and wastewater produced by the involved swine farms was sent into AWMSs to be handled and no any manure discharged outside that is prohibited. And the treatment process of the project is an anaerobic-aerobic combined treatment technology, main including anaerobic fermentation, and aerobic composting. Therefore 100% is applied for MS%j in different treatment system during the monitoring period, which is the maximum value and also more conservative.



	[bookmark: _Hlk77239910]Data/parameter
	vf

	Unit
	m3

	Description
	Biogas flow 

	Source of data
	Daily operation record

	Value(s) of monitored parameter
		Period
	Vf-   at outlet of the anaerobic digestion (m3)
	Vf- at the inlet of generator (m3)
	Vf- in inlet of flare system (m3)

	01/08/2021-31/08/2021
	5,079,774.74
	5,003,578.11
	0.00

	01/09/2021-30/09/2021
	4,916,362.44
	4,843,108.63
	0.00

	01/10/2021-31/10/2021
	5,082,889.29
	5,007,662.52
	0.00

	01/11/2021-30/11/2021
	4,920,583.82
	4,848,251.25
	0.00

	01/12/2021-31/12/2021
	5,086,581.05
	5,012,316.95
	0.00

	01/01/2022-31/01/2022
	5,081,983.60
	5,008,294.82
	0.00

	01/02/2022-28/02/2022
	4,591,097.98
	4,524,586.72
	0.00

	01/03/2022-31/03/2022
	5,084,075.06
	5,010,427.15
	0.00

	01/04/2022-30/04/2022
	4,920,772.03
	4,849,494.63
	0.00

	01/05/2022-31/05/2022
	5,088,775.77
	5,015,069.94
	0.00

	01/06/2022-30/06/2022
	4,922,184.37
	4,850,896.37
	0.00

	01/07/2022-31/07/2022
	5,087,427.25
	5,013,751.13
	0.00

	01/08/2021-31/07/2022
	59,862,507.40
	58,987,438.22
	0.00




	Measurement methods and procedures
	Monitored continuously, record hourly and saved automatically in the Data Collection System (DCS). The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month and then recorded in daily operation record.

	Monitoring frequency
	Continuously measured by flow meter 1, flowmeter 2 and flowmeter 3. 

	QA/QC procedures
	Total 30 flow meters were calibrated on 18/09/2020 by an officially accredited entity in compliance with JJG1029-2007” Verification Regulation of Vortex-shedding Flowmeter” in China.
Please refer to   Section C of the MR for more details.

	Purpose of data
	Calculation of project emission

	Additional comment
	For this monitoring period, all the biogas produced is used for power generation, no surplus biogas for the flaring system.



	Data/parameter
	Vt,db

	Unit
	m³ dry gas/h 

	Description
	Volumetric flow of the gaseous stream in time interval t on a dry basis 

	Source of data
	Daily operation record

	Value(s) of monitored parameter
		Swine farm
	average (m³ dry gas/h) during 2nd MP

	Guanxi
	147.78

	Jiading 
	604.37

	Datang 
	924.60

	Baishu 
	445.03

	Zhongshi 
	949.16

	Babaodong 
	1272.60

	Tangcun 
	655.80

	Taojiang 
	452.65

	Tianxiang 
	710.83

	Fuwang
	670.80




	Measurement methods and procedures
	Monitored continuously, record hourly and saved automatically in the Data Collection System (DCS). The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month and then recorded in daily operation record. Daily biogas flow is equal to the cumulative value of 24 hours, and monthly biogas flow can be accumulated on daily basis. 

	Monitoring frequency
	Continuous measurement 

	QA/QC procedures
	Total 30 flow meters were calibrated on 18/09/2020 by an officially accredited entity in compliance with JJG1029-2007” Verification Regulation of Vortex-shedding Flowmeter” in China.
Please refer to   Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	Data/parameter
	Vi,t,db

	Unit
	m³ gas i/m³ dry gas 

	Description
	Volumetric fraction of greenhouse gas i in a time interval t on a dry basis 

	Source of data
	Daily operation record

	Value(s) of monitored parameter
		Period
	Average CH4 Concentration

	01/08/2021-31/08/2021
	60.43%

	01/09/2021-30/09/2021
	60.93%

	01/10/2021-31/10/2021
	59.48%

	01/11/2021-30/11/2021
	58.22%

	01/12/2021-31/12/2021
	58.48%

	01/01/2022-31/01/2022
	61.04%

	01/02/2022-28/02/2022
	58.51%

	01/03/2022-31/03/2022
	59.58%

	01/04/2022-30/04/2022
	60.67%

	01/05/2022-31/05/2022
	58.61%

	01/06/2022-30/06/2022
	59.94%

	01/07/2022-31/07/2022
	61.07%




	Measurement methods and procedures
	Measured continuously and record hourly by online gas analysers installed at the outlet of the anaerobic digesters and saved automatically in the DCS (Data Collection System).
The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month and then recorded in daily operation record. Daily and Monthly CH4 concentration was calculated based on the 24-hour average and daily average CH4 concentration.

	Monitoring frequency
	Continuous measurement 

	QA/QC procedures
	[bookmark: OLE_LINK6]All the gas analysers were calibrated on 10/09/2020 and 30/08/2021 by an officially accredited entity in compliance with JJG693-2011” Verification Regulation of Alarmer Detectors of Combustible Gas” in China. And the zero verification with an inert gas (N2) and one reading verification with a standard gas (single calibration gas) are implemented in the process of calibration, which is in accordance with JJG693-2011. All calibration gases are from Nanjing Changyuan Industrial Gas Co. Ltd, which is a qualified reference materials manufacturer issued by the General Administration of Quality Supervision, Inspection and Quarantine of the People's Republic of China on 06/09/2017.
Please refer to   Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	Data/parameter
	Tt

	Unit
	K 

	Description
	Temperature of the gaseous stream in time interval t 

	Source of data
	Daily operation record

	Value(s) of monitored parameter
		Period
	Average Temperature(K)

	01/08/2021-31/08/2021
	311.05

	01/09/2021-30/09/2021
	310.65

	01/10/2021-31/10/2021
	310.25

	01/11/2021-30/11/2021
	309.95

	01/12/2021-31/12/2021
	308.75

	01/01/2022-31/01/2022
	308.95

	01/02/2022-28/02/2022
	309.55

	01/03/2022-31/03/2022
	309.95

	01/04/2022-30/04/2022
	310.35

	01/05/2022-31/05/2022
	310.65

	01/06/2022-30/06/2022
	310.75

	01/07/2022-31/07/2022
	311.15




	Measurement methods and procedures
	Measured continuously by the biogas flow meters, since the flowmeters can monitor other parameter such as Vt,db, Tt and Pt simultaneously. And record hourly and saved automatically in the DCS system. The readout of flowmeter was indicated degrees Celsius (°C). Therefore, the temperature Tt(K) is calculated as the equation T(K)=t(°C) +273.15
The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month and then recorded in daily operation record. Daily and Monthly temperature was calculated based on the 24-hour average and daily average temperature.

	Monitoring frequency
	Continuous measurement

	QA/QC procedures
	Total 30 flow meters were calibrated on 18/09/2020 by an officially accredited entity in compliance with JJG1029-2007” Verification Regulation of Vortex-shedding Flowmeter” in China.
Please refer to   Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	Data/parameter
	Pt

	Unit
	Pa 

	Description
	Pressure of the gaseous stream in time interval t 

	Source of data
	Daily operation record

	Value(s) of monitored parameter
		period
	Average Pressure

	01/08/2021-31/08/2021
	101.325kpa

	01/09/2021-30/09/2021
	101.325kpa

	01/10/2021-31/10/2021
	101.325kpa

	01/11/2021-30/11/2021
	101.325kpa

	01/12/2021-31/12/2021
	101.325kpa

	01/01/2022-31/01/2022
	101.325kpa

	01/02/2022-28/02/2022
	101.325kpa

	01/03/2022-31/03/2022
	101.325kpa

	01/04/2022-30/04/2022
	101.325kpa

	01/05/2022-31/05/2022
	101.325kpa

	01/06/2022-30/06/2022
	101.325kpa

	01/07/2022-31/07/2022
	101.325kpa




	Measurement methods and procedures
	Measured continuously by the biogas flow meters since the flowmeters can monitor other parameter such as Vt,db, Tt and Pt simultaneously. And record hourly and saved automatically in the DCS system.
The data can be obtained from this system and the monthly data was exported by the staff at the beginning of next month and then recorded in daily operation record.
Daily and Monthly pressure was calculated based on the 24-hour average and daily average pressure.

	Monitoring frequency
	Continuous measurement

	QA/QC procedures
	Total 30 flow meters were calibrated on 18/09/2020 by an officially accredited entity in compliance with JJG1029-2007” Verification Regulation of Vortex-shedding Flowmeter” in China.
Please refer to   Section C of the MR for more details.

	Purpose of data
	Calculation of project emissions

	Additional comment
	N/A



	Data/parameter
	

	Unit
	kg gas i/m³ gas i

	Description
	Density of greenhouse gas i in the gaseous stream in time interval t 

	Source of data
	Calculated 

	Value(s) of monitored parameter
		Period
	

	01/08/2021-31/08/2021
	0.00063 t/m3

	01/09/2021-30/09/2021
	0.00063 t/m3

	01/10/2021-31/10/2021
	0.00063 t/m3

	01/11/2021-30/11/2021
	0.00063 t/m3

	01/12/2021-31/12/2021
	0.00063 t/m3

	01/01/2022-31/01/2022
	0.00063 t/m3

	01/02/2022-28/02/2022
	0.00063 t/m3

	01/03/2022-31/03/2022
	0.00063 t/m3

	01/04/2022-30/04/2022
	0.00063 t/m3

	01/05/2022-31/05/2022
	0.00063 t/m3

	01/06/2022-30/06/2022
	0.00063 t/m3

	01/07/2022-31/07/2022
	0.00063 t/m3




	Measurement methods and procedures
	Calculated based on temperature of the gaseous stream in time interval t and pressure of the gaseous stream in time interval t.

	Monitoring frequency
	Pressure and temperature are measured continuously by the biogas flow meters 

	QA/QC procedures
	Calculated value according to the pressure and temperature

	Purpose of data
	Calculation of project emissions

	Additional comment
	NA


[bookmark: _Hlk95486228]
	Data/parameter
	B0, LT

	Unit
	 m3CH4/kg -dm

	Description
	Maximum methane producing potential of the volatile solid generated by animal type LT 

	Source of data
	IPCC 2006 table 10A-7 and 10A-8, chapter 10, volume 4 

	Value(s) applied
	B0, LT (Market swine) =0.29[footnoteRef:10] [10:  The proposed project is located in Ganzhou, Jiangxi Province, China, Asia. According to Table 10A-7 and 10A-8 of IPCC 2006 Guidelines for National Greenhouse Gas Inventories volume 4, chapter10, the maximum methane producing potential(B0,LT) for Market swine and Breeding swine in Asia region is 0.29 m3 CH4/kg VS.] 

B0, LT (Breeding swine) =0.29

	Measurement methods and procedures  
	 B0, LT can be measured as per ISO 11734:1995. As this parameter is not monitored in the actual operation. so, in the monitoring period 0.29 m3CH4/kg -dm is still applied. While the actual methane producing potential of the volatile solid generated by swine manure is 479.4ml/g VS according to the public literature[footnoteRef:11],which is higher. Therefore 0.29 m3CH4/kg -dm applied in monitoring period is conservative. [11:  http://www.doc88.com/p-9902182440715.html] 


	Monitoring frequency
	Annually

	QA/QC procedures
	The value is taken from published sources. The parameter value should be updated on latest available public data source.

	Purpose of data
	Used in project emission/baseline calculations

	Additional comment
	B0, LT is not monitored during this MR since the value is taken from IPCC 2006. The parameter value will be updated on latest available public data source. Till now, “2019 refinement to the 2006 IPCC guidelines” is the latest version. However, the value from IPCC 2006 is still used for B0, LT, which is in accordance with page 10.64 of 2019 refinement to the 2006 IPCC guidelines.



	Data/parameter
	Type

	Unit
	 /

	Description
	Type of barn and AWMS  

	Source of data
	Project proponent

	Value(s) applied
	N/A

	Measurement methods and procedures  
	 The swine barn and AWMS layout and configuration are collected. Archive electronically during project plus 5 years.

	Monitoring frequency
	Once for each monitoring period

	QA/QC procedures
	After the first verification, only changes in the type of barn and AWMS will be reported.

	Purpose of data
	Confirm whether the implementation of project as design 

	Additional comment
	Swine barn and AWMS layout and configuration.



	Data/parameter
	T

	Unit
	 °C

	Description
	Annual average ambient temperature at project site

	Source of data
	Ganzhou Meteorological Bureau

	Value(s) applied
		[bookmark: OLE_LINK8]Time
	T (°C)
	Time
	T (°C)

	Aug.2021
	29.2
	Feb.2022
	11.3

	Sep.2021
	28.4
	Mar.2022
	13.7

	Oct.2021
	20.1
	Apr.2022
	19.8

	Nov.2021
	14.3
	May.2022
	23.6

	Dec.2021
	8.4
	Jun.2022
	27.8

	Jan.2022
	8.8
	Jul.2022
	30.8

	Average ambient temperature in this monitoring period-Calculated (°C)
	19.6

	Average ambient temperature in PDD (°C)[footnoteRef:12] [12:  https://baike.baidu.com/item/%E8%B5%A3%E5%B7%9E/142839?fr=aladdin] 

	19.8

	Data used in this monitoring period
	19.6




	Measurement methods and procedures  
	In this monitoring Period, the average ambient temperature at Ganzhou Meteorological Observatory nearby project site is 19.6°C, the Annual average ambient temperature at project site from public website is 19.8°C, so the applied annual average ambient temperature at project site is 19.6, and the MCF should be applied 77%.

	Monitoring frequency
	monthly

	QA/QC procedures
	Cross-Check with the Annual average ambient temperature at project site from public website monthly ( https://www.tianqi24.com/ganzhou/history.html).

	Purpose of data
	Used to select the annual MCF from IPCC 2006 Guidelines

	Additional comment
	NA 



SDG 8
	Data / Parameter
	Number of males and females employed by the project

	Unit
	Number

	Description
	Jobs created for both men and women.

	Source of data
	Record keeping book and labor contract

	Value(s) of monitored parameter
	20 jobs are created including 10 males and 10 females 

	Measurement methods and procedures
	Source of data was record keeping book and cross checked by the labor contracts.

	Monitoring frequency
	Once for each monitoring period.

	QA/QC procedures
	After the first verification, only changes in employees will be reported.
The results shall be cross checked with training records of employees.

	Purpose of data
	To demonstrate contribution to SDG 8.

	Additional comment
	N/A



	[bookmark: _Hlk68774593]Data / Parameter
	Average monthly salary

	Unit
	RMB/person

	Description
	This parameter states the payment conditions of the people employed within the project. Equal pay for work of equal value regardless of gender.

	Source of data
	Payroll

	Value(s) of monitored parameter
	5,000 RMB/person with equal salaries for men and women in the same post. 

	Measurement methods and procedures
	The average monthly salary will be determined by the Payroll and cross checked by the labor contract.

	Monitoring frequency
	Once for each monitoring period.

	QA/QC procedures
	The results shall be also cross checked with labor contracts.
After checking the average salary of Ganzhou City though official website( http://tjj.jiangxi.gov.cn/art/2022/6/2/art_38582_3982696.html ), the average annual wage of employed persons in urban private enterprise of Ganzhou City in 2021 is RMB 52,810/year i.e. 4,401 RMB/month, it can prove that the salary that employees obtained monthly is higher than the local average.

	Purpose of data
	To demonstrate contribution to SDG 8.

	Additional comment
	N/A



SDG 7
	Data / Parameter
	EGd,y

	Unit
	MWh

	Description
	Quantity of electricity generation by capturing biogas

	Source of data
	Daily operation report

	Value(s) of monitored parameter
		Period
	 EGd,y(MWh)

	01/08/2021-31/08/2021
	       6,319.520 

	01/09/2021-30/09/2021
	       6,165.761 

	01/10/2021-31/10/2021
	       6,448.869 

	01/11/2021-30/11/2021
	       6,319.696 

	01/12/2021-31/12/2021
	       6,657.360 

	01/01/2022-31/01/2022
	       6,688.077 

	01/02/2022-28/02/2022
	       5,543.978 

	01/03/2022-31/03/2022
	       6,217.939 

	01/04/2022-30/04/2022
	       5,867.404 

	01/05/2022-31/05/2022
	       5,988.997 

	01/06/2022-30/06/2022
	       6,025.298 

	01/07/2022-31/07/2022
	       6,384.510 

	01/08/2021-31/07/2022
	     74,627.41




	Measurement methods and procedures
	Use electricity meters 1 installed at the outlet of generator. 
The readout records of electricity meter have been recorded at 24:00 of every day by the staff during the monitoring period. The daily electricity generation is equal to the difference between the previous day's and the next day's readings. Monthly value is the sum of the daily electricity generation.

	Monitoring frequency
	Continuous measurement and daily recording

	QA/QC procedures
	Total 10 meters were calibrated on 19/09/2020 by an officially accredited entity in compliance with JJG596-2012” Electrical Meters for Measuring Alternating-current Electrical Energy” in China.
Please refer to Section C of the MR for more details.

	Purpose of data
	To demonstrate contribution to SDG 7.

	Additional comment
	N/A



[bookmark: _Hlk75163211]Mitigation Measure for Safeguarding Principles
	Data / Parameter
	Employee Training of biogas safety operation

	Unit
	/

	Description
	Employees was trained on the safety operation of the biogas 

	Source of data
	Training notice 

	Value(s) of monitored parameter
	Training for the biogas safety operation was held on 23/08/2021

	Measurement methods and procedures
	Training once a year
The training content includes basic biogas knowledge, Operating condition control, operating procedure, patrol inspection, Operation management and failure process. All 20 staff in manure treatment plants and 10 technicians from these 10 swine farms attended this training. 
All staff strictly follow the operation procedures in the process of operation and there are no safety accidents occurred during this monitoring period. Therefore, the training is effective.

	Monitoring frequency
	once a year

	QA/QC procedures
	Attendance list can be proved that the training is held.

	Purpose of data
	To demonstrate Mitigation Measure for Safeguarding Principles

	Additional comment
	N/A




[bookmark: _Toc341456040][bookmark: _Toc40962778]Comparison of monitored parameters with last monitoring period

[bookmark: _Hlk110930956]There are 22 parameters that need to be monitored, the monitoring results in this monitoring period and last monitoring period are as follows:
	[bookmark: _Hlk110930968]Data/Parameter
	Value obtained in1st monitoring period
	Value obtained in 2nd monitoring period

	Np,LT
		Period
	 Np,LT (head)

	01/10/2020-31/10/2020
	96,89

	01/11/2020-30/11/2020
	95,905

	01/12/2020-31/12/2020
	94,915

	01/01/2021-31/01/2021
	93,929

	01/02/2021-28/02/2021
	92,938

	01/03/2021-31/03/2021
	91,957

	01/04/2021-30/04/2021
	94,719

	01/05/2021-31/05/2021
	90,962

	01/06/2021-30/06/2021
	93,534

	01/07/2021-31/07/2021
	91,857



		Period
	 Np,LT (head)

	01/08/2021-31/08/2021
	      79,447 

	01/09/2021-30/09/2021
	      78,935 

	01/10/2021-31/10/2021
	      78,187 

	01/11/2021-30/11/2021
	      81,037 

	01/12/2021-31/12/2021
	      84,822 

	01/01/2022-31/01/2022
	      87,149 

	01/02/2022-28/02/2022
	      90,132 

	01/03/2022-31/03/2022
	      91,710 

	01/04/2022-30/04/2022
	      90,315 

	01/05/2022-31/05/2022
	      91,388 

	01/06/2022-30/06/2022
	      85,190 

	01/07/2022-31/07/2022
	      89,969 




	Nda,LT
	180days
	180days

	NAA,LT
		Period
	 NAA,LT (head)

	01/10/2020-31/10/2020
	115,528

	01/11/2020-30/11/2020
	115,171

	01/12/2020-31/12/2020
	115,078

	01/01/2021-31/01/2021
	115,605

	01/02/2021-28/02/2021
	115,372

	01/03/2021-31/03/2021
	115,826

	01/04/2021-30/04/2021
	115,541

	01/05/2021-31/05/2021
	115,102

	01/06/2021-30/06/2021
	115,593

	01/07/2021-31/07/2021
	115,574



		Period
	 NAA,LT (head)

	01/08/2021-31/08/2021
	      128,305 

	01/09/2021-30/09/2021
	      128,299 

	01/10/2021-31/10/2021
	      128,566 

	01/11/2021-30/11/2021
	      128,716 

	01/12/2021-31/12/2021
	      128,899 

	01/01/2022-31/01/2022
	      128,260 

	01/02/2022-28/02/2022
	      128,323 

	01/03/2022-31/03/2022
	      128,393 

	01/04/2022-30/04/2022
	      128,419 

	01/05/2022-31/05/2022
	      128,852 

	01/06/2022-30/06/2022
	      128,473 

	01/07/2022-31/07/2022
	      128,555 




	Wsite
		Period
	Market swine
	Breeding swine

	01/10/2020-31/10/2020
	67.9
	75.2

	01/11/2020-30/11/2020
	67.8
	75.0

	01/12/2020-31/12/2020
	67.9
	73.5

	01/01/2021-31/01/2021
	67.7
	76.0

	01/02/2021-28/02/2021
	67.6
	75.0

	01/03/2021-31/03/2021
	69.1
	75.5

	01/04/2021-30/04/2021
	67.8
	74.9

	01/05/2021-31/05/2021
	68.1
	74.4

	01/06/2021-30/06/2021
	68.1
	75.7

	01/07/2021-31/07/2021
	68.0
	73.7



		Period
	Market swine
	Breeding swine

	01/08/2021-31/08/2021
	65.2
	79.4

	01/09/2021-30/09/2021
	64.6
	80.2

	01/10/2021-31/10/2021
	65.0
	78.1

	01/11/2021-30/11/2021
	64.7
	80.8

	01/12/2021-31/12/2021
	64.2
	78.4

	01/01/2022-31/01/2022
	64.8
	79.6

	01/02/2022-28/02/2022
	65.4
	80.2

	01/03/2022-31/03/2022
	64.6
	78.3

	01/04/2022-30/04/2022
	65.9
	79.1

	01/05/2022-31/05/2022
	64.4
	79.1

	01/06/2022-30/06/2022
	65.1
	77.5

	01/07/2022-31/07/2022
	65.2
	79.0




	ndy
		Period
	ndy(days)

	01/10/2020-31/10/2020
	31

	01/11/2020-30/11/2020
	30

	01/12/2020-31/12/2020
	31

	01/01/2021-31/01/2021
	31

	01/02/2021-28/02/2021
	28

	01/03/2021-31/03/2021
	31

	01/04/2021-30/04/2021
	30

	01/05/2021-31/05/2021
	31

	01/06/2021-30/06/2021
	30

	01/07/2021-31/07/2021
	31



		Period
	ndy(days)

	01/08/2021-31/08/2021
	31

	01/09/2021-30/09/2021
	30

	01/10/2021-31/10/2021
	31

	01/11/2021-30/11/2021
	30

	01/12/2021-31/12/2021
	31

	01/01/2022-31/01/2022
	31

	01/02/2022-28/02/2022
	28

	01/03/2022-31/03/2022
	31

	01/04/2022-30/04/2022
	30

	01/05/2022-31/05/2022
	31

	01/06/2022-30/06/2022
	30

	01/07/2022-31/07/2022
	31




	ECPJ,j,y
		Period
	ECPJ,j,y (MWh)

	01/10/2020-31/10/2020
	261.67

	01/11/2020-30/11/2020
	348.89

	01/12/2020-31/12/2020
	407.04

	01/01/2021-31/01/2021
	436.11

	01/02/2021-28/02/2021
	203.52

	01/03/2021-31/03/2021
	290.74

	01/04/2021-30/04/2021
	145.37

	01/05/2021-31/05/2021
	0.00

	01/06/2021-30/06/2021
	0.00

	01/07/2021-31/07/2021
	0.00



		Period
	ECPJ,j,y  (MWh)

	01/08/2021-31/08/2021
	238.3080 

	01/09/2021-30/09/2021
	230.8488 

	01/10/2021-31/10/2021
	238.7772 

	01/11/2021-30/11/2021
	231.3072 

	01/12/2021-31/12/2021
	239.2488 

	01/01/2022-31/01/2022
	239.4864 

	01/02/2022-28/02/2022
	216.5220 

	01/03/2022-31/03/2022
	239.9592 

	01/04/2022-30/04/2022
	232.4460

	01/05/2022-31/05/2022
	240.4284

	01/06/2022-30/06/2022
	232.9008 

	01/07/2022-31/07/2022
	240.9012 




	TDLj,y
	20%
	20%

	FAer
	100%
	100%

	MS%j
	100%,46%,54%
	100%

	vf
		Period
	Vf-   at outlet of the anaerobic digestion (m3)
	Vf- at the inlet of generator (m3)
	Vf- in inlet of flare system (m3)

	1/10/2020-31/10/2020
	4,729,630.8
	4,682,334.39
	0.00

	01/11/2020-30/11/2020
	4,574,236.2
	4,528,494.05
	0.00

	01/12/2020-31/12/2020
	4,725,948.6
	4,678,689.28
	0.00

	01/01/2021-31/01/2021
	4,730,261.4
	4,682,958.53
	0.00

	01/02/2021-28/02/2021
	4,270,771.8
	4,228,064.14
	0.00

	01/03/2021-31/03/2021
	4,732,070.4
	4,684,749.54
	0.00

	01/04/2021-30/04/2021
	4,577,166.00
	4,531,394.46
	0.00

	01/05/2021-31/05/2021
	4,726,144.8
	4,678,883.49
	0.00

	01/06/2021-30/06/2021
	4,577,578.2
	4,531,802.32
	0.00

	01/07/2021-31/07/2021
	4,730,008.2
	4,682,708.33
	0.00



		Period
	Vf-   at outlet of the anaerobic digestion (m3)
	Vf- at the inlet of generator (m3)
	Vf- in inlet of flare system (m3)

	01/08/2021-31/08/2021
	5,079,774.74
	5,003,578.11
	0.00

	01/09/2021-30/09/2021
	4,916,362.44
	4,843,108.63
	0.00

	01/10/2021-31/10/2021
	5,082,889.29
	5,007,662.52
	0.00

	01/11/2021-30/11/2021
	4,920,583.82
	4,848,251.25
	0.00

	01/12/2021-31/12/2021
	5,086,581.05
	5,012,316.95
	0.00

	01/01/2022-31/01/2022
	5,081,983.60
	5,008,294.82
	0.00

	01/02/2022-28/02/2022
	4,591,097.98
	4,524,586.72
	0.00

	01/03/2022-31/03/2022
	5,084,075.06
	5,010,427.15
	0.00

	01/04/2022-30/04/2022
	4,920,772.03
	4,849,494.63
	0.00

	01/05/2022-31/05/2022
	5,088,775.77
	5,015,069.94
	0.00

	01/06/2022-30/06/2022
	4,922,184.37
	4,850,896.37
	0.00

	01/07/2022-31/07/2022
	5,087,427.25
	5,013,751.13
	0.00




	Vt,db
		[bookmark: _Hlk111015781]Swine farm
	average (m³ dry gas/h) during 1st MP

	Guanxi
	135.40

	Jiading
	569.60

	Datang
	861.55

	Baishu
	417.25

	Zhongshi
	887.46

	Babaodong
	1,192.55

	Tangcun
	607.65

	Taojiang
	414.75

	Tianxiang
	650.33

	Fuwang
	620.48



		Swine farm
	average (m³ dry gas/h) during 2nd MP

	Guanxi
	147.78

	Jiading
	604.37

	Datang
	924.60

	Baishu
	445.03

	Zhongshi
	949.16

	Babaodong
	1272.60

	Tangcun
	655.80

	Taojiang
	452.65

	Tianxiang
	710.83

	Fuwang
	670.80




	Vi,t,db
		Period
	Average CH4 Concentration

	01/10/2020-31/10/2020
	59.98%

	01/11/2020-30/11/2020
	59.99%

	01/12/2020-31/12/2020
	59.97%

	01/01/2021-31/01/2021
	59.98%

	01/02/2021-28/02/2021
	60.00%

	01/03/2021-31/03/2021
	59.97%

	01/04/2021-30/04/2021
	59.98%

	01/05/2021-31/05/2021
	59.99%

	01/06/2021-30/06/2021
	59.97%

	01/07/2021-31/07/2021
	59.98%



		Period
	Average CH4 Concentration

	01/08/2021-31/08/2021
	60.43%

	01/09/2021-30/09/2021
	60.93%

	01/10/2021-31/10/2021
	59.48%

	01/11/2021-30/11/2021
	58.22%

	01/12/2021-31/12/2021
	58.48%

	01/01/2022-31/01/2022
	61.04%

	01/02/2022-28/02/2022
	58.51%

	01/03/2022-31/03/2022
	59.58%

	01/04/2022-30/04/2022
	60.67%

	01/05/2022-31/05/2022
	58.61%

	01/06/2022-30/06/2022
	59.94%

	01/07/2022-31/07/2022
	61.07%




	Tt
		Period
	Average Temperature(K)

	01/10/2020-31/10/2020
	310.75

	01/11/2020-30/11/2020
	310.05

	01/12/2020-31/12/2020
	310.45

	01/01/2021-31/01/2021
	308.55

	01/02/2021-28/02/2021
	310.35

	01/03/2021-31/03/2021
	310.85

	01/04/2021-30/04/2021
	309.75

	01/05/2021-31/05/2021
	309.65

	01/06/2021-30/06/2021
	310.65

	01/07/2021-31/07/2021
	310.95



		Period
	Average Temperature(K)

	01/08/2021-31/08/2021
	311.05

	01/09/2021-30/09/2021
	310.65

	01/10/2021-31/10/2021
	310.25

	01/11/2021-30/11/2021
	309.95

	01/12/2021-31/12/2021
	308.75

	01/01/2022-31/01/2022
	308.95

	01/02/2022-28/02/2022
	309.55

	01/03/2022-31/03/2022
	309.95

	01/04/2022-30/04/2022
	310.35

	01/05/2022-31/05/2022
	310.65

	01/06/2022-30/06/2022
	310.75

	01/07/2022-31/07/2022
	311.15




	Pt
	101.325K
	101.325K

	
	0.00063 t/m3
	0.00063 t/m3

	B0, LT
	B0, LT (Market swine) =0.29
B0, LT (Breeding swine) =0.29
	B0, LT (Market swine) =0.29
B0, LT (Breeding swine) =0.29

	Type
	N/A. T The type of barn and AWMS was not changed as the design during 1st MP.
	N/A. The type of barn and AWMS was not changed as the design during 2nd MP.

	T
		Time
	T (°C)
	Time
	T (°C)

	Oct-2020
	21.0
	Mar-2021
	18.5

	Nov-2020
	18.0
	Apr-2021
	20.0

	Dec-2020
	10.0
	May-2021
	25.5

	Jan-2021
	9.5
	Jun-2021
	29.0

	Feb-2021
	16.0
	Jul-2021
	31.5



		Time
	T (°C)
	Time
	T (°C)

	Aug.2021
	29.2
	Feb.2022
	11.3

	Sep.2021
	28.4
	Mar.2022
	13.7

	Oct.2021
	20.1
	Apr.2022
	19.8

	Nov.2021
	14.3
	May.2022
	23.6

	Dec.2021
	8.4
	Jun.2022
	27.8

	Jan.2022
	8.8
	Jul.2022
	30.8




	Number of males and females employed by the project
	20 jobs created including 10 females and 10 males
	20 jobs created including 10 females and 10 males

	Average monthly salary
	5,000 RMB/person with equal salaries for men and women
	5,000 RMB/person with equal salaries for men and women

	EGd,y
		Period
	 EGd,y(MWh)

	01/10/2020-31/10/2020
	5,912.51 

	01/11/2020-30/11/2020
	5,794.55 

	01/12/2020-31/12/2020
	6,055.62 

	01/01/2021-31/01/2021
	6,135.06 

	01/02/2021-28/02/2021
	5,644.24

	01/03/2021-31/03/2021
	6,287.61 

	01/04/2021-30/04/2021
	5,580.66

	01/05/2021-31/05/2021
	5,835.88 

	01/06/2021-30/06/2021
	5,510.66 

	01/07/2021-31/07/2021
	5,620.62 



		Period
	 EGd,y(MWh)

	01/08/2021-31/08/2021
	       6,319.520 

	01/09/2021-30/09/2021
	       6,165.761 

	01/10/2021-31/10/2021
	       6,448.869 

	01/11/2021-30/11/2021
	       6,319.696 

	01/12/2021-31/12/2021
	       6,657.360 

	01/01/2022-31/01/2022
	       6,688.077 

	01/02/2022-28/02/2022
	       5,543.978 

	01/03/2022-31/03/2022
	       6,217.939 

	01/04/2022-30/04/2022
	       5,867.404 

	01/05/2022-31/05/2022
	       5,988.997 

	01/06/2022-30/06/2022
	       6,025.298 

	01/07/2022-31/07/2022
	       6,384.510 




	Employee Training of biogas safety operation
	Training for the biogas safety operation was held on 01/09/2020.
	Training for the biogas safety operation was held on 23/08/2021.


Comparing to the previous monitoring period, the number of market swine and breeding swine is slightly higher, which causes the increasing of biogas and electricity generation. The maximum value of 100% for MS%j is applied in 2nd monitoring period. The values of other parameters were the same or remained basically stable compared to the first monitoring period.




Implementation of sampling plan
>>
According to the PDD, the sample size will be recalculated due to the number of swine is changed during the monitoring period. During this monitoring period, the sampling is implemented according to the stratified sampling method for the monitoring of Wsite described in Section C of MR. The detailed steps are as following:
1. the overall sample size based on the actual population of pigs in stock firstly is calculated. 
2. As the project involved 10 swine farms (including 8 fattening farms and 2 breeding farms), then the sample size in each swine farm is adjusted based on the proportion of the number of each farm in the total number of 10 farms. 
3. Similarly, the sample size of each age group of Market swine and Breeding swine in a farm is also calculated based on the proportion of the number of each age group of Market swine and Breeding swine to the total number of swine in two kinds of farms. 
4. After the sample size in each age group of Market swine and Breeding swine of each swine farm determined, the sample is conducted in every swine farm. Since swine in different age are kept in the different pig houses, samples can be randomly selected from pig houses of this age group. 
5. After the samples are selected, the weight is measured in each farm monthly by weight measurers and recorded in the weight record table. 
6. [bookmark: _Hlk95486336]The sample will be marked after weighting and if the sample swine is still drawn next month, then this sample swine needs to be discarded and a new sample swine is drawn, this will be done every month until the end of the monitoring period. 

Step 1 overall sample size calculation
According to “Standard: Sampling and surveys for CDM project activities and programmes of activities (Version 09.0)”, the desired confidence level is 95% and the desired precision is 10%. According to statistical principles and sampling survey method, 423 samples should be sufficient to satisfy the desired confidence and precision. For mean value sampling, the required sampling quantity is calculated by the following steps:


n2= n1N/(N+n1)
n3=Bn2
n4= n3/r
n= n4 (110%) 
Where:
[bookmark: OLE_LINK1]Z    the Z-statistic and the value taken is 1.96 (corresponding to 95% confidence level);
σ   the standard deviation;
d   the maximum error of estimate;
X   the mean value of samples;
V   the coefficient of variation, V= σ/X≤1 and its maximum value 1 is taken;
e   the allowed relative sampling error (“precision”) and the value taken is 10% 
N   the total number of swine population 635,602; 
B   the survey design effect and the B value taken is 1 because for stratification sampling the B value is less than or equal to 1;
r    the survey reply rate and the value taken is 100%; 
110% 10% contingency was added to produce the final sample size; 
n1, n2, n3, n4, n  the adjusted values after each step with n being the final number of samples to be taken. Actually, n4 is the required number of samples based on calculation, 10% contingency was added to n4 to produce n in this sampling.

	[bookmark: _Hlk56001304]Z
	V
	e
	N
	B
	r

	1.96
	1
	10%
	635,602
	1
	100%

	n1
	
	384

	n2
	n1N/(N+n1)
	384

	n3
	Bn2
	384

	n4
	n3/r
	384

	n
	n4 (110%)
	423



Step 2 adjust sample size based on the proportion of the number of each farm in the total number of 10 farms
[bookmark: _Hlk56001316]Stratified sampling (with samples of 423) was used for the monitoring of Wsite. However, the samples number in the ten subsidiary farms is decimals according to the proportion of the number of each farm in the total number of 10 farms. To be conservative, both the samples number of the ten subsidiary farms is adjusted to be integer value. As a result, 428 samples of swine population were selected within the project boundary using Excel to ensure conservation. 

[bookmark: _Hlk56001479]The distribution of the samples in each swine farm shows as follow:
	NO.
	Swine farm
	Sample number

	1
	Guanxi
	10

	2
	Jiading
	38

	3
	Datang
	58

	4
	Baishu
	28

	5
	Zhongshi
	59

	6
	Babaodong
	79

	7
	Tangcun
	41

	8
	Taojiang
	29

	9
	Tianxiang
	44

	10
	Fuwang
	42

	Total
	428



Step 3 Determine sample size based on the proportion of the number of each age group of Market swine and Breeding swine to the total number of swine in two kinds of farms.
According to the methodology ACM0010, each defined livestock population should be classified into a minimum of three age categories. Nursery phase, Growing phase and Mature phase in fattening farms and breeding farms was be selected through the proportion of swine population in three age categories during this monitoring period. At the same time, to be conservative, both the samples number of the three age categories is adjusted to be integer value.
In conclusion, 443 samples of swine population are fixed and the distribution of the samples for three age categories in each swine farm shows as follow:
	NO.
	Swine farm
	Sample number
	Nursery phase
	Growing phase
	Mature phase

	1
	Guanxi
	11
	3
	4
	4

	2
	Jiading
	40
	12
	14
	14

	3
	Datang
	60
	18
	22
	20

	4
	Baishu
	29
	9
	10
	10

	5
	Zhongshi
	60
	18
	21
	21

	6
	Babaodong
	81
	24
	28
	29

	7
	Tangcun
	42
	12
	15
	15

	8
	Taojiang
	31
	10
	11
	10

	9
	Tianxiang
	45
	13
	16
	16

	10
	Fuwang
	44
	13
	16
	15

	Total
	443
	132
	157
	154



Step 4 sampling and measure
After the sample size in each age group of Market swine and Breeding swine of each swine farm determined, the sample and measure are conducted in every swine farm. Since swine in different age are kept in the different pig houses, samples can be randomly selected from pig houses of this age group. After the samples are selected, the weight is measured in each farm monthly by weight measurers and recorded in the weight record table. If the same sample is taken the following month, then a new sample will be taken. This will be done every month until the end of the monitoring period. 
For this monitoring period, the sample size is determined at the beginning of the monitoring period, then samples are selected randomly from pig houses of this age group by the technicians in the swine farms and then be measured by weight measures in the middle of each month. At the same time, the measured value is recorded in the weight record table by the technicians in the swine farms.
At last, monthly average Wsite of market swine and breeding swine was calculated based on Wsite of all market swine sample and breeding swine sample. 

[bookmark: _Hlk63427732]All of the sample size will be changed at the beginning of the next monitoring period during the credit periods according to the actual population of pigs in stock, a new round of sampling will be conducted as this sampling method. 

The Monitoring Team implemented the sampling investigation strictly follow the guidance. The monitoring data will be collected throughout the entire crediting period of the project.

According to Standard: Sampling and surveys of CDM project activities and programmes of activities (Version 09.0), confidence/precision have been calculated and checked as follows:

1. The stratified estimated overall mean
The sample estimate of the overall mean is calculated with the equation below:(1)


Where:
mStrat  The stratified estimated overall mean
gi  Size of the ith district where i=a,…,k
N  Population total (635,602)
mi  Mean of the ith district where i=a,…,k

2. The standard error of the stratified estimated overall mean
The standard error of the stratified estimated overall mean is calculated as follows:(2)


Where:
s.e.(mStrat)  Standard error of the stratified estimated overall mean
gi  Size of the ith district where i=a,…,k
N  Population total (635,602)
ni  Number of sampled units the ith district where i=a,…,k
SDi2  Variance of the ith district where i=a,…,k

3. t-value
t-value is depending on:
(i) The level of confidence, and
(ii) The size of the sample.
The t-value associated with 95% confidence and the sample size of 443 is 1.9653 as derived in Microsoft Excel using the TINV function.

4. Precision
The precision associated with an estimate is:
t-value × standard error of the mean

5. Calculation results
[bookmark: _Hlk63427774]For Wsite, according to “Standard: Sampling and surveys for CDM project activities and programmes of activities (Version 09.0)”, the desired confidence level is 95% and the desired precision is 10%. According to statistical principles and sampling survey method, 443 samples should be sufficient to satisfy the desired confidence and precision.
[bookmark: _Hlk63427796]The calculation results are shown below. For more details of these calculations, please refer to the ER calculation spread sheet.
	Period
	t-value
	mStrat
	s.e.(mStrat)
	Precision
	Relative Precision

	01/08/2021-31/08/2021
	1.9653 
	68.01 
	1.1956 
	2.3497 
	3.45%

	01/09/2021-30/09/2021
	1.9653 
	67.81 
	1.2159 
	2.3897 
	3.52%

	01/10/2021-31/10/2021
	1.9653 
	67.72 
	1.1902 
	2.3392 
	3.45%

	01/11/2021-30/11/2021
	1.9653 
	68.04 
	1.2432 
	2.4433 
	3.59%

	01/12/2021-31/12/2021
	1.9653 
	67.19 
	1.2150 
	2.3879 
	3.55%

	01/01/2022-31/01/2022
	1.9653 
	67.78 
	1.2410 
	2.4389 
	3.60%

	01/02/2022-28/02/2022
	1.9653 
	68.45 
	1.2069 
	2.3721 
	3.47%

	01/03/2022-31/03/2022
	1.9653 
	67.35 
	1.2352 
	2.4276 
	3.60%

	01/04/2022-30/04/2022
	1.9653 
	68.62 
	1.2294 
	2.4161 
	3.52%

	01/05/2022-31/05/2022
	1.9653 
	67.42 
	1.1972 
	2.3530 
	3.49%

	01/06/2022-30/06/2022
	1.9653 
	67.66 
	1.2425 
	2.4419 
	3.61%

	01/07/2022-31/07/2022
	1.9653 
	68.09 
	1.2168 
	2.3914 
	3.51%



[bookmark: _Hlk63428020]In conclusion, the 443 samples are sufficient to satisfy the desired confidence and precision.




[bookmark: _Toc315189228][bookmark: _Toc317860226][bookmark: _Toc341474081][bookmark: _Toc40962779][bookmark: _Ref47706333][bookmark: _Ref49860683]CALCULATION OF SDG IMPACTS
[bookmark: _Ref315873983][bookmark: _Ref418095428][bookmark: _Toc40962780]Calculation of baseline value or estimation of baseline situation of each SDG Impact
>>
SDG 7 Impact of baseline situation
From 01/08/2021 to 31/12/2021, 0 MWh of electricity can be generated through capturing biogas without the project activity.
From 01/01/2022 to 31/07/2022, 0 MWh of electricity can be generated through capturing biogas Without the project activity.
Without the project activity, 0 MWh of electricity can be generated through capturing biogas during the 2nd monitoring period from 01/08/2021 to 31/07/2022.

SDG 8 Impact of baseline situation
From 01/08/2021 to 31/12/2021, SDG 8 baseline impact was 0 job created and 0 monthly earning got without the project activity.
From 01/01/2022 to 31/07/2022, SDG 8 baseline impact was 0 job created and 0 monthly earning got without the project activity.
Without the project activity, SDG 8 baseline impact was 0 job created and 0 monthly earning got during the 2nd monitoring period from 01/08/2021 to 31/07/2022.

SDG 13 Impact of baseline situation
As per section B.6 of the PDD, baseline emissions in year y (BEy) can be calculated as follows,
Baseline emissions are：
         (Equation 1)
where:
	BEy
	Baseline emissions in year y (t CO2/yr)

	BECH4, y
	Baseline CH4 emissions in year y (t CO2/yr)

	BEN2O, y
	Baseline N2O emissions in year y (t CO2/yr)

	BEelec/heat,y
	Baseline CO2 emissions from electricity and/or heat used in the baseline (t CO2/yr) 


i) Baseline CH4 emissions (BECH4, y)
    (Equation 2)
where:
	BECH4, y
	Baseline CH4 emissions in year y (t CO2/yr)

	GWPCH4
	Global Warming Potential (GWP) of CH4 (t CO2e/t CH4) 

	DCH4
	Density of CH4 (t/m3). 0.00067t/m3 at room temperature(20℃)and 1am pressure.

	MCFj
	Annual methane conversion factor (MCF) for the baseline AWMSj. IPCC 2006, Table 10.17, chapter 10, volume 4.

	B0,LT
	Maximum methane producing potential of the volatile solid generated by animal type LT (m3CH4/kg -dm) 

	NLT
	Annual average number of animals of type LT for the year y (number)

	VSLT,y
	Annual volatile solid excretions for livestock LT entering all AWMS on a dry matter weight basis (kg -dm/animal/yr)

	MS%Bl,j
	Fraction of manure handled in system j in the baseline. In this project, the baseline manure management system is uncovered anaerobic lagoon only. The amount of manure handled by the anaerobic lagoon is 100%. MS%Bl,j =100% 

	LT
	Type of livestock 

	j
	Type of treatment system 



Estimation of various variables and parameters for above equations:
(A) As per PDD, VSLT,y shall be determined in following way.

Scaling default IPCC values VSdefault to adjust for a site-specific average animal weight as shown in equation below:
                      (Equation 3)
where:
	VSLT,y
	Annual volatile solid excretions for livestock LT entering all AWMS on a dry matter weight basis (kg -dm/animal/yr) 

	Wsite
	Average animal weight of a defined livestock population at the project site (kg) 

	Wdefault
	Default average animal weight of a defined population (kg) 

	VSdefault
	Default value for the volatile solid excretion per day on a dry-matter basis for a defined livestock population (kg-dm/animal/day) 

	ndy
	Number of days treatment plant was operational in year y 



 
(B)Annual average number of animals of type LT (NLT) shall be determined in one of the following ways, presented in order of preference
Option 1:
          (Equation 4)
where:
	NLT
	Annual average number of animals of type LT for the year y (number) 

	Nda,LT
	Number of days animal of type LT is alive in the farm in the year y (number) 

	Np,LT
	Number of animals of type LT produced annually for the year y (number) 



Option 2:
If the project developer can monitor in a reliable and traceable way the daily stock of animals in the farm, discounting dead animals and animals discarded from the productive process from the daily stock, then the annual average number of animals (NLT) may be calculated as follows: 
     (Equation 5)
where:
	NLT
	Annual average number of animals of type LT for the year y (number) 

	NAA,LT
	Daily stock of animals of type LT in the farm, discounting dead and discarded animals (number) 



[bookmark: OLE_LINK4]There are two types of swine in this project, i.e., Market swine and Breeding swine. For Market swine, since there is no way to trace the daily stock, so the Option 1 is adopted to calculate NLT for Market swine. For Breeding swine, the PP can monitor the daily stock of breeding swine in a reliable way, discounting dead breeding swine and discarded them from the productive process from the daily stock. So, the Option 2 is adopted to calculate NLT for Breeding swine. 

(C) Maximum methane producing potential(B0,LT)
According to applied methodology ACM0010(Version 08.0), this value varies by species and diet. Default values are used, and they are taken from tables 10A-4 through 10A-9 (IPCC 2006 Guidelines for National Greenhouse Gas Inventories volume 4, chapter10).

The proposed project is located in Ganzhou city, Jiangxi Province, China, Asia. According to Table 10A-7 and 10A-8 of IPCC 2006 Guidelines for National Greenhouse Gas Inventories volume 4, chapter10, the maximum methane producing potential(B0,LT) for Market swine and Breeding swine in Asia region is 0.29 m3 CH4/kg VS.

(D) Annual methane conversion factor (MCFj) for the baseline AWMSj
(a)The MCFj values given in Table 10.17, chapter 10, volume 4, IPCC 2006 Guidelines should be used. MCFj values depend on the annual average temperature where the anaerobic manure treatment facility in the baseline existed. For this project, the annual average temperature is 19.8℃and the value of 77% is applied.
(b)A conservativeness factor should be applied by multiplying MCFj values (estimated as per above bullet) with a value of 0.94, to account for the 20% uncertainty in the MCFj values as reported by IPCC 2006.

ii)Baseline N2O emissions (BEN2O,y)
        (Equation 6)
where：
	BEN2O,y
	Annual baseline N2O emissions in (t CO2e/yr) 

	GWPN2O
	Global Warming Potential (GWP) for N2O (t CO2e/tN2O) 

	CFN2O-N,N
	Conversion factor N2O-N to N2O (44/28) 

	EN2O,D,y
	Direct N2O emission in year y (kg N2O-N/year) 

	EN2O,ID,y
	Indirect N2O emission in year y (kg N2O-N/year) 



              (Equation 7)
where：
	EN2O,D,y
	Direct N2O emission in year y (kg N2O-N/yr) 

	EFN2O,D,j
	Direct N2O emission factor for the treatment system j of the manure management system (kg N2O-N/kg N).(Estimated with site-specific, regional or national data if such data is available, otherwise use default EF3 from Table 10.21, chapter 10, volume 4, in the IPCC 2006 Guidelines for National Greenhouse Gas Inventories). The site-specific, regional or national data are not available, so this project activity adopts default EF3.

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) estimated as described in appendix 2 

	MS%Bl,j
	Fraction of manure handled in system j (fraction) 

	NLT
	Annual Average number of animals of type LT for the year y estimated as per equation (4) or (5) (number) 



                   (Equation 8)
where:
	EN2O,ID,y
	Indirect N2O emission in year y (kg N2O-N/year) 

	EFN2O,ID
	Indirect N2O emission factor for N2O emissions from atmospheric deposition of nitrogen on soils and water surfaces (kgN2O-N/kg NH3-N and NOX-N). (Estimated with site-specific, regional or national data if such data is available. Otherwise, default values for EF4 from Table 11.3, chapter 11, volume 4 of IPCC 2006 Guidelines for National Greenhouse Gas Inventories
can be used). The site-specific, regional or national data are not available, so this project activity adopts default EF4.

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) estimated as described in appendix 2 

	MS%Bl,j
	Fraction of manure handled in system j (fraction) 

	FgasMS,j,LT
	Default values for nitrogen loss due to volatilisation of NH3 and NOX from manure management (fraction) 

	NLT
	Annual Average number of animals of type LT for the year y estimated as per equation (4) or (5) (number) 



Estimation of various variables and parameters for above equations:
(A) As per PDD, the procedure for estimating NEXLT,y  in following way:
In the absence of availability of project specific information on protein intake, which should be justified in the CDM-PDD, national or regional data should be used for the nitrogen excretion NEXLT,y, if available. In the absence of such data, default values from Table 10.19 of the IPCC 2006, volume 4, chapter 10) may be used and should be corrected for the animal weight at the project site in the following way: 
                     (Equation 9)
where:
	[bookmark: OLE_LINK5]NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) 

	Wsite
	Average animal weight of a defined livestock population at the project site (kg) 

	Wdefault
	Default average animal weight of a defined population (kg) 

	NEX IPCC default
	Default value for the nitrogen excretion per head of a defined livestock population (kg N/animal/year) 



                (Equation 10)
where:
	Nrate(T)
	the default N excretion rate, kg N/ (1000 kg animal mass)/ day, Table 10.19, chapter 10, volume 4 of IPCC 2006 Guidelines

	TAM
	Typical animal mass for livestock in kg/animal




iii) Baseline CO2 emission from electricity and/or heat used in the baseline
              (Equation 11)
where:
	BEelec/heat,y
	Baseline CO2 emissions from electricity and/or heat used in the baseline (t CO2/yr) 

	BEEC,y
	Baseline emissions associated with electricity generation in year y (t CO2/yr) 

	BEHG,y
	Baseline emissions associated with heat generation in year y (t CO2/yr) 



[bookmark: _Hlk85542342][bookmark: _Hlk85542358]As described in PDD, the baseline scenario of this project is uncovered anaerobic lagoon, and no heat used in the baseline, only minor electricity is used, so the emission can be excluded for simplification. In addition, the biogas generated during the treatment process in this project will be captured for power generation and all the electricity generated from this project is used by the AWMS and 10 swine farms. The electricity generated is connected to another user or to the regional power grid. So, the baseline CO2 emission from electricity and/or heat used in the baseline is 0, which is conservative.
[bookmark: _Hlk81904243]Table 8 Basic parameter
	Period
	NLT
	NAA
	Wsite (kg)
	VSLT,y (kg-dm/ animal/year)
	ndy(day)
	NEXIPCC (kg N/animal/year)
	NEXLT,y (kg N/animal/year)

	
	Market swine
	Breeding swine
	Market swine
	Breeding swine
	Market swine
	Breeding swine
	
	Market swine
	Breeding swine
	Market swine
	Breeding swine

	01/08/2021-31/08/2021
	507,097 
	128,305 
	65.2
	79.4
	21.66
	26.36
	31
	0.36
	0.21
	0.85
	0.59

	01/09/2021-30/09/2021
	507,097 
	128,299 
	64.6
	80.2
	20.76
	25.78
	30
	0.35
	0.20
	0.81
	0.58

	01/10/2021-31/10/2021
	507,097 
	128,566 
	65.0
	78.1
	21.60
	25.93
	31
	0.36
	0.21
	0.85
	0.58

	01/11/2021-30/11/2021
	507,097 
	128,716 
	64.7
	80.8
	20.79
	25.96
	30
	0.35
	0.20
	0.81
	0.58

	01/12/2021-31/12/2021
	507,097 
	128,899 
	64.2
	78.4
	21.33
	26.03
	31
	0.36
	0.21
	0.84
	0.58

	01/01/2022-31/01/2022
	507,097 
	128,260 
	64.8
	79.6
	21.51
	26.45
	31
	0.36
	0.21
	0.84
	0.59

	01/02/2022-28/02/2022
	507,097 
	128,323 
	65.4
	80.2
	19.63
	24.06
	28
	0.33
	0.19
	0.77
	0.54

	01/03/2022-31/03/2022
	507,097 
	128,393 
	64.6
	78.3
	21.44
	26.01
	31
	0.36
	0.21
	0.84
	0.58

	01/04/2022-30/04/2022
	507,097 
	128,419 
	65.9
	79.1
	21.18
	25.41
	30
	0.35
	0.20
	0.83
	0.57

	01/05/2022-31/05/2022
	507,097 
	128,852 
	64.4
	79.1
	21.40
	26.27
	31
	0.36
	0.21
	0.84
	0.59

	01/06/2022-30/06/2022
	507,097
	128,473
	65.1
	77.5
	20.93
	24.91
	30
	0.35
	0.20
	0.82
	0.56

	01/07/2022-31/07/2022
	507,097
	128,555
	65.2
	79.0
	21.66
	26.24
	31
	0.36
	0.21
	0.85
	0.59



Table 9 The calculation result of BECH4,y
	Parameter
	Value　
	Unit

	species
	Market Swine
	Breeding Swine
	

	GWPCH4
	28
	28
	tCO2/tCH4

	DCH4
	0.00067
	0.00067
	t/m3

	MCFj
	77%
	77%
	%

	Conservative Factor
	0.94
	0.94
	/　

	MCF with cons. Factor
	0.7238
	0.7238
	/　

	B0,LT
	0.29
	0.29
	m3 CH4 /kg_dm

	NLT
	 Refer to Table 8

	Wsite
	 Refer to Table 8

	Wdefault
	28
	28
	kg

	VSdefault
	0.3
	0.3
	Kg-dm/animal/day

	VSLT,y
	Refer to Table 8

	MS%Bl,j
	100%
	100%
	%

	ndy
	Refer to Table 8

	01/08/2021-31/12/2021
	277,773
	tCO2e

	01/01/2022-31/07/2022
	385,739
	tCO2e

	BECH4,y
	663,512
	tCO2e



Table 10 The calculation result of BEN2O,y
	Parameter
	Value
	Unit

	species
	Market Swine
	Breeding Swine
	

	EFN2O,D,j
	0
	0
	kg N2O-N/kg N

	EFN2O,ID,j
	0.01
	0.01
	kg N2O-N/kg N

	Nrate(T)
	0.42
	0.24
	kg N/1000kg animal mass/day

	NEXIPCC default
	 Refer to Table 8

	Wsite
	 Refer to Table 8

	TAM
	28.00
	28.00
	kg

	Wdefault
	28
	28
	kg

	NEXLT,y
	 Refer to Table 8

	NLT
	 Refer to Table 8

	MS%Bl,j
	100%
	100%
	/

	Fgasm
	40%
	40%
	/

	GWPN2O
	265
	265
	tCO2/t N2O

	CFN20,N-N
	1.57
	1.57
	Conversion Factor N2O-N to N2O

	01/08/2021-31/12/2021
	4,138
	tCO2e

	01/01/2022-31/07/2022
	5,751
	tCO2e

	BEN2O,y
	9,889
	tCO2e



Table 11 The calculation results of baseline emissions for SDG 13
	Period
	BECH4(tCO2e)
	BEN2O,y(tCO2e)
	BEy(tCO2e)

	01/08/2021-31/12/2021
	277,773
	4,138
	281,911

	01/01/2022-31/07/2022
	385,739
	5,751
	391,490

	2nd monitoring period
	663,512
	9,889
	673,401



[bookmark: _Hlk75252423]Total SDG 13 baseline impact (baseline emissions) of the 2nd monitoring period was 673,401 tCO2e.

[bookmark: _Ref315873986][bookmark: _Ref418095432][bookmark: _Toc40962781]Calculation of project value or estimation of project situation of each SDG Impact
>>
SDG 7 Impact of project situation
From 01/08/2021 to 31/12/2021, 31,911.21 MWh of electricity was generated through capturing biogas.
From 01/01/2022 to 31/07/2022,42,716.20 MWh of electricity was generated through capturing biogas.
For the 2nd monitoring period from 01/08/2021 to 31/07/2022, total 74,627.41MWh of electricity was generated through capturing biogas.

SDG 8 Impact of project situation
From 01/08/2021 to 31/12/2021, 20 jobs for local people were created (including 10 females and 10 males), the average monthly earnings of employees were 5,000 RMB/person. Equal salaries were paid for men and women in the same position.
From 01/01/2022 to 31/07/2022, 20 jobs for local people were created (including 10 females and 10 males), the average monthly earnings of employees were 5,000 RMB/person. Equal salaries were paid for men and women in the same position.
For the 2nd monitoring period from 01/08/2021 to 31/07/2022, 20 jobs for local people were created (including 10 females and 10 males), the average monthly earnings of employees were 5,000 RMB/person. Equal salaries were paid for men and women in the same position.

SDG 13 Impact of project situation
As per section B.6 of the PDD, project emissions can be calculated as follows,


            (Equation 12)
where：
	PEy
	Project emissions in year y

	PEAD,y
	Project emissions associated with the anaerobic digester in year y (t CO2e/yr) 

	PEAer,y
	Project CH4 emissions from aerobic AWMS treatment (t CO2e/yr) 

	PEN2O,y
	Project N2O emissions in year y (t CO2/yr) 

	PEEC/FC,y
	Project emissions from electricity consumption and fossil fuel combustion (t CO2e/yr)



i) Project emissions associated with the anaerobic digester in year y (PEAD,y)
Based on the methodology ACM0010” GHG emission reductions from manure management systems (Version 08.0)”. PEAD,y is determined using the methodological tool “Project and leakage emissions from anaerobic digesters”.
According to the TOOL14” Project and leakage emissions from anaerobic digesters (Version 02.0)”, the project emissions associated with the anaerobic digester (PEAD,y) are determined as follows:
              (Equation 13)
where:
	PEAD,y
	Project emissions associated with the anaerobic digester in year y (t CO2e) 

	PEEC,y
	Project emissions from electricity consumption associated with the anaerobic digester in year y (t CO2e) 

	PEFC,y
	Project emissions from fossil fuel consumption associated with the anaerobic digester in year y (t CO2e) 

	PECH4, y
	Project emissions of methane from the anaerobic digester in year y (t CO2e) 

	PEflare,y
	Project emissions from flaring of biogas in year y (t CO2e) 



The biogas generated during the treatment process in this project will be captured for power generation and all the electricity generated from this project will be used by the AWMSs and 10 swine farms. The electricity generated will not be connected to another user or the regional power grid. As the electricity consumption of the anaerobic digestion system cannot be measured separately from the entire AWMSs, so the Project emissions from electricity consumption associated with the anaerobic digester and that is not related to the anaerobic digester is calculated together.
The project emissions from electricity consumption calculated according to the “Baseline, project and/or leakage emissions from electricity consumption and monitoring of electricity generation”, 
              (Equation 14)
Where 
	PEEC,y
	Project emissions from electricity consumption in year y (t CO2e) 

	EGPJ,J,y
	Quantity of electricity consumed by the project electricity consumption source j in year y (MWh/yr) 

	EFEF,j, y
	Emission factor for electricity generation for source j in year y (t CO2/MWh)  

	TDLj,y
	Average technical transmission and distribution losses for providing electricity to source j in year y  



[bookmark: _Hlk111022399][bookmark: _Hlk95486478]During this monitoring period, the electricity generated by the project was used firstly for the operation of AWMSs normally, only when the biogas generators were not operation, the electricity consumption of AWMSs were sourced from the grid company.

The anaerobic digestion process of this project does not involve the use of fossil fuels, so the project emissions from fossil fuel consumption associated with the anaerobic digester is 0, i.e., PEFC,y=0 

The residual gas is sent to flare system (if any) and project emissions from flaring of biogas (PEflare,y) shall be estimated using the tool  “ Project emissions from flaring”. For this monitoring period, there is no residual gas to be flared, so PEflare,y=0.

In summary, the project emissions associated with the anaerobic digester in year y (t CO2e) is the project emissions of methane from the anaerobic digester in year y (t CO2e). i.e., PEAD,y= PECH4, y.

Determination of project emissions of methane from the anaerobic digester (PECH4,y)
PECH4,y was determined following the step 4 of the applied tool “Project and leakage emissions from anaerobic digesters(Version 02.0)”.Project emissions of methane from the anaerobic digester include emissions during maintenance of the digester, physical leaks through the roof and side walls, and release through safety valves due to excess pressure in the digester. These emissions are calculated using a default emission factor (𝐸𝐹𝐶𝐻4, 𝑑𝑒𝑓𝑎𝑢𝑙𝑡), as follows:
             (Equation 15)
where:
	PECH4, y
	Project emissions of methane from the anaerobic digester in year y (t CO2e) 

	QCH4,y
	Quantity of methane produced in the anaerobic digester in year y (t CH4) 

	EFCH4,default
	Default emission factor for the fraction of CH4 produced that leaks from the anaerobic digester (fraction) 

	GWPCH4
	Global warming potential of CH4 (t CO2 / t CH4) 



Estimation of various variables and parameters for above equations:
(A) Quantity of methane produced in the anaerobic digester QCH4,y
As per PDD, the biogas is produced and collected from anaerobic digestion process. The flowmeters are installed at the outlet of the biogas digesters and the measured on an hourly basis time interval. So the quantity of methane produced in the digester in year y (𝑄𝐶𝐻4,𝑦) is the accumulation of the mass flow of methane in the gaseous stream in an hourly basis time interval. i.e., QCH4,y =

The mass flow of greenhouse gas i (Fi,t) is determined as follows: 
               (Equation 16)
                  (Equation 17)
where:
	Fi,t
	Mass flow of greenhouse gas i in the gaseous stream in time interval t (kg gas/h) 

	Vt,db
	Volumetric flow of the gaseous stream in time interval t on a dry basis (m³ dry gas/h) 

	
	Volumetric fraction of greenhouse gas i in the gaseous stream in a time interval t on a dry basis (m³ gas i/m³ dry gas) 

	
	Density of greenhouse gas i in the gaseous stream in time interval t (kg gas i/m³ gas i) 

	Pt
	Absolute pressure of the gaseous stream in time interval t (Pa) 

	MMi
	Molecular mass of greenhouse gas i (kg/kmol) 

	Ru
	Universal ideal gases constant (Pa.m3/kmol.K) 

	Tt
	Temperature of the gaseous stream in time interval t (K) 



ii) Project CH4 emissions from aerobic AWMS treatment (PEAer, y)
IPCC guidelines specify emissions from aerobic lagoons as 0.1 per cent of total methane generating potential of the waste processed, which can be used as a default for all types of aerobic AWMS treatment. 
               (Equation 18)
where:
	GWPCH4
	Global Warming Potential (GWP) of CH4 (t CO2e/tCH4) 

	RVS,n
	Fraction of volatile solid degraded in AWMS treatment method n of the N treatment steps prior to waste being treated (fraction) 

	DCH4
	Density of CH4 (t/m3) 

	FAer
	Fraction of volatile solid directed to aerobic system (fraction) 

	LT
	Type of livestock 

	Bo,LT
	Maximum methane producing potential of the volatile solid generated by animal type LT (m3CH4/kg dm) 

	VSLT,y
	Annual volatile solid excretion livestock type LT entering all AWMS on a dry matter weight basis in (kg -dm/animal/yr) 

	NLT
	Annual average number of animals of type LT for the year y (number) as estimated in equation (5(a)) or (5(b)) 

	PEsl,y
	Project CH4 emissions from sludge disposed of in storage pit prior to disposal during the year y (t CO2e/yr) 

	MS%j
	Fraction of manure handled in system j in the project activity (fraction) 



[bookmark: _Hlk95486508]All sludge produced from the aerobic composting will be used for land application, which is calculated as leakage emission, so the PEsl,y=0.
So,       (Equation 19)
where:
	GWPCH4
	Global Warming Potential (GWP) of CH4 (t CO2e/tCH4) 

	RVS,n
	Fraction of volatile solid degraded in AWMS treatment method n of the N treatment steps prior to waste being treated (fraction) 

	DCH4
	Density of CH4 (t/m3) 

	FAer
	Fraction of volatile solid directed to aerobic system (fraction) 

	LT
	Type of livestock 

	Bo,LT
	Maximum methane producing potential of the volatile solid generated by animal type LT (m3CH4/kg dm) 

	VSLT,y
	Annual volatile solid excretion livestock type LT entering all AWMS on a dry matter weight basis in (kg -dm/animal/yr) 

	NLT
	Annual average number of animals of type LT for the year y (number) as estimated in equation (5(a)) or (5(b)) 

	MS%j
	Fraction of manure handled in system j in the project activity (fraction) 



iii) Project N2O emissions in year y (PEN2O,y)
          (Equation 20)
where:
	PEN2O,y
	Project N2O emissions in year y (t CO2/yr) 

	GWPN2O
	Global Warming Potential (GWP) for N2O (t CO2e/tN2O) 

	CFN2O-N,N
	Conversion factor N2O-N to N2O (44/28) 

	EN2O,D,y
	Direct N2O emission in year y (kg N2O-N/year) 

	EN2O,ID,y
	Indirect N2O emission in year y (kg N2O-N/year) 



             (Equation 21)
where：
	EN2O,D,y
	Direct N2O emission in year y (kg N2O-N/yr) 

	EFN2O,D,j
	Direct N2O emission factor for the treatment system j of the manure management system (kg N2O-N/kg N) 

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) estimated as described in appendix 2 

	MS%j
	Fraction of manure handled in system j (fraction) 

	NLT
	Annual Average number of animals of type LT for the year y estimated as per equation (4) or (5) (number) 



     (Equation 22)
where:
	EN2O,ID,y
	Indirect N2O emission in year y (kg N2O-N/year) 

	EFN2O,ID
	Indirect N2O emission factor for N2O emissions from atmospheric deposition of nitrogen on soils and water surfaces (kgN2O-N/kg NH3-N and NOX-N) 

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/yr) estimated as described in appendix 2 

	MS%j
	Fraction of manure handled in system j (fraction) 

	FgasMS,j,LT
	Default values for nitrogen loss due to volatilisation of NH3 and NOX from manure management (fraction) 

	NLT
	Annual Average number of animals of type LT for the year y estimated as per equation (4) or (4) (number) 



iV) Project emissions from use of heat and/or electricity (PEelec/heat)
        (Equation 23)
where:
	PEEC,y
	Project emissions from electricity consumption in year y. The project emissions from electricity consumption will be calculated following the latest version of the “Tool to calculate baseline, project and/or leakage emissions from electricity consumption”. In case, the electricity consumption is not measured then the electricity consumption shall be estimated as follows , where CPi,y is the rated capacity (in MW) of electrical equipment i used for the project activity. 

	PEFC,y
	Project emissions from fossil fuel combustion in process j during the year y. The project emissions from fossil fuel combustion will be calculated following the latest version of the “Tool to calculate project or leakage CO2 emissions from fossil fuel combustion”. For this purpose, the processes j in the tool corresponds to all fossil fuel combustion in the AWMS (not including fossil fuels consumed for transportation of feed material and sludge or any other on-site transportation). 



[bookmark: _Hlk95297346]These emissions should only be considered for consumption of electricity or heat that is not related to the anaerobic digester. As described in above, since the electricity consumption that is not related to the anaerobic digester cannot be separated from the total electricity consumption, therefore the emission for consumption of electricity is calculated in PEEC,y.

[bookmark: _Hlk95486529] No fossil fuel was consumed in process that is not related to the anaerobic digester, so PEFC,y=0 

[bookmark: _Hlk95486546]Therefore, PEelec/heat that is not related to the anaerobic digester =0
[bookmark: _Hlk95486571]Table 12 The calculation result of PEEC,y
	Period
	ECPJ,j,y (MWh)
	EFEF,j,y (tCO2/MWh)
	TDLj,y
	PEEC,y (tCO2e)

	01/08/2021-31/08/2021
	238.308
	0.57205
	20%
	163.59

	01/09/2021-30/09/2021
	230.8488
	0.57205
	20%
	158.47

	01/10/2021-31/10/2021
	238.7772
	0.57205
	20%
	163.92

	01/11/2021-30/11/2021
	231.3072
	0.57205
	20%
	158.79

	01/12/2021-31/12/2021
	239.2488
	0.57205
	20%
	164.24

	01/01/2022-31/01/2022
	239.4864
	0.57205
	20%
	164.40

	01/02/2022-28/02/2022
	216.522
	0.57205
	20%
	148.64

	01/03/2022-31/03/2022
	239.9592
	0.57205
	20%
	164.73

	01/04/2022-30/04/2022
	232.446
	0.57205
	20%
	159.57

	01/05/2022-31/05/2022
	240.4284
	0.57205
	20%
	165.05

	01/06/2022-30/06/2022
	232.9008
	0.57205
	20%
	159.88

	01/07/2022-31/07/2022
	240.9012
	0.57205
	20%
	165.37

	01/08/2021-31/12/2021
	1,178.49
	0.57205
	20%
	810

	01/01/2022-31/07/2022
	1,642.644
	0.57205
	20%
	1,128



Table 13 The calculation result of PECH4,y
	Period
	GWPCH4 (tCO2/tCH4)
	EFCH4,default (
tCH4 leaked / tCH4 produced)
	QCH4,y (tCH4)
	PECH4,y (tCO2e)

	01/08/2021-31/08/2021
	28
	0.05
	1,933.92
	2,707.49

	01/09/2021-30/09/2021
	28
	0.05
	1,887.19
	2,642.07

	01/10/2021-31/10/2021
	28
	0.05
	1,904.68
	2,666.56

	01/11/2021-30/11/2021
	28
	0.05
	1,804.80
	2,526.73

	01/12/2021-31/12/2021
	28
	0.05
	1,874.02
	2,623.63

	01/01/2022-31/01/2022
	28
	0.05
	1,954.29
	2,736.01

	01/02/2022-28/02/2022
	28
	0.05
	1,692.34
	2,369.28

	01/03/2022-31/03/2022
	28
	0.05
	1,908.33
	2,671.66

	01/04/2022-30/04/2022
	28
	0.05
	1,880.82
	2,633.16

	01/05/2022-31/05/2022
	28
	0.05
	1,878.99
	2,630.60

	01/06/2022-30/06/2022
	28
	0.05
	1,858.73
	2,602.22

	01/07/2022-31/07/2022
	28
	0.05
	1,957.34
	2,740.28

	01/08/2021-31/12/2021
	-
	-
	9,404.61
	13,167

	01/01/2022-31/07/2022
	-
	-
	13,130.84
	18,384



Table 14 The calculation result of PEAD,y
	Period
	PEEC,y
(tCO2e)
	PECH4,y
(tCO2e)
	PEAD,y
(tCO2e)

	01/08/2021-31/12/2021
	810
	13,167
	13,977

	01/01/2022-31/07/2022
	1,128
	18,384
	19,512

	2nd monitoring period
	1,938
	31,551
	33,489



Table 15 The calculation result of PEAer,y
	Parameter
	Value
	Unit

	species
	Market Swine
	Breeding Swine
	

	GWPCH4
	28
	28
	tCO2/tCH4

	DCH4
	0.00067
	0.00067
	t/m3

	
	0.001
	0.001
	kg N/1000kg animal mass/day

	FAer
	100%
	100%
	/

	1-Rvs,1
	54%
	54%
	/

	B0,LT
	0.29
	0.29
	m3CH4/kg-dm 

	NLT
	Refer to Table 8

	VSLT,y
	Refer to Table 8

	MS%j
	100%
	100%
	

	01/08/2021-31/12/2021
	210
	tCO2e

	01/01/2022-31/07/2022
	293
	tCO2e

	PEAer,y
	503
	tCO2e



Table 16 The calculation result of PEN2O,y
	Parameter
	Value
	Unit

	species
	Market Swine
	Breeding Swine
	

	EFN2O,D,j
	0
	0
	kg N2O-N/kg N

	NEXLT,y
	 Refer to Table 8

	NLT
	Refer to Table 8

	MS%j
	100%
	100%
	/

	01/08/2021-31/12/2021
	0
	kg N2O-N/year

	01/01/2022-31/07/2022
	0
	kg N2O-N/year

	EN2O,D,y
	0.00

	kg N2O-N/year

	EFN2O,D,j
	0.006
	0.006
	kg N2O-N/kg N

	NEXLT,y
	Refer to Table 8

	NLT
	Refer to Table 8

	MS%j
	100%
	100%
	/

	01/08/2021-31/12/2021
	14,912
	kg N2O-N/year

	01/01/2022-31/07/2022
	20,724
	kg N2O-N/year

	EN2O,D,y
	35,636
	kg N2O-N/year

	EFN2O,iD,j
	0.01
	0.01
	kg N2O-N/kg NH3 and NOX-N

	FgasMS,j,LT
	0.4
	0.4
	/

	NEXLT,y
	 Refer to Table 8

	NLT
	Refer to Table 8

	MS%j
	100%
	100%
	%

	GWPN2O
	265
	265
	tCO2/tN2O

	01/08/2021-31/12/2021
	9,943
	kg N2O-N/year

	01/01/2022-31/07/2022
	13,819
	kg N2O-N/year

	EN2O,ID,y
	23,762
	kg N2O-N/year

	EFN2O,iD,j
	0.01
	0.01
	kg N2O/kg N

	FgasMS,j,LT
	0.45
	0.45
	/

	NEXLT,y
	 Refer to Table 8

	NLT
	Refer to Table 8

	MS%j
	100%
	100%
	%

	GWPN2O
	265
	265
	tCO2/t N2O

	01/08/2021-31/12/2021
	11,184
	kg N2O-N/year

	01/01/2022-31/07/2022
	15,544
	kg N2O-N/year

	EN2O,ID,y
	26,728
	kg N2O-N/year

	01/08/2021-31/12/2021
	15,008
	tCO2e

	01/01/2022-31/07/2022
	20,858
	tCO2e

	PEN2O,y
	35,866
	tCO2e



Table 17 Calculation results of project emissions for SDG 13
	Period
	PEAD,y
(tCO2e)
	PEAer,y 
(tCO2e)
	PEN2O,y
(tCO2e)
	PEy
(tCO2e)

	01/08/2021-31/12/2021
	13,977
	210
	15,008
	29,195

	01/01/2022-31/07/2022
	19,512
	293
	20,858
	40,663

	2nd monitoring period
	33,489
	503
	35,866
	69,858



[bookmark: _Toc40962782]Calculation of leakage 
>>
As per section B.6.1 of the PDD, Leakage can be calculated as follows,
            (Equation 24)
Where:
	LEPJ, N2O, y
	Leakage N2O emissions released during project activity from land application of the treated manure in year y (t CO2e/yr) 

	LEBL, N2O, y
	Leakage N2O emissions released during baseline scenario from land application of the treated manure in year y (t CO2e/yr) 

	LEPJ, CH4, y
	Leakage CH4 emissions released during project activity from land application of the treated manure in year y (t CO2e/yr) 

	LEBL, CH4, y
	Leakage CH4 emissions released during baseline scenario from land application of the treated manure in year y (t CO2e/yr) 

	LEAD, y
	Leakage emissions associated with the anaerobic digester in year y (t CO2e) 



i) Estimation of leakage N2O emissions released during baseline scenario from land application of the treated manure in year y, LEBL, N2O, y
       (Equation 25)
         (Equation 26)
        (Equation 27)
      (Equation 28)
where:
	GWPN2O
	Global Warming Potential (GWP) for N2O (t CO2e/tN2O)

	CFN2O-N,N
	Conversion factor N2O-N to N2O (44/28)

	LEN2O,land,y
	Leakage N2O emissions from application of manure waste in year y (kg N2O-N/year)

	LEN2O,runoff,y
	Leakage N2O emissions due to leaching and run-off in year y (kg N2O-N/year)

	LEN2O,vol,y
	Leakage N2O emissions due to volatilisation in year y (kg N2O-N/year)

	Fgasm
	Fraction of N lost due to volatilization (fraction) 

	NLT
	Annual average number of animals of type LT estimated as per equation (4) or (5) (number) 

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/year) estimated as described in appendix 2 

	EF1
	Emission factor for N2O emissions from N inputs (kg N2O-N/kg N input) 

	EF5
	Emission factor for N2O emissions from N leaching and runoff in (kg N2O-N/kg N leached and runoff) 

	EF4
	Emission factor for N2O emissions from atmospheric deposition of N on soils and water surfaces, [kg N- N2O/ (kg NH3-N + NOX-N volatilized)] 

	Fleach
	Fraction of all N added to/mineralised in managed soils in regions where leaching/runoff occurs that is lost through leaching and runoff (fraction) 

	RN,n
	Nitrogen reduction factor (fraction) 



ii) Estimation of leakage N2O emissions released during project activity from land application of the treated manure in year y, LEPJ, N2O
  (Equation 29)
    (Equation 30)
    (Equation 31)
    (Equation 32)
where:
	GWPN2O
	Global Warming Potential (GWP) for N2O (t CO2e/tN2O)

	CFN2O-N,N
	Conversion factor N2O-N to N2O (44/28)

	LEN2O,land,y
	Leakage N2O emissions from application of manure waste in year y (kg N2O-N/year)

	LEN2O,runoff,y
	Leakage N2O emissions due to leaching and run-off in year y (kg N2O-N/year)

	LEN2O,vol,y
	Leakage N2O emissions due to volatilisation in year y (kg N2O-N/year)

	Fgasm
	Fraction of N lost due to volatilization (fraction) 

	NLT
	Annual average number of animals of type LT estimated as per equation (4) or (5) (number) 

	NEXLT,y
	Annual average nitrogen excretion per head of a defined livestock population (kg N/animal/year) estimated as described in appendix 2 

	EF1
	Emission factor for N2O emissions from N inputs (kg N2O-N/kg N input) 

	EF5
	Emission factor for N2O emissions from N leaching and runoff in (kg N2O-N/kg N leached and runoff) 

	EF4
	Emission factor for N2O emissions from atmospheric deposition of N on soils and water surfaces, [kg N- N2O/ (kg NH3-N + NOX-N volatilized)] 

	Fleach
	Fraction of all N added to/mineralised in managed soils in regions where leaching/runoff occurs that is lost through leaching and runoff (fraction) 

	RN,n
	Nitrogen reduction factor (fraction) 



[bookmark: _Hlk111023305]It is not possible to measure the quantity of manure applied to land in kg manure/yr (QDM) and the nitrogen concentration in kg N/kg manure (NDM) in the manure to estimate the total quantity of nitrogen applied to land. In this case, is used for calculation. 

iii) Estimation of leakage CH4 emissions from land application of the treated manure
The calculation of methane emissions from land application of manure in the baseline and project cases are estimated as below: 
   (Equation 33)
   (Equation 34)
where:
	LEBL,CH4,y
	Leakage CH4 emissions released during baseline scenario from land application of the treated manure in year y (t CO2e/yr) 

	LEPJ,CH4,y
	Leakage CH4 emissions released during project activity from land application of the treated manure in year y (t CO2e/yr) 

	RVS,n
	Fraction of volatile solid degraded in AWMS treatment method n of the N treatment steps prior to sludge being treated 

	GWPCH4
	Global Warming Potential (GWP) of CH4 (t CO2e/tCH4) 

	DCH4
	Density of CH4 (t/m3) 

	B0,LT
	Maximum methane producing potential of the volatile solid generated by animal type LT (m3CH4/kg dm) 

	NLT
	Annual average number of animals of type LT estimated as per equation (4) or (5), expressed (number) 

	VSLT,y
	Annual volatile solid excretions for livestock LT entering all AWMS on a dry matter weight basis (kg -dm/animal/yr) 

	MS%j
	Fraction of manure handled in system j in the project activity (fraction) 

	MCFd
	Methane conversion factor (MCF) assumed to be equal to 1 



iV) Estimation of leakage emissions associated with the anaerobic digester
LEAD,y is determined using the methodological tool “Project and leakage emissions from anaerobic digesters(Version 02.0). 
The leakage emissions associated with the anaerobic digester (𝐿𝐸𝐴𝐷,𝑦) depend on how the digestate is managed. They include emissions associated with storage and composting of the digestate and are determined as follows:
     (Equation 35)
where:
	LEAD,y
	Leakage emissions associated with the anaerobic digester in year y (t CO2e) 

	LEstorage,y
	Leakage emissions associated with storage of digestate in year y (t CO2e) 

	LEcomp,y
	Leakage emissions associated with composting digestate in year y (t CO2e) 



The anaerobic digestion process of this project is carried out in a fully enclosed system, the flaring will be not taken into account as the equipment will only be used when there will be surplus biogas, normally there will be no surplus biogas during the operational period of the project. After anaerobic digestion, the fermented sludge will be treated in aerobic composting system, which will be used as fertilizer. Wastewater from the new animal waste management systems will be treated aerobically and then used for agriculture irrigation.so, the Estimation of leakage emissions associated with the anaerobic digester is 0. i.e., LEAD,y =0.
Table  18 The calculation results of LEB,CH4、LEp,CH4、LEB,N2O and LEp,N2O
	Parameter
	Value
	Unit

	species
	Market Swine
	Breeding Swine
	

	NLT
	Refer to Table 8

	NEXLT,y
	 Refer to Table 8

	RN,n
	80%
	80%
	/

	EF1
	0.01
	0.01
	kg N2O-N/kg N

	EF5
	0.0075
	0.0075
	kg N2O-N/kg N

	EF4
	0.01
	0.01
	 KgN-N2O-N/kg NH3-N+NOX-N

	Fleach
	0.3
	0.3
	/

	Fgasm
	0.2
	0.2
	/

	GWPN2O
	265
	265
	tCO2/t N2O

	01/08/2021-31/12/2021
	4,964
	kg N2O-N/year

	01/01/2022-31/07/2022
	6,900
	kg N2O-N/year 

	LEN2O,land,y
	11,864
	kg N2O-N/year

	01/08/2021-31/12/2021
	1,112
	kg N2O-N/year

	01/01/2022-31/07/2022
	1,548
	kg N2O-N/year

	LEN2O,runoff,y
	2,660
	kg N2O-N/year

	01/08/2021-31/12/2021
	989
	kg N2O-N/year

	01/01/2022-31/07/2022
	1,376
	kg N2O-N/year

	LEN2O,vol,y
	2,365
	kg N2O-N/year

	01/08/2021-31/12/2021
	2,942
	tCO2e

	01/01/2022-31/07/2022
	4,090
	tCO2e

	LEBJ,N2O,y
	7,032
	tCO2e

	NLT
	Refer to Table 8

	NEXLT
	 Refer to Table 8

	RN
	25%
	25%
	/

	EF1
	0.01
	0.01
	kg N2O-N/kg N

	EF5
	0.0075
	0.0075
	kg N2O-N/kg N

	EF4
	0.01
	0.01
	KgN-N2O-N/kg NH3-N+NOX-N

	Fleach
	0.3
	0.3
	/

	Fgasm
	0.2
	0.2
	/

	01/08/2021-31/12/2021
	18,638
	  kg N2O-N/year

	01/01/2022-31/07/2022
	25,902
	  kg N2O-N/year

	 LEN2O,land,y
	44,540
	  kg N2O-N/year

	01/08/2021-31/12/2021
	4,198
	  kg N2O-N/year

	01/01/2022-31/07/2022
	5,834
	  kg N2O-N/year

	LEN2O,runoff,y
	10,032
	  kg N2O-N/year

	01/08/2021-31/12/2021
	3,731
	  kg N2O-N/year

	01/01/2022-31/07/2022
	5,186
	  kg N2O-N/year

	LEN2O,vol,y
	8,917
	  kg N2O-N/year

	01/08/2021-31/12/2021
	11,064
	 tCO2e

	01/01/2022-31/07/2022
	15,376
	 tCO2e

	LEPJ,N2O,y
	26,440
	tCO2e

	GWPCH4
	28
	28
	tCO2e/t CH4

	DCH4
	0.00067
	0.00067
	t/m3

	MCFd
	1
	1
	/

	VSLT,y
	 Refer to Table 8

	NLT
	Refer to Table 8

	B0,LT
	0.29
	0.29
	m3 CH4/kg-VS

	RVS
	85%
	85%
	/

	MS%j
	100%
	100%
	/

	01/08/2021-31/12/2021
	57,562
	tCO2e

	01/01/2022-31/07/2022
	79,935
	tCO2e

	LEBLCH4,y
	137,497
	tCO2e

	GWPCH4
	28
	28
	tCO2/tCH4

	DCH4
	0.00067
	0.00067
	t/m3

	MCFd
	1
	1
	/

	VSLT,y
	 Refer to Table 8

	NLT
	Refer to Table 8

	B0
	0.29
	0.29
	m3 CH4/kg-VS

	RVS
	2%
	2%
	/

	RVS
	45%
	45%
	/

	RVS
	35%
	35%
	/

	MS%j
	100%
	100%
	/

	01/08/2021-31/12/2021
	134,460
	tCO2e

	01/01/2022-31/07/2022
	186,722
	tCO2e

	LE PJ,CH4,y
	321,182
	tCO2e



Table 19 Calculation results of leakage for SDG 13
	Period
	LEPJ,CH4,y 
(tCO2e)
	LEBL,CH4,y 
(tCO2e)
	LEBL,N2O,y (tCO2e)
	LEPJ,N2O,y (tCO2e)
	LEy
(tCO2e/yr)

	01/08/2021-31/12/2021
	134,460
	57,562
	2,942
	11,064
	85,020

	01/01/2022-31/07/2022
	186,722
	79,935
	4,090
	15,376
	118,073

	2nd monitoring period
	321,182
	137,497
	7,032
	26,440
	203,093



[bookmark: _Toc40953319][bookmark: _Toc40953601][bookmark: _Toc40962783][bookmark: _Ref315873988][bookmark: _Toc40962784][bookmark: _Toc40962785]Calculation of net benefits or direct calculation for each SDG Impact

	SDG
	SDG Impact
	Baseline 
estimate
	Project 
estimate
	Leakage estimate
	Net 
benefit

	13
	Emission Reductions
	673,401tCO2e
	69,858tCO2e
	203,093tCO2e
	400,450tCO2e

	7
	Quantity of electricity generation by capturing biogas
	0MWh
	74,627.41MWh
	NA
	74,627.41MWh

	8
	Number of males and females employed by the project
	0 jobs for local people were created
	20 jobs for local people were created (including 10 females and 10 males)
	NA
	20 jobs for local people were created (including 10 females and 10 males)

	8
	Average monthly salary
	0 jobs created, 0 income
	5,000 RMB/person, and equal salaries were paid for men and women in the same position.
	NA
	5,000 RMB/person, and equal salaries were paid for men and women in the same position.



Furthermore, if the actual methane captured from anaerobic digesters in project activity is lower than (BECH4,y - PEAD,y), then (BECH4,y - PEAD,y) is replaced by actual methane captured QCH4,y.

Biogas captured during monitoring period is 59,862,507.40 m3, which equals to 630,992 tCO2e[footnoteRef:14]. Baseline methane emission (BECH4,y) is 663,512 tCO2e. project emissions associated with anaerobic digester is (PEAD,y) is 33,489 tCO2e. Actual methane captured from anaerobic digesters is higher than the difference of BECH4,y and  PEAD,y. Therefore, the equation (BECH4,y - PEAD,y) can be used to calculate emission reduction. [14:  Biogas captured during this monitoring period is 59,862,507.40m3. The quality of methane is 22,535.44tCH4, which can be calculated by the amount of biogas, the density of biogas and the content of methane in this monitoring period. Then the quality of methane multiplied by the global warming potential of CH4 i.e. 28tCO2/tCH4.is the result of 630,992 tCO2e.Please refer to the ER calculation sheet for more details.] 


[bookmark: _Toc40962786]Comparison of actual SDG Impacts with estimates in approved PDD 
	SDG
	Values estimated in ex ante calculation of approved PDD 
for this monitoring period
	Actual values[footnoteRef:15] achieved during this monitoring period [15:  Whenever emission reductions are capped, both the original and capped values used for calculations must be transparently reported.  Use brackets to denote original values.] 


	13
	2nd monitoring period: 498,011tCO2e[footnoteRef:16] [16:  Yearly total amount estimated emission reduction in PDD is 498,011 tCO2e, the 2nd monitoring period is from 01/08/2021 to 31/07/2022, covering 365 days. ] 

	400,450 tCO2e

	7
	2nd monitoring period: 105,690.39MWh[footnoteRef:17] of electricity generation by capturing biogas [17:  Annually electricity generation in PDD is 105,690.39MWh, the 2nd monitoring period is from 01/08/2021 to 31/07/2022, covering 365 days.] 

	74,627.41MWh of electricity generation by capturing biogas

	8
	2nd monitoring period:20 jobs for local people created (including 10 females and 10 males).
Average monthly salary 5,000 RMB/person, and equal salaries paid for men and women in the same position.
	20 jobs for local people created (including 10 females and 10 males).
Average monthly salary 5,000 RMB/person, and equal salaries paid for men and women in the same position.




[bookmark: _Ref4665389]Explanation of calculation of value estimated ex ante calculation of approved PDD for this monitoring period
>>
[bookmark: _Hlk111028224]According to PDD, the estimated outcomes of SDG 7 for the 2nd monitoring period are 105,690.39MWh of electricity generation which is calculated according to the amount of biogas produced theoretically and the assumed electricity generation value per cubic metre of biogas in project evaluation report. while the actual outcomes of SDG7 is 74,627.41MWh of electricity generation in the 2nd monitoring period, which is monitored by the meters installed at the outlet of generators. 

The estimated value of the outcomes of SDG 13 for the 2nd monitoring period is 498,011 tCO2e, while the actual outcomes of SDG13 is 400,450 tCO2e. The calculation of the estimated and actual value of SDG 13 is based on methodology ACM0010” GHG emission reductions from manure management systems” (version 08.0). The mainly difference between the estimated value and actual value is due to the changes of the number of animals in the swine farm (NLT), the average animal weight (Wsite) and the actual biogas captured from anaerobic digester.

Number of males and females employed by the project and average monthly salary during the 2nd monitoring period were determined by the Record Keeping Book and Labor contracts and Payrolls. 20 jobs for local people were created (including 10 females and 10 males). The average monthly salary was 5,000 RMB/person (equal salaries paid for men and women in the same position). Outcomes of SDG 8 are consistent with the estimated outcomes in the PDD. 

[bookmark: _Toc40962789]Remarks on increase in achieved SDG Impacts from estimated value in approved PDD
>>
[bookmark: _Hlk111028384]The actual outcomes of SDG 7 are much lower than the estimated value in the PDD. The main reason for the difference is that the actual electricity generation through capturing biogas is related to the amount of methane produced, the efficiency of generator, etc. And the captured biogas during this MP is lower than the estimated value in PDD. 

The estimated value of the outcomes of SDG 13 for the 2nd monitoring period is 498,011 tCO2e, and the actual value is 400,450 tCO2e, which is lower than the estimated value in PDD. the difference between the estimated value and actual values is mainly due to the number of animals in the swine farm and the average animal weight is lower than the estimated values in the PDD. Furthermore, a maximum 100% of MS%j is applied for calculation project emission during this monitoring period, which brings a higher project emission comparing to the PDD.

Outcomes of SDG 8 are consistent with the estimated outcomes in the PDD. 

[bookmark: _Toc40962790][bookmark: _Ref47706347][bookmark: _Ref49860694]SAFEGUARDS REPORTING
[bookmark: _Toc40962791]>>
According to the Section D.1 and Appendix 1 in PDD, only one assessment question answered ‘Potentially’ i.e., in case of biogas is not handled properly during the operation period of the project, methane explosion may be caused. Therefore, mitigation measure for safeguarding principles is required and the parameter of Employee Training of biogas safety operation during the operation period shall be monitored, which is described in section D.2 of this MR.

During this monitoring period, no biogas explosion or leakage was happened. The monitoring of this parameters was fully implemented in accordance with the monitoring plan in PDD and the monitoring activities was successful, so there is no need to update the mitigation measures.
[bookmark: _Toc40962792][bookmark: _Ref47706354][bookmark: _Ref49860701]STAKEHOLDER INPUTS AND LEGAL DISPUTES 
[bookmark: _Toc40962793]List all Inputs and Grievances which have been received via the Continuous Input and Grievance Mechanism together with their respective responses/mitigations. 
>>
	Method
	Include all details of Chosen Method (s) so that they may be understood and, where relevant, used by readers.  

	Continuous Input / Grievance Expression Process Book (mandatory)
	The grievance books were put in Front Desk Administration of the project owner i.e., each farm (the address of each farm is as below table:) All stakeholders are allowed to record their grievances or comments in the book. The project owner will assign specific person to deal with related issues. When assessing the relevance and appropriateness of the stakeholders’ comments, the project owner will apply a gender lens.
	Swine farm
	Address

	Guanxi
	Guanxi Town, Longnan County, Ganzhou City

	Jiading
	Jiading Town, Xinfeng County, Ganzhou City

	Datang
	Datangbu Town, Xinfeng County, Ganzhou City

	Baishu
	Jiading Town, Xinfeng County, Ganzhou City

	Zhongshi
	Banshi Town, Anyuan County, Ganzhou City

	Babaodong
	Liren Town, Longnan County, Ganzhou City

	Tangcun
	Tangcun Village, Anyuan County, Ganzhou City

	Taojiang
	Taojiang Village, Longnan County, Ganzhou City

	Tianxiang
	Chemen Village, Jinxi County, Fuzhou City

	Fuwang
	Sunfang Town, Chongren County, Fuzhou City




	GS Contact (mandatory)
	help@goldstandard.org 

	Other
	Feedback can be made directly through visiting Jiangxi Zhengbang Breeding Co. Ltd. (north of Hu Dong 4th Road and east of Chanye Road, Nanchang City, Jiangxi Province), calling+86 0791--8639 7834 or sending e-mail to 57566640@qq.com.



No inputs/grievances received during the 2nd monitoring period through all the methods.

Report on any stakeholder mitigations that were agreed to be monitored. 
>>
No inputs/grievances received during the 2nd monitoring period, therefore stakeholder mitigations do not need to be reported.

[bookmark: _Toc40962796]Provide details of any legal contest that has arisen with the project during the monitoring period
>>
No legal contest or dispute has been arisen with the project during the 2nd monitoring period.
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