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U.S. Landfill Protocol
Project Data Report

The Project Data Report (PDR) Template must be completed for each verification period. This template is only intended as a guide and provides the minimum required information to be reported. This template is designed for use with the U.S. Landfill Protocol V6.0 (US LP). The project developer has the option to include additional information at their discretion.

Please note that this document will be made publicly available once the project has registered credits the verification cycle. If there is proprietary information, please provide a redacted version for publication and a non-redacted version for internal review. Please contact the Reserve to discuss what information may be allowed to be redacted.

	Account Holder
	Anew Environmental, LLC

	Project ID and Name
	CAR403 - Black Warrior Solid Waste Facility

	Cooperative/Aggregate ID (if applicable)
	Not applicable

	Current Reporting Period Dates
	01/01/2024 - 12/31/2024

	Protocol Version
	U.S. Landfill V6.0

	Claimed CRTs by Vintage
	2024: 65,612

	Date Submitted
	12/30/2025



1 [bookmark: _Toc161137246]
Introduction
Provide a general description of the project, including location, baseline scenario, project activity, etc.
The project consists of the flaring of methane in landfill gas (LFG) from the Black Warrior Solid Waste Facility. A landfill gas collection and control system (GCCS) was voluntary installed at the Black Warrior Solid Waste Facility in 2009 consisting of an active LFG collection system witn an open flare. The project start date is January 14, 2009, which is when flaring of LFG from the GCCS began.
The landfill and project are located in Coker, Alabama. The landfill is owned by the Black Warrior Solid Waste Disposal Authority (BWSWA) and began operations in 1978. The design capacity of IRCL is 8.915 million tonnes.
In the baseline scenario, LFG from the GCCS would have been vented to the amosphere, since BWSWA is not required to destroy the LFG. LFG from Black Warrior Solid Waste Facility had never been destroyed in any manner prior to the project start date. 
The project activity involves operation of the flare to destroy methane in the LFG.
2 [bookmark: _Toc161137247]Project Definition
a [bookmark: _Toc161137248]Project Definition
Provide information on whether the project is an expansion of an existing landfill project or is being submitted as a new project, the type of destruction device (e.g. utility flares, enclosed flares, engines, turbines, microturbines, boilers, pipelines, leachate evaporators, kilns, sludge dryers, burners, furnaces, or fuel cells), default or site-specific destruction efficiency values, and whether landfill gas is destroyed onsite or transported for offsite use. Supporting documentation must be provided to the verifier during each verification cycle, which may include project diagrams, LFG flow data, methane flow data, facility records, etc.
The project was submitted as a new project (i.e., not an expansion of an existing project).
The destruction device is a utility flare with an assumed destruction efficiency of 96% (default value for "Open Flare" per the Protocol).
LFG is destroyed onsite.
b [bookmark: _Toc161137249]Project Developer
List the entities which have any amount of legal control over the project boundary and identify the mechanism through which the Account Holder has legal authority to implement the project. In addition, please state which entity will be designated as the project developer and will sign the Attestation of Title. If the Account Holder is not the entity listed on the facility’s operating permit, explain how they obtain the right to operate the project on the facility’s behalf.
The Black Warrior Solid Waste Disposal Authority is the landfill owner/operator and has sole legal control over the project boundary.
Anew Environmental, LLC is the project developer and has legal authority to implement the project through an agreement entered with BWSWA on June 7, 2021 to develop and monetize carbon credits from the destruction of methane from LFG. Anew has title to the offsets upon issuance from CAR. As the designated project developer, Anew will sign the Attestation of Title.
3 [bookmark: _Toc161137250]Project Eligibility
a [bookmark: _Toc161137251]Project Location
Provide the project location.
The project is located in Coker, Alabama at the following coordinates:
•	Latitude: 33.1420
•	Longitude: -87.3913
b [bookmark: _Toc161137252]Project Start Date
Briefly describe the documentation used to demonstrate the date at which the GCCS system became operational, i.e., the date landfill gas was first destroyed in a project destruction device. Provide a description of the start-up testing period (destruction device, timeline, etc.), if applicable. Include what documentation will be provided to the verification body to demonstrate the commencement of methane destruction.
The project start date is January 14, 2009, as demonstrated by the initial calibration dates provided by CDG Engineers & Associates, Inc. to confirm when the project first began continuous methane destruction.
c [bookmark: _Toc161137253]Project Crediting Period
State the project’s crediting period as defined in Section 3.2 of the Protocol.
01/14/2019 to 01/13/2029
d [bookmark: _Toc161137254]Additionality
i [bookmark: _Toc161137255]Performance Standard Test
Check the box below and provide a brief description of how the landfill gas destruction project meets the performance standard test as outlined in Section 3.4.1 of the protocol. 
|_| Installation of a landfill gas collection and a new qualifying destruction device at an eligible landfill where landfill gas has never been collected and destroyed prior to the start date.
|_| Installation of a new qualifying destruction device at an eligible landfill where landfill gas is currently collected and vented, but has never been destroyed in any manner prior to the start date.
|_| Installation of a new qualifying destruction device at an eligible landfill where landfill gas was collected and destroyed at any time prior to the project start date using:
|_| A non-qualifying destruction device (e.g., passive flare)
|_| A destruction device that is not otherwise eligible under the protocol
|_| Installation of a new gas collection system on a physically-distinct cell (or cells) where neither gas collection nor destruction has previously occurred.

Description: BWSWA had never collected or destroyed LFG prior to installing the GCCS and qualifying destruction device (utility flare) from the project. The project thus meets conditions in scenario (1) of section 3.4.1 of the Protocol and passes the performance standard test.
ii [bookmark: _Toc161137256]Limits on Credit Stacking 
Disclose if the project participates in carbon or other types of mitigation project types outside of the Reserve. If so, include a brief description of the project activity, the Registry in which the project is listed, and how the two projects do not result in double counting. Confirm that the Reserve and the other registry are aware of and provided approval for credit stacking. If no project stacking / credit stacking is occurring, state, “Not applicable.”
Not applicable
iii [bookmark: _Toc161137257]Legal Requirement Test
Attest that the project activities are not legally required. Identify any federal, provincial, or local regulations or legally binding mandates that are relevant to the project. State whether the project is subject to NSPS regulations and provide information regarding recent NMOC emission rate testing. Confirm that the landfill has not exceeded the NMOC threshold or provide the date at which the landfill is legally required to implement the GCCS.
The project is subject to the NSPS regulations for municipal solid waste landfills. NSPS regulations require landfills that are new or expanded capacity after July 17, 2014 with a design capacity greater than 2.5 million Mg to control emissions of non-methane organic compounds (NMOC) when the estimated NMOC emissions exceed 34 Mg per year. If a landfill exceeds the threshold, it has 30 months to install a LFG capture system. Results of a Tier II Report conducted by Geosyntec Consultants in September 2021 estimated IRCL's NMOC emission levels for 2024 and 2025 to be 12.18 and 12.38 Mg per year, respectively. IRCL has thus not exceeded the NMOC threshold.
Furthermore, BWSWA is not required to manage its LFG under any state or local regulations. BWSWA has met all applicable state and local environmental regulations and has obtained all applicable permits, including:
• Solid Waste Management Permit
• Title V Permit
• National Pollutant Discharge Elimination System (NPDES) Permit     
e [bookmark: _Toc161137258]Social and Environmental Safeguards
i [bookmark: _Toc161137259]Social Safeguards
Confirm below that the project is in material compliance with all labor and safety laws for the verification period.
The project is in material compliance with all labor and safety laws for the verification period.
ii [bookmark: _Toc161137260]Environmental Safeguards
Confirm below that the project was in material compliance with all environmental regulations during the reporting period, and how the project is designed and implemented in such a way to mitigate potential releases of pollutants that may cause degradation of the quality of soil, air, and surface and groundwater. Provide a brief description of any environmental benefits or harms that have resulted from the project. 
The project was in material compliance with all environmental regulations during the reporting period, as demonstrated by inspection records from regulatory bodies. The project's LFG utility flare is covered under BWSWA's Title V Air Operation Permit, so BWSWA will mitigate potential releases of pollutants that may cause degradation of the quality of air by completing the periodic testing and reporting of air pollutants required in the permit. The project does not result in the release of pollutants that may cause degradation of the quality of soil or surface and groundwater.
Environmental benefits that have resulted from the project include the destruction of methane that would have otherwise been vented to the atmosphere. Methane is a potent greenhouse gas.
f [bookmark: _Toc161137261]Regulatory Compliance
Provide the national, provincial, and/or local regulatory agencies with jurisdiction over the project boundary. Disclose any instances of non-compliance during the reporting period. Describe how the project will monitor for compliance during future reporting periods.
The regulatory agencies with jursidiciton over the project boundary are the U.S. Environmental Protection Agency and the Alabama Department of Environmental Management (ADEM).
There were no instances of non-compliance during the reporting period.
The project will continue following all relevant regulations and abiding by all conditions in BWSWA's environmental permits to monitor for compliance during future reporting periods.
4 [bookmark: _Toc161137262]GHG Assessment Boundary
a [bookmark: _Toc161137263]GHG Assessment Boundary
The table below includes only the SSRs that are included in the project quantification. For all SSRs considered in the GHG Assessment Boundary (included and excluded GHGs and their justification) refer to Table 4.1 in the Protocol.
	SSR
	Source Description
	Gas
	Baseline (B) or Project (P)

	4
	Emissions from
Waste Breakdown in
Landfill
	CH4
	B,P

	5
	Emissions from Gas
Collection System
	CO2
	P

	6
	Emissions from
Supplemental Fuel
	CO2, CH4
	P

	7
	Emissions from Project LFG Boiler Destruction
	CH4
	P

	
	Emissions from Baseline LFG Boiler Destruction
	CH4
	B

	8
	Emissions from
Project LFG
Electricity Generation
	CH4
	P

	
	Emissions from
Baseline LFG
Electricity Generation
	CH4
	B

	9
	Emissions from
Project LFG Flare
Destruction
	CH4
	P

	
	Emissions from
Baseline LFG Flare
Destruction
	CH4
	B

	10
	Emissions from
Upgrade of LFG
	CO2
	B,P

	11
	Emissions from Project LFG Pipeline or other NG end-use
	CH4
	P

	
	Emissions from
Baseline LFG
Pipeline or other NG
end-use
	CH4
	B


5 [bookmark: _Toc161137264]Quantifying GHG Emission Reductions
a [bookmark: _Toc161137265]Quantifying Baseline Emissions
i [bookmark: _Toc161137266]Summary of Baseline Quantification
Provide the total methane destroyed by the GCCS, factor for the oxidation of methane by soil bacteria, discount factor to account for modeling uncertainties, and adjustment factor to account for baseline LFG destruction device in the verification period, as calculated in the Protocol.
	Vintage:  2024
	Vintage:       

	Total methane destroyed: 2,607.94 tCH4
	Total methane destroyed:       tCH4

	Oxidation factor by soil bacteria: 10%
	Oxidation factor by soil bacteria:      

	Monitoring uncertainties discount factor: 0%
	Monitoring uncertainties discount factor:      

	Adjustment factor for baseline LFG destruction device: Not applicable
	Adjustment factor for baseline LFG destruction device:      

	Baseline Emissions: 65,720.03 tCO2e
	Baseline Emissions:       tCO2e


b [bookmark: _Toc161137267]Quantifying Project Emissions
i [bookmark: _Toc161137268]Site-Specific Destruction Efficiency
Provide the name of the state or local agency accredited service provider utilized to conduct the site-specific destruction efficiency testing, as well as the date the test was conducted and the destruction efficiency used for quantification.
Not applicable since default destruction efficiencies were used for the quantification of project emissions.
ii [bookmark: _Toc161137269]Summary of Project Emissions
Provide the total carbon dioxide emissions from the destruction of fossil fuel, total carbon dioxide emissions from the consumption of electricity from the grid, and the total quantity of emissions from supplemental natural gas in the verification period, as calculated in the Protocol.
	Vintage:  2024
	Vintage:       

	Emissions from fossil fuel use: 0.03 tCO2
	Emissions from fossil fuel use:       tCO2

	Emissions from electricity use: 107.28 tCO2
	Emissions from electricity use:       tCO2

	Emissions from supplemental natural gas: 0 tCO2
	Emissions from supplemental natural gas:       tCO2

	Project Emissions: 107.31 tCO2e

	Project Emissions:       tCO2e



c [bookmark: _Toc161137270]Final CRT Summary
Summarize the final result for determining the net GHG Reductions by vintage.
	Vintage:  2024
	Vintage:       

	Baseline Emissions: 65,720.03 tCO2e
	Baseline Emissions:       tCO2e

	Project Emissions: 107.31 tCO2e
	Project Emissions:       tCO2e

	Total GHG Emission Reductions/Removals: 65,612 tCO2e
	Total GHG Emission Reductions/Removals:       tCO2e


6 [bookmark: _Toc161137271]Project Monitoring
Check the boxes below and attest that project monitoring has occurred according to the Protocol. If requirements were not met, please list the date of variance request and fill out Section 7.
Have all monitoring and QA/QC requirements been met? |_| Yes |_| No
Have all field checks and calibrations been performed by a third-party? |_| Yes |_| No
Date of Variance Request, if applicable: Not applicable
7 Variance Request
If a variance was requested during the reporting period, provide a brief description of the rule/requirement in the protocol in question, the conditions of the determination, and the date of the variance request and determination.
Date of Variance Request:      
Protocol Section and Rule/Requirement:      
Description of how the project did not meet the protocol requirement above:      
Date Reserve Issued Determination:      
Variance Conditions:      
8 [bookmark: _Toc161137272]Project Documentation
The following documents are required to be submitted for project registration. In cases where there is proprietary information, please provide unredacted and redacted versions. If additional documents were submitted, please include the document title and its associated file name. 
	Document 
	File Name

	Project Diagram
	BW Flare Skid Drawing.pdf

	Attestation of Title
	Attestation-Title_Black-Warrior_2024 TB signed.pdf

	Attestation of Voluntary Implementation
	Attestation-Voluntary-Implementation_Black-Warrior_2024 TB signed.pdf

	Attestation of Regulatory Compliance
	Attestation-Regulatory-Compliance_Black-Warrior_2024 TB signed.pdf

	Monitoring Plan
	Black Warrior Monitoring Plan 2024 V2.0.docx

	Project Contributions to the U.N. Sustainable Development Goals Report Tool (if applicable)
	2024-SDG-REPORTING-TOOL-CAR403.pdf


	Project Data Report (this document)
	U.S. Landfill PDR_Black Warrior_2024_v2.0.docx

	List of Findings
	Black Warrior 2024 LoF Final

	Variance Request (if applicable)
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